$ EZ-EDS Version 3.36.1.20241010 Generated Electronic Data Sheet

[File]
        DescText = "EDS file for Lenze i550 motec Inverter Drive";
        CreateDate = 05-24-2022;
        CreateTime = 12:10:17;
        ModDate = 11-19-2024;
        ModTime = 10:23:49;
        Revision = 3.1;
        HomeURL = "https://www.lenze.com/";

[Device]
        VendCode = 587;
        VendName = "Lenze";
        ProdType = 2;
        ProdTypeStr = "AC Drive Device";
        ProdCode = 600;
        MajRev = 6;
        MinRev = 1;
        ProdName = "i550 motec";
        Catalog = "Inverter Drive i550 motec";
        Icon = "i550motec_eip_eds_icon.ico";
        IconContents =
                "AAABAAEAQEAAAAEACAAoFgAAFgAAACgAAABAAAAAgAAAAAEACAAAAAAAABYA"
                "AAAAAAAAAAAAAAAAAAAAAAD///8A///+AP7++wD+/f0A/Pz8AP78+gD7+/sA"
                "+vr6APr5+QD7+fcA+fj4APj39wD39/UA+ff0APX19QD19fQA8/PyAPPy7wDy"
                "8e8A8fDwAO/v7wDw7+wA8O7rAO3t7ADt7OkA7OvrAOzq5wDp6ekA6ejmAOfn"
                "5wDn5uQA5eTkAOTj4gDh4d8A4N/dAN/e3gDf3tsA3d3dANrb2wDd29kA3NrY"
                "ANnZ2QDa2dcA19fXANnX1ADX1tMA1dXVANXT0QDT0tIA1NLQANHR0QDQ0NAA"
                "0tDOAM/OzQDMzMwAzczKAMvKyQDKycYAyMjIAMbGxgDIxsQAxcXEAMXEwQDC"
                "wsIAw8LAAMLBvgDAwMAAv7+/AMC/vQC9vb0Avr26ALu7uQC7urkAuLi3ALm4"
                "tQC2trYAt7WzALW0swCzsrEAsbGwALKwrQCvr64Arq2sAKyrqgCtq6gAqqqq"
                "AKqppgCpqKYApqakAKWkogCjo6MAo6KgAKKhnwCgoJ8AoJ+dAJ2dnQCfnZsA"
                "m5qZAJiYmACXl5cAl5aVAJWVlACWlJEAlJOSAJORkACQkJAAkpCOAJCPjQCP"
                "jYsAjYyLAI2MiQCLi4oAjIuIAImJiQCLiYYAiIiHAIeHhwCIh4UAh4aDAISE"
                "hQCGhIIAgYKCAIOCfwCAgH8Af35+AH18fAB+fHkAe3t7AHp6egB8engAeXl4"
                "AHl4dgB2dnUAd3VyAHR0dABycnIAdHJwAHFxcABvb28AbW1tAG1sawBqamsA"
                "aGhpAGdnZwBmZmUAZWRkAGJiYQBfX18AXl1dAFtbWwBaWloAWFhYAFdXVgBV"
                "VVUAVFNUAFNTUwBSUlIAUFFQAE9OTgBMTEwASkpKAElJSQBHR0cARkZGAERE"
                "RABDQ0MAQkJCAEFBQQBCQT4AQEBAAD8/PwBAPzwAPj4+AD09PQA8PDwAOzs7"
                "ADk6OQA5OTkAODg4ADY3NgA2NjYANTU1ADQ0NAAzMzMAMjIyADExMQAwMDAA"
                "LzAvADAvLwAvLy8ALi4uAC4tLgAtLS0ALCwsACsrKwAqKioAKSkpACgoKAAn"
                "JycAJiYmACUlJQAkJCQAIyMjACIiIQAhISEAICAfAB8eHwAeHh4AHR0cABwc"
                "HAAbGxsAGhoZABkZGQAYGBgAGhgXABcXFwAYFhUAFhUWABQVFQAWFBIAExMT"
                "ABISEwATEhAAERERABEREAAPEBAAEhAOAA8PDwARDw0ADg4OAAwMDQAMDAwA"
                "DgwKAAoLCwAMCwkACQoJAAkJCQALCQcACgcGAAcHBwAGBgYACQYEAAgGAwAH"
                "BQMABAQEAAYDAQACAgIABAIAAAEBAQADAAAAAgAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAA4QAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAEEBxdBXCAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAXIyo7UlIxMS0GAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAQMGSFlmaWVTklJJzkGAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAYOIDZSd5CfuMzg"
                "08bFz541DEt9OAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAACNRZYemx8rKzdHOysW6tba+vsLPnZF0SbN9AAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAABxcpVWMHAA/a5tPMw7m9wL3AxMjN0Nba3uTOucfc"
                "nh930AcGUgsAAAAAAAAAAAAAAAAAAAAAAAAAAAAHGTpijKfO39LfpxRj2r6+"
                "wsLByNjk6u7t8ff6+ff73rO9scCcorMqRnohAAAAAAAAAAAAAAAAAAAAAAMA"
                "ABOhvsnL0NDJwbrAutDaybq+ucTKxMv1+vf19fXy8vLy+tuyvbSquNeqJ0R4"
                "IQAAAAAAAAAAAAAAAA8lT5CqHwB/6b7AwsDAwMjKurq9u7a0tcWSaZra9fPx"
                "9fPx9fv18frbsbq1rKzPtyghXiAAAAAAAAAAARA4aZzn9M7I0NWZxMLBwL/A"
                "uMaposO2tra3t8adXYJ5xvrb9e7t+/v7+/P62MLPt6qszLo0CSEXAAAAAAAU"
                "aZ7h4+bJkZfFwLnD0sC1ube1tcOicXejxbe3t7fOhH++j8P71uTF3vuCRZj7"
                "9+2km7murMnDPRIgEwAAAAAA0/u6k39fSwA74MO3tbW2t7e3t7fFd46akMC3"
                "t7i4wqSHkaXd8djk0PuSAAAPwuL7Yzu5tKrIxkARNBMAAAABTo9aSwcOJSAA"
                "Q9y+tre3t7e3t7e3wn2QkqPDt7i4uLbEubTEy+jk8fv7aQAAINb59ZeLsrCq"
                "yMdBDQsAAAAALlodHTAAHTMjAUXawLa3t7e3t7e4uMGlkqLGur2/wLq4tcfV"
                "vsny4u3P5NNORKv7+t7HwbCuqsfHQQ0AAAAAAC5IICsyFyY4SR5O3L23t7e3"
                "t7e3uLi2w9HMt7q3p6++uMeti6rc8uLty837+/v77vnet7i1rqrFyUYNAQAA"
                "AAAzQjNDJQszNR8EWPDVxbS3t7e3t7i4tsbEwMe0oamqssqqcXeGzOrb8u3y"
                "7vv78fH54re3tq2qwtBRCQMAAAAANlEwKQ8AOh0fBGTrh53Dt7i4t7i4uMKx"
                "gIO0uKzCqbXfhInOi7fz4vH38/Lx8fLy+ui3t7WsqsHSUwkDAAAAADI7BCMQ"
                "DD8zPRNt0S6NzLe4t7i4uLjHfXmLlMK5sKTG0JmEkprU9/rz9ff5+fn6+frW"
                "rrq3qanB1FIJAwAAAAArKSAlAAA2ITBPk9Cht7m4uLi4uLi5w3GSlKDGvbbD"
                "x7fEoJjC1e719e3b2NjW0MrHvrW1zcSmvdRRCQMAAAAAO1NdQhRFd5a20dTC"
                "xbm3uLi4uLi4uMSci5nBw726w7m2tsHAsb7NzsfDxcTCvLjBw8HDvsXawbvZ"
                "VwkEAAAAAF2ZnaXE7+vr6evOwbq4uLi4uLi4uLi4x77GwLWurra2ub26vcHG"
                "xcK+wsfEwMDBwLm3wMe3yd3Z5WACBAAAAABT2czd08rQys7OxMO5uLi4uLm4"
                "uLS1ubSyub2+xMbDxMnHxMPFw766vrq2t7i4t7m6ubrDt7fFjbJtBQQAAAAA"
                "Seu3tbTAzb7AyMLCube3uLazubq+wsPFysfExsjDwcG4tri4uLm5ubq6urq6"
                "urq6urq4wsCtqZHAaAUEAAAAADrnycvO0tDU6fbSwL64uL3AxsbGycbCw765"
                "ubm3t7i4ubq6urq6urq6urq6urq6vLq5wMbCrafG8F4CBgAAJWV8ytHV19PQ"
                "09PNwsDAvr66xcO9vbi2t7e5urq6urq6urq6urq6urq8u7q6vb29ury9vcO9"
                "wrCptulnAQcAAI34x8e+usO6trOytbi3uLi4vcC2uLi5ubm6urq6urq6urq6"
                "urq9vbu9vb29vb29vb29vc6OOqPFp7T0cwAHAAB0zLfMxLC0ub69vcG+uLm5"
                "uL3CuLm5urq6urq6urq6vLy8vb29vb29vb29vb29vb29vb3Lk2KuwKe09HMA"
                "BwAAb825y8W4vcTFxMHFwbi5ubm9wbm6urq6urq6ur28vb29vb29vb29vb29"
                "vb29vb29vb29vsK2tbKps/RzAAcAAIDKucvKvsLCwsHBwr25urq5ucrawLi6"
                "ury9ur29vb29vb29vb69vb29vr29vr6+vb6+vr23vcKvqrP0dAALAACTx7nN"
                "0rW1vLq5ucC+ubq6ucmqc67DvLq8vb29vb29vb29vr6+vr6+vr6+vr6+vr6+"
                "vr29wL2+sKqy7H0FCgAApNTJwXusubnE0eDgyba6urrUkzOvxr29vb29vb6+"
                "vb6+vr6+vr6+vr6+vr6+vr6+vr69vrm+wrCpsueGDQgAAIrDytKyz9LU1+X2"
                "+861vLu7w7esw7q9vb2+vr6+vr6+vr6+vr6+vr6+vr7AwL6+v8DBwsK9vsGx"
                "qbHnhw0IAAAECxMZJpns7PT09PjPtb6+vb7Ix7y9vr6+vr6+vr6+vr6+vr6+"
                "wcLBwcG+t7i6urq3sbKzuMK6rqqx64YJCgAAAAAAAAB959/s3OP2zLe+vr7B"
                "w72+vr6+vr6+v8HAwMDAv77AvrWyt7e3tbOztLS1t72+urGvvrKmr+mHCQwA"
                "AAAAABNdydzr3NXd5cm5wMC+wcO9wL6+wMLBwr61t725tbO1tba4ubi4ucDI"
                "yMXHxcPCwruwsb7Fs67gkRILAAAAE5XT+9nl3Nfl4evLucHBwMHFvrq9vri0"
                "t7e3t7axtsDDw8LCxcbDwb23sa2srq+ys6qtycS0ws3O35IYCAAAADbg0enX"
                "2ePXzt/0zLrBwsHCw7W1tbe5wL69w8zErrfDtrOwr62qqaempaqvqZqTi4Rv"
                "acjfw8q4tOmSFQoAAAAry8rg1OPg09/l8M29w8PCw8C+x8fEwsK9uLKjvdC+"
                "t5mgs6WfnJaRhnlhUjYuGwAAAAA7rdy+h0u6nBIMAAAAOszK5uHh3PDm5/TP"
                "xMm2s8PBubKup6Ognpyblqfc2se4ilxaQjolDg4PAAAAAAADABQDBmfUz2lf"
                "+KEWDAAAAEXM0cqz3+v05uHdyb26wra4oZucmpudn6CipKWks9Da55cdAAcA"
                "AAAAAAAAQ1VhjXmVobnC09enqrZvERAAAABCzNW9nNXZzsjLzK+cnsjdxami"
                "paWpqqqsrKyqpqKnxtKfc09SSE1xf46ep63CxsO6pJ+TglxITEYvIh4XAAAA"
                "Te/Twb7BzszJ0M+1n6OsytTavqOpp6ampqeqrrO5ucXsnI3jxcfKxLqumZB8"
                "ZFZALywkJCo+VldKPD4vGgwAAEepp93AuMG/t7Oxsq6qpKK256x0sr7AyM3S"
                "2ubj0sSxop6UhG5dSDw3LCcaJzExYImMmGZMrOHPg0RMPigeCgABAAOCxLGl"
                "pqalpKSnrbO+yendrNHHva+ekYNtW09ALRwSDwoSDS0oR3qBRFJ4YIimrqFh"
                "OV5uZ0w4GQEdHBMAAAAAAHmmrKanrrbH1NrhyqKQiX1cTDUiHBYBAAAABQMA"
                "EAADYVRKRVioqFc5fm5WVFdENT43NT5MTQgAGTcAAAAAAABkoc3P2encvp+E"
                "WTQYAgAAAgABAgAHAAABAAAAAAAAATlMRBkhl7WQL2t4eGZbXmtycnBscoEp"
                "AE1ZCwAAAAAAYtOun5RxSSUIAAAAAAMAAAEAAAAAAAAAAAAAAAAAAAAAJGAH"
                "AHW5nzVOhYiDenJubGxramp1WwRRcjAAAAAAAAAICgMAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAABOBHwAxpHxOMX6Bem5ra2xsa2hoamdKZnA8AAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA0hFcMJ1tXSB5Q"
                "iHJqam5ydXZ2cGpoa15YIQAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAWYNlT2c0Sk1GQXJ4bmhhXFRHOC0hGRAIAwAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAGSMhYN7VkxXTjUoIhcPCAMA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAcPSQbEAsEAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAACBMLCAQDAQAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA";

[Device Classification]
        Class1 = EtherNetIP;

[Params]
        Param1 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC2,                   $ Data Type
                1,                      $ Data Size in bytes
                "SINT_INP",             $ name
                "",                     $ units
                "(8bit)",               $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param2 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "INT_INP",              $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param3 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC4,                   $ Data Type
                4,                      $ Data Size in bytes
                "DINT_INP",             $ name
                "",                     $ units
                "(32bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param4 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "2B0B/0 Freq Setpoint Hz",    $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param5 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "2D40/4 Device Load Act.",    $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param6 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "2D4F/0 Motor i2t utiliz.",    $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param7 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC4,                   $ Data Type
                4,                      $ Data Size in bytes
                "2D82/0 Motor voltage", $ name
                "",                     $ units
                "(32bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param8 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "2D88/0 Motor current", $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param9 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC4,                   $ Data Type
                4,                      $ Data Size in bytes
                "2DA2/1 Effective Power",    $ name
                "",                     $ units
                "(32bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param10 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC4,                   $ Data Type
                4,                      $ Data Size in bytes
                "2DA2/2 Apparent Power",$ name
                "",                     $ units
                "(32bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param11 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC4,                   $ Data Type
                4,                      $ Data Size in bytes
                "2DA3/1 Energy Out Motor",    $ name
                "",                     $ units
                "(32bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param12 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC4,                   $ Data Type
                4,                      $ Data Size in bytes
                "2DA3/2 Energy Out Gen.",    $ name
                "",                     $ units
                "(32bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param24 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC4,                   $ Data Type
                4,                      $ Data Size in bytes
                "2DD3/1 Speed set",     $ name
                "",                     $ units
                "(32bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param26 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "2DDD/0 Actual Frequency",    $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param27 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "400A/1 NetWordOUT1",   $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param29 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "400C/1 AC Drv Stat Word",    $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param31 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "400C/3 Actual Speed Hz",    $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param32 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "400C/4 Actual Speed RPM",    $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param33 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "400C/5 Drive State",   $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param34 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "400C/6 Act Speed 0.01Hz",    $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param35 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "400C/7 Actual Torque Scaled",    $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param37 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "401F/1 Actual PID Stpnt",    $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param38 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "401F/2 Actual PID Fbk",$ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param39 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC2,                   $ Data Type
                1,                      $ Data Size in bytes
                "401F/3 PID bits",      $ name
                "",                     $ units
                "(8bit)",               $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param40 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "603F/0 Current Fault", $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param41 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "6041/0 Status Word",   $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param42 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "6043/0 Veloc Demand",  $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param43 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "6044/0 Veloc Actual",  $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param44 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC2,                   $ Data Type
                1,                      $ Data Size in bytes
                "6061/0 402 Mode Display",    $ name
                "",                     $ units
                "(8bit)",               $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param45 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "6077/0 402 ActualTorq %",    $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param46 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "6078/0 402 ActualCur %",    $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param47 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC4,                   $ Data Type
                4,                      $ Data Size in bytes
                "6079/0 402 DClink Volt",    $ name
                "",                     $ units
                "(32bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param48 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC4,                   $ Data Type
                4,                      $ Data Size in bytes
                "60FD/0 Dig Inputs Stat",    $ name
                "",                     $ units
                "(32bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param50 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "400C/9 Proc Output Freq",    $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places




        Param51 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC2,                   $ Data Type
                1,                      $ Data Size in bytes
                "SINT_OUT",             $ name
                "",                     $ units
                "(8bit)",               $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param52 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "INT_OUT",              $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param53 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC4,                   $ Data Type
                4,                      $ Data Size in bytes
                "DINT_OUT",             $ name
                "",                     $ units
                "(32bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places

        Param54 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC4,                   $ Data Type
                4,                      $ Data Size in bytes
                "2946/1 Trq Mode Hi Spd",    $ name
                "",                     $ units
                "(32bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places

        Param55 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC4,                   $ Data Type
                4,                      $ Data Size in bytes
                "2946/2 Trq Mode Lo Spd",    $ name
                "",                     $ units
                "(32bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places


        Param56 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "4008/1 NetWordIN1",    $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places

        Param57 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "4008/2 NetWordIN2",    $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places

        Param60 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "400B/1 AC Drv Ctrl Word",    $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places

        Param62 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "400B/3 Net Spd Stpnt Hz",    $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param63 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "400B/4 Net Spd Stpnt RPM",    $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param64 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "400B/5 Net Spd 0.01 Hz",    $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param65 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "400B/6 NetSpdSign 0.1Hz",    $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param66 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "400B/7 Net PID Stpnt", $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param67 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "400B/8 Net Torque Stpnt",    $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param68 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "6040/0 Control Word",  $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param69 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "6042/0 Target Veloc",  $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param70 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC4,                   $ Data Type
                4,                      $ Data Size in bytes
                "6046/1 Veloc Min",     $ name
                "",                     $ units
                "(32bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param71 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC4,                   $ Data Type
                4,                      $ Data Size in bytes
                "6046/2 Veloc Max",     $ name
                "",                     $ units
                "(32bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param72 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC4,                   $ Data Type
                4,                      $ Data Size in bytes
                "6048/1 Delta Speed",   $ name
                "",                     $ units
                "(32bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param73 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "6048/2 Delta Time",    $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param74 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC4,                   $ Data Type
                4,                      $ Data Size in bytes
                "6049/1 Delta Speed",   $ name
                "",                     $ units
                "(32bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param75 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "6049/2 Delta Time",    $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param76 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC2,                   $ Data Type
                1,                      $ Data Size in bytes
                "6060/0 402 Control Modes",    $ name
                "",                     $ units
                "(8bit)",               $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param77 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "6071/0 402 TargetTorq",$ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param78 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC4,                   $ Data Type
                4,                      $ Data Size in bytes
                "6080/0 Mot Max Speed", $ name
                "",                     $ units
                "(32bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param79 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "60E0/0 Pos TorqLimit", $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param80 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "60E1/0 Neg TorqLimit", $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param82 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "400B/13 Proc Input Freq",    $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places


        Param100 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC4,                   $ Data Type
                4,                      $ Data Size in bytes
                "Trailer Input",        $ name
                "",                     $ units
                "(32bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places

        Param101 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC4,                   $ Data Type
                4,                      $ Data Size in bytes
                "Trailer Output",       $ name
                "",                     $ units
                "(32bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places


        Param1000 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0002,                 $ Descriptor
                0xC6,                   $ Data Type
                1,                      $ Data Size in bytes
                "OUT Ctrl1:",           $ name
                "",                     $ units
                "New Help String",      $ help string
                0x14,0x15,0x15,         $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum1000 =
                0x14,"Basic",
                0x15,"Extended";
        Param1001 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0002,                 $ Descriptor
                0xC6,                   $ Data Type
                1,                      $ Data Size in bytes
                "INP Ctrl1:",           $ name
                "",                     $ units
                "New Help String",      $ help string
                0x46,0x47,0x47,         $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum1001 =
                0x46,"Basic",
                0x47,"Extended";
        Param1002 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0002,                 $ Descriptor
                0xC6,                   $ Data Type
                1,                      $ Data Size in bytes
                "OUT Ctrl2:",           $ name
                "",                     $ units
                "New Help String",      $ help string
                0x16,0x17,0x17,         $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum1002 =
                0x16,"Basic",
                0x17,"Extended";
        Param1003 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0002,                 $ Descriptor
                0xC6,                   $ Data Type
                1,                      $ Data Size in bytes
                "INP Ctrl2:",           $ name
                "",                     $ units
                "New Help String",      $ help string
                0x48,0x49,0x49,         $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum1003 =
                0x48,"Basic",
                0x49,"Extended";


        Param2000 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC8,                   $ Data Type
                4,                      $ Data Size in bytes
                "RPI Value",            $ name
                "",                     $ units
                "",                     $ help string
                4000,100000,10000,      $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places


        Param34000000 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Input#1",       $ name
                "",                     $ units
                "",                     $ help string
                0,65535,29,             $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000000 =
                0,"ignore",
                1,"SINT_INP",
                2,"INT_INP",
                3,"DINT_INP",
                4,"2B0B/0 Freq Setpoint Hz",
                5,"2D40/4 Device Load Act.",
                6,"2D4F/0 Motor i2t utiliz.",
                7,"2D82/0 Motor voltage",
                8,"2D88/0 Motor current",
                9,"2DA2/1 Effective Power",
                10,"2DA2/2 Apparent Power",
                11,"2DA3/1 Energy Out Motor",
                12,"2DA3/2 Energy Out Gen.",
                13,"2DA4/1 Anlg In1 %",
                14,"2DA4/2 Anlg In1 Freq",
                15,"2DA4/3 Anlg In1 PidVal",
                16,"2DA4/4 Anlg In1 TorqVal",
                17,"2DA5/1 Anlg In2 %",
                18,"2DA5/2 Anlg In2 Freq",
                19,"2DA5/3 Anlg In2 PidVal",
                20,"2DA5/4 Anlg In2 TorqVal",
                21,"2DAA/1 AO1 Value (VDC)",
                22,"2DAA/2 AO1 Value (IDC)",
                23,"reserved23",
                24,"2DD3/1 Speed set",
                25,"reserved25",
                26,"2DDD/0 Actual Frequency",
                27,"400A/1 NetWordOUT1",
                28,"400A/2 NetWordOUT2",
                29,"400C/1 AC Drv Stat Word",
                30,"400C/2 C0150 Stat Word",
                31,"400C/3 Actual Speed Hz",
                32,"400C/4 Actual Speed RPM",
                33,"400C/5 Drive State",
                34,"400C/6 Act Speed 0.01Hz",
                35,"400C/7 Actual Torque Scaled",
                36,"400D/0 Scaled Speed",
                37,"401F/1 Actual PID Stpnt",
                38,"401F/2 Actual PID Fbk",
                39,"401F/3 PID bits",
                40,"603F/0 Current Fault",
                41,"6041/0 Status Word",
                42,"6043/0 Veloc Demand",
                43,"6044/0 Veloc Actual",
                44,"6061/0 402 Mode Display",
                45,"6077/0 402 ActualTorq %",
                46,"6078/0 402 ActualCur %",
                47,"6079/0 402 DClink Volt",
                48,"60FD/0 Dig Inputs Stat",
                50,"400C/9 Proc Output Freq";
        Param34000001 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Input#2",       $ name
                "",                     $ units
                "",                     $ help string
                0,65535,32,             $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000001 =
                0,"ignore",
                1,"SINT_INP",
                2,"INT_INP",
                3,"DINT_INP",
                4,"2B0B/0 Freq Setpoint Hz",
                5,"2D40/4 Device Load Act.",
                6,"2D4F/0 Motor i2t utiliz.",
                7,"2D82/0 Motor voltage",
                8,"2D88/0 Motor current",
                9,"2DA2/1 Effective Power",
                10,"2DA2/2 Apparent Power",
                11,"2DA3/1 Energy Out Motor",
                12,"2DA3/2 Energy Out Gen.",
                13,"2DA4/1 Anlg In1 %",
                14,"2DA4/2 Anlg In1 Freq",
                15,"2DA4/3 Anlg In1 PidVal",
                16,"2DA4/4 Anlg In1 TorqVal",
                17,"2DA5/1 Anlg In2 %",
                18,"2DA5/2 Anlg In2 Freq",
                19,"2DA5/3 Anlg In2 PidVal",
                20,"2DA5/4 Anlg In2 TorqVal",
                21,"2DAA/1 AO1 Value (VDC)",
                22,"2DAA/2 AO1 Value (IDC)",
                23,"reserved23",
                24,"2DD3/1 Speed set",
                25,"reserved25",
                26,"2DDD/0 Actual Frequency",
                27,"400A/1 NetWordOUT1",
                28,"400A/2 NetWordOUT2",
                29,"400C/1 AC Drv Stat Word",
                30,"400C/2 C0150 Stat Word",
                31,"400C/3 Actual Speed Hz",
                32,"400C/4 Actual Speed RPM",
                33,"400C/5 Drive State",
                34,"400C/6 Act Speed 0.01Hz",
                35,"400C/7 Actual Torque Scaled",
                36,"400D/0 Scaled Speed",
                37,"401F/1 Actual PID Stpnt",
                38,"401F/2 Actual PID Fbk",
                39,"401F/3 PID bits",
                40,"603F/0 Current Fault",
                41,"6041/0 Status Word",
                42,"6043/0 Veloc Demand",
                43,"6044/0 Veloc Actual",
                44,"6061/0 402 Mode Display",
                45,"6077/0 402 ActualTorq %",
                46,"6078/0 402 ActualCur %",
                47,"6079/0 402 DClink Volt",
                48,"60FD/0 Dig Inputs Stat",
                50,"400C/9 Proc Output Freq";
        Param34000002 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Input#3",       $ name
                "",                     $ units
                "",                     $ help string
                0,65535,35,             $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000002 =
                0,"ignore",
                1,"SINT_INP",
                2,"INT_INP",
                3,"DINT_INP",
                4,"2B0B/0 Freq Setpoint Hz",
                5,"2D40/4 Device Load Act.",
                6,"2D4F/0 Motor i2t utiliz.",
                7,"2D82/0 Motor voltage",
                8,"2D88/0 Motor current",
                9,"2DA2/1 Effective Power",
                10,"2DA2/2 Apparent Power",
                11,"2DA3/1 Energy Out Motor",
                12,"2DA3/2 Energy Out Gen.",
                13,"2DA4/1 Anlg In1 %",
                14,"2DA4/2 Anlg In1 Freq",
                15,"2DA4/3 Anlg In1 PidVal",
                16,"2DA4/4 Anlg In1 TorqVal",
                17,"2DA5/1 Anlg In2 %",
                18,"2DA5/2 Anlg In2 Freq",
                19,"2DA5/3 Anlg In2 PidVal",
                20,"2DA5/4 Anlg In2 TorqVal",
                21,"2DAA/1 AO1 Value (VDC)",
                22,"2DAA/2 AO1 Value (IDC)",
                23,"reserved23",
                24,"2DD3/1 Speed set",
                25,"reserved25",
                26,"2DDD/0 Actual Frequency",
                27,"400A/1 NetWordOUT1",
                28,"400A/2 NetWordOUT2",
                29,"400C/1 AC Drv Stat Word",
                30,"400C/2 C0150 Stat Word",
                31,"400C/3 Actual Speed Hz",
                32,"400C/4 Actual Speed RPM",
                33,"400C/5 Drive State",
                34,"400C/6 Act Speed 0.01Hz",
                35,"400C/7 Actual Torque Scaled",
                36,"400D/0 Scaled Speed",
                37,"401F/1 Actual PID Stpnt",
                38,"401F/2 Actual PID Fbk",
                39,"401F/3 PID bits",
                40,"603F/0 Current Fault",
                41,"6041/0 Status Word",
                42,"6043/0 Veloc Demand",
                43,"6044/0 Veloc Actual",
                44,"6061/0 402 Mode Display",
                45,"6077/0 402 ActualTorq %",
                46,"6078/0 402 ActualCur %",
                47,"6079/0 402 DClink Volt",
                48,"60FD/0 Dig Inputs Stat",
                50,"400C/9 Proc Output Freq";
        Param34000003 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Input#4",       $ name
                "",                     $ units
                "",                     $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000003 =
                0,"ignore",
                1,"SINT_INP",
                2,"INT_INP",
                3,"DINT_INP",
                4,"2B0B/0 Freq Setpoint Hz",
                5,"2D40/4 Device Load Act.",
                6,"2D4F/0 Motor i2t utiliz.",
                7,"2D82/0 Motor voltage",
                8,"2D88/0 Motor current",
                9,"2DA2/1 Effective Power",
                10,"2DA2/2 Apparent Power",
                11,"2DA3/1 Energy Out Motor",
                12,"2DA3/2 Energy Out Gen.",
                13,"2DA4/1 Anlg In1 %",
                14,"2DA4/2 Anlg In1 Freq",
                15,"2DA4/3 Anlg In1 PidVal",
                16,"2DA4/4 Anlg In1 TorqVal",
                17,"2DA5/1 Anlg In2 %",
                18,"2DA5/2 Anlg In2 Freq",
                19,"2DA5/3 Anlg In2 PidVal",
                20,"2DA5/4 Anlg In2 TorqVal",
                21,"2DAA/1 AO1 Value (VDC)",
                22,"2DAA/2 AO1 Value (IDC)",
                23,"reserved23",
                24,"2DD3/1 Speed set",
                25,"reserved25",
                26,"2DDD/0 Actual Frequency",
                27,"400A/1 NetWordOUT1",
                28,"400A/2 NetWordOUT2",
                29,"400C/1 AC Drv Stat Word",
                30,"400C/2 C0150 Stat Word",
                31,"400C/3 Actual Speed Hz",
                32,"400C/4 Actual Speed RPM",
                33,"400C/5 Drive State",
                34,"400C/6 Act Speed 0.01Hz",
                35,"400C/7 Actual Torque Scaled",
                36,"400D/0 Scaled Speed",
                37,"401F/1 Actual PID Stpnt",
                38,"401F/2 Actual PID Fbk",
                39,"401F/3 PID bits",
                40,"603F/0 Current Fault",
                41,"6041/0 Status Word",
                42,"6043/0 Veloc Demand",
                43,"6044/0 Veloc Actual",
                44,"6061/0 402 Mode Display",
                45,"6077/0 402 ActualTorq %",
                46,"6078/0 402 ActualCur %",
                47,"6079/0 402 DClink Volt",
                48,"60FD/0 Dig Inputs Stat",
                50,"400C/9 Proc Output Freq";
        Param34000004 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Input#5",       $ name
                "",                     $ units
                "",                     $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000004 =
                0,"ignore",
                1,"SINT_INP",
                2,"INT_INP",
                3,"DINT_INP",
                4,"2B0B/0 Freq Setpoint Hz",
                5,"2D40/4 Device Load Act.",
                6,"2D4F/0 Motor i2t utiliz.",
                7,"2D82/0 Motor voltage",
                8,"2D88/0 Motor current",
                9,"2DA2/1 Effective Power",
                10,"2DA2/2 Apparent Power",
                11,"2DA3/1 Energy Out Motor",
                12,"2DA3/2 Energy Out Gen.",
                13,"2DA4/1 Anlg In1 %",
                14,"2DA4/2 Anlg In1 Freq",
                15,"2DA4/3 Anlg In1 PidVal",
                16,"2DA4/4 Anlg In1 TorqVal",
                17,"2DA5/1 Anlg In2 %",
                18,"2DA5/2 Anlg In2 Freq",
                19,"2DA5/3 Anlg In2 PidVal",
                20,"2DA5/4 Anlg In2 TorqVal",
                21,"2DAA/1 AO1 Value (VDC)",
                22,"2DAA/2 AO1 Value (IDC)",
                23,"reserved23",
                24,"2DD3/1 Speed set",
                25,"reserved25",
                26,"2DDD/0 Actual Frequency",
                27,"400A/1 NetWordOUT1",
                28,"400A/2 NetWordOUT2",
                29,"400C/1 AC Drv Stat Word",
                30,"400C/2 C0150 Stat Word",
                31,"400C/3 Actual Speed Hz",
                32,"400C/4 Actual Speed RPM",
                33,"400C/5 Drive State",
                34,"400C/6 Act Speed 0.01Hz",
                35,"400C/7 Actual Torque Scaled",
                36,"400D/0 Scaled Speed",
                37,"401F/1 Actual PID Stpnt",
                38,"401F/2 Actual PID Fbk",
                39,"401F/3 PID bits",
                40,"603F/0 Current Fault",
                41,"6041/0 Status Word",
                42,"6043/0 Veloc Demand",
                43,"6044/0 Veloc Actual",
                44,"6061/0 402 Mode Display",
                45,"6077/0 402 ActualTorq %",
                46,"6078/0 402 ActualCur %",
                47,"6079/0 402 DClink Volt",
                48,"60FD/0 Dig Inputs Stat",
                50,"400C/9 Proc Output Freq";
        Param34000005 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Input#6",       $ name
                "",                     $ units
                "",                     $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000005 =
                0,"ignore",
                1,"SINT_INP",
                2,"INT_INP",
                3,"DINT_INP",
                4,"2B0B/0 Freq Setpoint Hz",
                5,"2D40/4 Device Load Act.",
                6,"2D4F/0 Motor i2t utiliz.",
                7,"2D82/0 Motor voltage",
                8,"2D88/0 Motor current",
                9,"2DA2/1 Effective Power",
                10,"2DA2/2 Apparent Power",
                11,"2DA3/1 Energy Out Motor",
                12,"2DA3/2 Energy Out Gen.",
                13,"2DA4/1 Anlg In1 %",
                14,"2DA4/2 Anlg In1 Freq",
                15,"2DA4/3 Anlg In1 PidVal",
                16,"2DA4/4 Anlg In1 TorqVal",
                17,"2DA5/1 Anlg In2 %",
                18,"2DA5/2 Anlg In2 Freq",
                19,"2DA5/3 Anlg In2 PidVal",
                20,"2DA5/4 Anlg In2 TorqVal",
                21,"2DAA/1 AO1 Value (VDC)",
                22,"2DAA/2 AO1 Value (IDC)",
                23,"reserved23",
                24,"2DD3/1 Speed set",
                25,"reserved25",
                26,"2DDD/0 Actual Frequency",
                27,"400A/1 NetWordOUT1",
                28,"400A/2 NetWordOUT2",
                29,"400C/1 AC Drv Stat Word",
                30,"400C/2 C0150 Stat Word",
                31,"400C/3 Actual Speed Hz",
                32,"400C/4 Actual Speed RPM",
                33,"400C/5 Drive State",
                34,"400C/6 Act Speed 0.01Hz",
                35,"400C/7 Actual Torque Scaled",
                36,"400D/0 Scaled Speed",
                37,"401F/1 Actual PID Stpnt",
                38,"401F/2 Actual PID Fbk",
                39,"401F/3 PID bits",
                40,"603F/0 Current Fault",
                41,"6041/0 Status Word",
                42,"6043/0 Veloc Demand",
                43,"6044/0 Veloc Actual",
                44,"6061/0 402 Mode Display",
                45,"6077/0 402 ActualTorq %",
                46,"6078/0 402 ActualCur %",
                47,"6079/0 402 DClink Volt",
                48,"60FD/0 Dig Inputs Stat",
                50,"400C/9 Proc Output Freq";
        Param34000006 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Input#7",       $ name
                "",                     $ units
                "",                     $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000006 =
                0,"ignore",
                1,"SINT_INP",
                2,"INT_INP",
                3,"DINT_INP",
                4,"2B0B/0 Freq Setpoint Hz",
                5,"2D40/4 Device Load Act.",
                6,"2D4F/0 Motor i2t utiliz.",
                7,"2D82/0 Motor voltage",
                8,"2D88/0 Motor current",
                9,"2DA2/1 Effective Power",
                10,"2DA2/2 Apparent Power",
                11,"2DA3/1 Energy Out Motor",
                12,"2DA3/2 Energy Out Gen.",
                13,"2DA4/1 Anlg In1 %",
                14,"2DA4/2 Anlg In1 Freq",
                15,"2DA4/3 Anlg In1 PidVal",
                16,"2DA4/4 Anlg In1 TorqVal",
                17,"2DA5/1 Anlg In2 %",
                18,"2DA5/2 Anlg In2 Freq",
                19,"2DA5/3 Anlg In2 PidVal",
                20,"2DA5/4 Anlg In2 TorqVal",
                21,"2DAA/1 AO1 Value (VDC)",
                22,"2DAA/2 AO1 Value (IDC)",
                23,"reserved23",
                24,"2DD3/1 Speed set",
                25,"reserved25",
                26,"2DDD/0 Actual Frequency",
                27,"400A/1 NetWordOUT1",
                28,"400A/2 NetWordOUT2",
                29,"400C/1 AC Drv Stat Word",
                30,"400C/2 C0150 Stat Word",
                31,"400C/3 Actual Speed Hz",
                32,"400C/4 Actual Speed RPM",
                33,"400C/5 Drive State",
                34,"400C/6 Act Speed 0.01Hz",
                35,"400C/7 Actual Torque Scaled",
                36,"400D/0 Scaled Speed",
                37,"401F/1 Actual PID Stpnt",
                38,"401F/2 Actual PID Fbk",
                39,"401F/3 PID bits",
                40,"603F/0 Current Fault",
                41,"6041/0 Status Word",
                42,"6043/0 Veloc Demand",
                43,"6044/0 Veloc Actual",
                44,"6061/0 402 Mode Display",
                45,"6077/0 402 ActualTorq %",
                46,"6078/0 402 ActualCur %",
                47,"6079/0 402 DClink Volt",
                48,"60FD/0 Dig Inputs Stat",
                50,"400C/9 Proc Output Freq";
        Param34000007 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Input#8",       $ name
                "",                     $ units
                "",                     $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000007 =
                0,"ignore",
                1,"SINT_INP",
                2,"INT_INP",
                3,"DINT_INP",
                4,"2B0B/0 Freq Setpoint Hz",
                5,"2D40/4 Device Load Act.",
                6,"2D4F/0 Motor i2t utiliz.",
                7,"2D82/0 Motor voltage",
                8,"2D88/0 Motor current",
                9,"2DA2/1 Effective Power",
                10,"2DA2/2 Apparent Power",
                11,"2DA3/1 Energy Out Motor",
                12,"2DA3/2 Energy Out Gen.",
                13,"2DA4/1 Anlg In1 %",
                14,"2DA4/2 Anlg In1 Freq",
                15,"2DA4/3 Anlg In1 PidVal",
                16,"2DA4/4 Anlg In1 TorqVal",
                17,"2DA5/1 Anlg In2 %",
                18,"2DA5/2 Anlg In2 Freq",
                19,"2DA5/3 Anlg In2 PidVal",
                20,"2DA5/4 Anlg In2 TorqVal",
                21,"2DAA/1 AO1 Value (VDC)",
                22,"2DAA/2 AO1 Value (IDC)",
                23,"reserved23",
                24,"2DD3/1 Speed set",
                25,"reserved25",
                26,"2DDD/0 Actual Frequency",
                27,"400A/1 NetWordOUT1",
                28,"400A/2 NetWordOUT2",
                29,"400C/1 AC Drv Stat Word",
                30,"400C/2 C0150 Stat Word",
                31,"400C/3 Actual Speed Hz",
                32,"400C/4 Actual Speed RPM",
                33,"400C/5 Drive State",
                34,"400C/6 Act Speed 0.01Hz",
                35,"400C/7 Actual Torque Scaled",
                36,"400D/0 Scaled Speed",
                37,"401F/1 Actual PID Stpnt",
                38,"401F/2 Actual PID Fbk",
                39,"401F/3 PID bits",
                40,"603F/0 Current Fault",
                41,"6041/0 Status Word",
                42,"6043/0 Veloc Demand",
                43,"6044/0 Veloc Actual",
                44,"6061/0 402 Mode Display",
                45,"6077/0 402 ActualTorq %",
                46,"6078/0 402 ActualCur %",
                47,"6079/0 402 DClink Volt",
                48,"60FD/0 Dig Inputs Stat",
                50,"400C/9 Proc Output Freq";
        Param34000008 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Input#9",       $ name
                "",                     $ units
                "",                     $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000008 =
                0,"ignore",
                1,"SINT_INP",
                2,"INT_INP",
                3,"DINT_INP",
                4,"2B0B/0 Freq Setpoint Hz",
                5,"2D40/4 Device Load Act.",
                6,"2D4F/0 Motor i2t utiliz.",
                7,"2D82/0 Motor voltage",
                8,"2D88/0 Motor current",
                9,"2DA2/1 Effective Power",
                10,"2DA2/2 Apparent Power",
                11,"2DA3/1 Energy Out Motor",
                12,"2DA3/2 Energy Out Gen.",
                13,"2DA4/1 Anlg In1 %",
                14,"2DA4/2 Anlg In1 Freq",
                15,"2DA4/3 Anlg In1 PidVal",
                16,"2DA4/4 Anlg In1 TorqVal",
                17,"2DA5/1 Anlg In2 %",
                18,"2DA5/2 Anlg In2 Freq",
                19,"2DA5/3 Anlg In2 PidVal",
                20,"2DA5/4 Anlg In2 TorqVal",
                21,"2DAA/1 AO1 Value (VDC)",
                22,"2DAA/2 AO1 Value (IDC)",
                23,"reserved23",
                24,"2DD3/1 Speed set",
                25,"reserved25",
                26,"2DDD/0 Actual Frequency",
                27,"400A/1 NetWordOUT1",
                28,"400A/2 NetWordOUT2",
                29,"400C/1 AC Drv Stat Word",
                30,"400C/2 C0150 Stat Word",
                31,"400C/3 Actual Speed Hz",
                32,"400C/4 Actual Speed RPM",
                33,"400C/5 Drive State",
                34,"400C/6 Act Speed 0.01Hz",
                35,"400C/7 Actual Torque Scaled",
                36,"400D/0 Scaled Speed",
                37,"401F/1 Actual PID Stpnt",
                38,"401F/2 Actual PID Fbk",
                39,"401F/3 PID bits",
                40,"603F/0 Current Fault",
                41,"6041/0 Status Word",
                42,"6043/0 Veloc Demand",
                43,"6044/0 Veloc Actual",
                44,"6061/0 402 Mode Display",
                45,"6077/0 402 ActualTorq %",
                46,"6078/0 402 ActualCur %",
                47,"6079/0 402 DClink Volt",
                48,"60FD/0 Dig Inputs Stat",
                50,"400C/9 Proc Output Freq";
        Param34000009 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Input#10",      $ name
                "",                     $ units
                "",                     $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000009 =
                0,"ignore",
                1,"SINT_INP",
                2,"INT_INP",
                3,"DINT_INP",
                4,"2B0B/0 Freq Setpoint Hz",
                5,"2D40/4 Device Load Act.",
                6,"2D4F/0 Motor i2t utiliz.",
                7,"2D82/0 Motor voltage",
                8,"2D88/0 Motor current",
                9,"2DA2/1 Effective Power",
                10,"2DA2/2 Apparent Power",
                11,"2DA3/1 Energy Out Motor",
                12,"2DA3/2 Energy Out Gen.",
                13,"2DA4/1 Anlg In1 %",
                14,"2DA4/2 Anlg In1 Freq",
                15,"2DA4/3 Anlg In1 PidVal",
                16,"2DA4/4 Anlg In1 TorqVal",
                17,"2DA5/1 Anlg In2 %",
                18,"2DA5/2 Anlg In2 Freq",
                19,"2DA5/3 Anlg In2 PidVal",
                20,"2DA5/4 Anlg In2 TorqVal",
                21,"2DAA/1 AO1 Value (VDC)",
                22,"2DAA/2 AO1 Value (IDC)",
                23,"reserved23",
                24,"2DD3/1 Speed set",
                25,"reserved25",
                26,"2DDD/0 Actual Frequency",
                27,"400A/1 NetWordOUT1",
                28,"400A/2 NetWordOUT2",
                29,"400C/1 AC Drv Stat Word",
                30,"400C/2 C0150 Stat Word",
                31,"400C/3 Actual Speed Hz",
                32,"400C/4 Actual Speed RPM",
                33,"400C/5 Drive State",
                34,"400C/6 Act Speed 0.01Hz",
                35,"400C/7 Actual Torque Scaled",
                36,"400D/0 Scaled Speed",
                37,"401F/1 Actual PID Stpnt",
                38,"401F/2 Actual PID Fbk",
                39,"401F/3 PID bits",
                40,"603F/0 Current Fault",
                41,"6041/0 Status Word",
                42,"6043/0 Veloc Demand",
                43,"6044/0 Veloc Actual",
                44,"6061/0 402 Mode Display",
                45,"6077/0 402 ActualTorq %",
                46,"6078/0 402 ActualCur %",
                47,"6079/0 402 DClink Volt",
                48,"60FD/0 Dig Inputs Stat",
                50,"400C/9 Proc Output Freq";
        Param34000010 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Input#11",      $ name
                "",                     $ units
                "",                     $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000010 =
                0,"ignore",
                1,"SINT_INP",
                2,"INT_INP",
                3,"DINT_INP",
                4,"2B0B/0 Freq Setpoint Hz",
                5,"2D40/4 Device Load Act.",
                6,"2D4F/0 Motor i2t utiliz.",
                7,"2D82/0 Motor voltage",
                8,"2D88/0 Motor current",
                9,"2DA2/1 Effective Power",
                10,"2DA2/2 Apparent Power",
                11,"2DA3/1 Energy Out Motor",
                12,"2DA3/2 Energy Out Gen.",
                13,"2DA4/1 Anlg In1 %",
                14,"2DA4/2 Anlg In1 Freq",
                15,"2DA4/3 Anlg In1 PidVal",
                16,"2DA4/4 Anlg In1 TorqVal",
                17,"2DA5/1 Anlg In2 %",
                18,"2DA5/2 Anlg In2 Freq",
                19,"2DA5/3 Anlg In2 PidVal",
                20,"2DA5/4 Anlg In2 TorqVal",
                21,"2DAA/1 AO1 Value (VDC)",
                22,"2DAA/2 AO1 Value (IDC)",
                23,"reserved23",
                24,"2DD3/1 Speed set",
                25,"reserved25",
                26,"2DDD/0 Actual Frequency",
                27,"400A/1 NetWordOUT1",
                28,"400A/2 NetWordOUT2",
                29,"400C/1 AC Drv Stat Word",
                30,"400C/2 C0150 Stat Word",
                31,"400C/3 Actual Speed Hz",
                32,"400C/4 Actual Speed RPM",
                33,"400C/5 Drive State",
                34,"400C/6 Act Speed 0.01Hz",
                35,"400C/7 Actual Torque Scaled",
                36,"400D/0 Scaled Speed",
                37,"401F/1 Actual PID Stpnt",
                38,"401F/2 Actual PID Fbk",
                39,"401F/3 PID bits",
                40,"603F/0 Current Fault",
                41,"6041/0 Status Word",
                42,"6043/0 Veloc Demand",
                43,"6044/0 Veloc Actual",
                44,"6061/0 402 Mode Display",
                45,"6077/0 402 ActualTorq %",
                46,"6078/0 402 ActualCur %",
                47,"6079/0 402 DClink Volt",
                48,"60FD/0 Dig Inputs Stat",
                50,"400C/9 Proc Output Freq";
        Param34000011 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Input#12",      $ name
                "",                     $ units
                "",                     $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000011 =
                0,"ignore",
                1,"SINT_INP",
                2,"INT_INP",
                3,"DINT_INP",
                4,"2B0B/0 Freq Setpoint Hz",
                5,"2D40/4 Device Load Act.",
                6,"2D4F/0 Motor i2t utiliz.",
                7,"2D82/0 Motor voltage",
                8,"2D88/0 Motor current",
                9,"2DA2/1 Effective Power",
                10,"2DA2/2 Apparent Power",
                11,"2DA3/1 Energy Out Motor",
                12,"2DA3/2 Energy Out Gen.",
                13,"2DA4/1 Anlg In1 %",
                14,"2DA4/2 Anlg In1 Freq",
                15,"2DA4/3 Anlg In1 PidVal",
                16,"2DA4/4 Anlg In1 TorqVal",
                17,"2DA5/1 Anlg In2 %",
                18,"2DA5/2 Anlg In2 Freq",
                19,"2DA5/3 Anlg In2 PidVal",
                20,"2DA5/4 Anlg In2 TorqVal",
                21,"2DAA/1 AO1 Value (VDC)",
                22,"2DAA/2 AO1 Value (IDC)",
                23,"reserved23",
                24,"2DD3/1 Speed set",
                25,"reserved25",
                26,"2DDD/0 Actual Frequency",
                27,"400A/1 NetWordOUT1",
                28,"400A/2 NetWordOUT2",
                29,"400C/1 AC Drv Stat Word",
                30,"400C/2 C0150 Stat Word",
                31,"400C/3 Actual Speed Hz",
                32,"400C/4 Actual Speed RPM",
                33,"400C/5 Drive State",
                34,"400C/6 Act Speed 0.01Hz",
                35,"400C/7 Actual Torque Scaled",
                36,"400D/0 Scaled Speed",
                37,"401F/1 Actual PID Stpnt",
                38,"401F/2 Actual PID Fbk",
                39,"401F/3 PID bits",
                40,"603F/0 Current Fault",
                41,"6041/0 Status Word",
                42,"6043/0 Veloc Demand",
                43,"6044/0 Veloc Actual",
                44,"6061/0 402 Mode Display",
                45,"6077/0 402 ActualTorq %",
                46,"6078/0 402 ActualCur %",
                47,"6079/0 402 DClink Volt",
                48,"60FD/0 Dig Inputs Stat",
                50,"400C/9 Proc Output Freq";
        Param34000012 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Input#13",      $ name
                "",                     $ units
                "",                     $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000012 =
                0,"ignore",
                1,"SINT_INP",
                2,"INT_INP",
                3,"DINT_INP",
                4,"2B0B/0 Freq Setpoint Hz",
                5,"2D40/4 Device Load Act.",
                6,"2D4F/0 Motor i2t utiliz.",
                7,"2D82/0 Motor voltage",
                8,"2D88/0 Motor current",
                9,"2DA2/1 Effective Power",
                10,"2DA2/2 Apparent Power",
                11,"2DA3/1 Energy Out Motor",
                12,"2DA3/2 Energy Out Gen.",
                13,"2DA4/1 Anlg In1 %",
                14,"2DA4/2 Anlg In1 Freq",
                15,"2DA4/3 Anlg In1 PidVal",
                16,"2DA4/4 Anlg In1 TorqVal",
                17,"2DA5/1 Anlg In2 %",
                18,"2DA5/2 Anlg In2 Freq",
                19,"2DA5/3 Anlg In2 PidVal",
                20,"2DA5/4 Anlg In2 TorqVal",
                21,"2DAA/1 AO1 Value (VDC)",
                22,"2DAA/2 AO1 Value (IDC)",
                23,"reserved23",
                24,"2DD3/1 Speed set",
                25,"reserved25",
                26,"2DDD/0 Actual Frequency",
                27,"400A/1 NetWordOUT1",
                28,"400A/2 NetWordOUT2",
                29,"400C/1 AC Drv Stat Word",
                30,"400C/2 C0150 Stat Word",
                31,"400C/3 Actual Speed Hz",
                32,"400C/4 Actual Speed RPM",
                33,"400C/5 Drive State",
                34,"400C/6 Act Speed 0.01Hz",
                35,"400C/7 Actual Torque Scaled",
                36,"400D/0 Scaled Speed",
                37,"401F/1 Actual PID Stpnt",
                38,"401F/2 Actual PID Fbk",
                39,"401F/3 PID bits",
                40,"603F/0 Current Fault",
                41,"6041/0 Status Word",
                42,"6043/0 Veloc Demand",
                43,"6044/0 Veloc Actual",
                44,"6061/0 402 Mode Display",
                45,"6077/0 402 ActualTorq %",
                46,"6078/0 402 ActualCur %",
                47,"6079/0 402 DClink Volt",
                48,"60FD/0 Dig Inputs Stat",
                50,"400C/9 Proc Output Freq";
        Param34000013 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Input#14",      $ name
                "",                     $ units
                "",                     $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000013 =
                0,"ignore",
                1,"SINT_INP",
                2,"INT_INP",
                3,"DINT_INP",
                4,"2B0B/0 Freq Setpoint Hz",
                5,"2D40/4 Device Load Act.",
                6,"2D4F/0 Motor i2t utiliz.",
                7,"2D82/0 Motor voltage",
                8,"2D88/0 Motor current",
                9,"2DA2/1 Effective Power",
                10,"2DA2/2 Apparent Power",
                11,"2DA3/1 Energy Out Motor",
                12,"2DA3/2 Energy Out Gen.",
                13,"2DA4/1 Anlg In1 %",
                14,"2DA4/2 Anlg In1 Freq",
                15,"2DA4/3 Anlg In1 PidVal",
                16,"2DA4/4 Anlg In1 TorqVal",
                17,"2DA5/1 Anlg In2 %",
                18,"2DA5/2 Anlg In2 Freq",
                19,"2DA5/3 Anlg In2 PidVal",
                20,"2DA5/4 Anlg In2 TorqVal",
                21,"2DAA/1 AO1 Value (VDC)",
                22,"2DAA/2 AO1 Value (IDC)",
                23,"reserved23",
                24,"2DD3/1 Speed set",
                25,"reserved25",
                26,"2DDD/0 Actual Frequency",
                27,"400A/1 NetWordOUT1",
                28,"400A/2 NetWordOUT2",
                29,"400C/1 AC Drv Stat Word",
                30,"400C/2 C0150 Stat Word",
                31,"400C/3 Actual Speed Hz",
                32,"400C/4 Actual Speed RPM",
                33,"400C/5 Drive State",
                34,"400C/6 Act Speed 0.01Hz",
                35,"400C/7 Actual Torque Scaled",
                36,"400D/0 Scaled Speed",
                37,"401F/1 Actual PID Stpnt",
                38,"401F/2 Actual PID Fbk",
                39,"401F/3 PID bits",
                40,"603F/0 Current Fault",
                41,"6041/0 Status Word",
                42,"6043/0 Veloc Demand",
                43,"6044/0 Veloc Actual",
                44,"6061/0 402 Mode Display",
                45,"6077/0 402 ActualTorq %",
                46,"6078/0 402 ActualCur %",
                47,"6079/0 402 DClink Volt",
                48,"60FD/0 Dig Inputs Stat",
                50,"400C/9 Proc Output Freq";
        Param34000014 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Input#15",      $ name
                "",                     $ units
                "",                     $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000014 =
                0,"ignore",
                1,"SINT_INP",
                2,"INT_INP",
                3,"DINT_INP",
                4,"2B0B/0 Freq Setpoint Hz",
                5,"2D40/4 Device Load Act.",
                6,"2D4F/0 Motor i2t utiliz.",
                7,"2D82/0 Motor voltage",
                8,"2D88/0 Motor current",
                9,"2DA2/1 Effective Power",
                10,"2DA2/2 Apparent Power",
                11,"2DA3/1 Energy Out Motor",
                12,"2DA3/2 Energy Out Gen.",
                13,"2DA4/1 Anlg In1 %",
                14,"2DA4/2 Anlg In1 Freq",
                15,"2DA4/3 Anlg In1 PidVal",
                16,"2DA4/4 Anlg In1 TorqVal",
                17,"2DA5/1 Anlg In2 %",
                18,"2DA5/2 Anlg In2 Freq",
                19,"2DA5/3 Anlg In2 PidVal",
                20,"2DA5/4 Anlg In2 TorqVal",
                21,"2DAA/1 AO1 Value (VDC)",
                22,"2DAA/2 AO1 Value (IDC)",
                23,"reserved23",
                24,"2DD3/1 Speed set",
                25,"reserved25",
                26,"2DDD/0 Actual Frequency",
                27,"400A/1 NetWordOUT1",
                28,"400A/2 NetWordOUT2",
                29,"400C/1 AC Drv Stat Word",
                30,"400C/2 C0150 Stat Word",
                31,"400C/3 Actual Speed Hz",
                32,"400C/4 Actual Speed RPM",
                33,"400C/5 Drive State",
                34,"400C/6 Act Speed 0.01Hz",
                35,"400C/7 Actual Torque Scaled",
                36,"400D/0 Scaled Speed",
                37,"401F/1 Actual PID Stpnt",
                38,"401F/2 Actual PID Fbk",
                39,"401F/3 PID bits",
                40,"603F/0 Current Fault",
                41,"6041/0 Status Word",
                42,"6043/0 Veloc Demand",
                43,"6044/0 Veloc Actual",
                44,"6061/0 402 Mode Display",
                45,"6077/0 402 ActualTorq %",
                46,"6078/0 402 ActualCur %",
                47,"6079/0 402 DClink Volt",
                48,"60FD/0 Dig Inputs Stat",
                50,"400C/9 Proc Output Freq";
        Param34000015 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Input#16",      $ name
                "",                     $ units
                "",                     $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000015 =
                0,"ignore",
                1,"SINT_INP",
                2,"INT_INP",
                3,"DINT_INP",
                4,"2B0B/0 Freq Setpoint Hz",
                5,"2D40/4 Device Load Act.",
                6,"2D4F/0 Motor i2t utiliz.",
                7,"2D82/0 Motor voltage",
                8,"2D88/0 Motor current",
                9,"2DA2/1 Effective Power",
                10,"2DA2/2 Apparent Power",
                11,"2DA3/1 Energy Out Motor",
                12,"2DA3/2 Energy Out Gen.",
                13,"2DA4/1 Anlg In1 %",
                14,"2DA4/2 Anlg In1 Freq",
                15,"2DA4/3 Anlg In1 PidVal",
                16,"2DA4/4 Anlg In1 TorqVal",
                17,"2DA5/1 Anlg In2 %",
                18,"2DA5/2 Anlg In2 Freq",
                19,"2DA5/3 Anlg In2 PidVal",
                20,"2DA5/4 Anlg In2 TorqVal",
                21,"2DAA/1 AO1 Value (VDC)",
                22,"2DAA/2 AO1 Value (IDC)",
                23,"reserved23",
                24,"2DD3/1 Speed set",
                25,"reserved25",
                26,"2DDD/0 Actual Frequency",
                27,"400A/1 NetWordOUT1",
                28,"400A/2 NetWordOUT2",
                29,"400C/1 AC Drv Stat Word",
                30,"400C/2 C0150 Stat Word",
                31,"400C/3 Actual Speed Hz",
                32,"400C/4 Actual Speed RPM",
                33,"400C/5 Drive State",
                34,"400C/6 Act Speed 0.01Hz",
                35,"400C/7 Actual Torque Scaled",
                36,"400D/0 Scaled Speed",
                37,"401F/1 Actual PID Stpnt",
                38,"401F/2 Actual PID Fbk",
                39,"401F/3 PID bits",
                40,"603F/0 Current Fault",
                41,"6041/0 Status Word",
                42,"6043/0 Veloc Demand",
                43,"6044/0 Veloc Actual",
                44,"6061/0 402 Mode Display",
                45,"6077/0 402 ActualTorq %",
                46,"6078/0 402 ActualCur %",
                47,"6079/0 402 DClink Volt",
                48,"60FD/0 Dig Inputs Stat",
                50,"400C/9 Proc Output Freq";

        Param34000050 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Output#1",      $ name
                "",                     $ units
                "",                     $ help string
                0,65535,60,             $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000050 =
                0,"ignore",
                51,"SINT_OUT",
                52,"INT_OUT",
                53,"DINT_OUT",
                54,"2946/1 Trq Mode Hi Spd",
                55,"2946/2 Trq Mode Lo Spd",
                56,"4008/1 NetWordIN1",
                57,"4008/2 NetWordIN2",
                58,"4008/3 NetWordIN3",
                59,"4008/4 NetWordIN4",
                60,"400B/1 AC Drv Ctrl Word",
                61,"400B/2 C0135 Ctrl Word",
                62,"400B/3 Net Spd Stpnt Hz",
                63,"400B/4 Net Spd Stpnt RPM",
                64,"400B/5 Net Spd 0.01 Hz",
                65,"400B/6 NetSpdSign 0.1Hz",
                66,"400B/7 Net PID Stpnt",
                67,"400B/8 Net Torque Stpnt",
                68,"6040/0 Control Word",
                69,"6042/0 Target Veloc",
                70,"6046/1 Veloc Min",
                71,"6046/2 Veloc Max",
                72,"6048/1 Delta Speed",
                73,"6048/2 Delta Time",
                74,"6049/1 Delta Speed",
                75,"6049/2 Delta Time",
                76,"6060/0 402 Control Modes",
                77,"6071/0 402 TargetTorq",
                78,"6080/0 Mot Max Speed",
                79,"60E0/0 Pos TorqLimit",
                80,"60E1/0 Neg TorqLimit",
                82,"400B/13 Proc Input Freq";
        Param34000051 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Output#2",      $ name
                "",                     $ units
                "",                     $ help string
                0,65535,63,             $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000051 =
                0,"ignore",
                51,"SINT_OUT",
                52,"INT_OUT",
                53,"DINT_OUT",
                54,"2946/1 Trq Mode Hi Spd",
                55,"2946/2 Trq Mode Lo Spd",
                56,"4008/1 NetWordIN1",
                57,"4008/2 NetWordIN2",
                58,"4008/3 NetWordIN3",
                59,"4008/4 NetWordIN4",
                60,"400B/1 AC Drv Ctrl Word",
                61,"400B/2 C0135 Ctrl Word",
                62,"400B/3 Net Spd Stpnt Hz",
                63,"400B/4 Net Spd Stpnt RPM",
                64,"400B/5 Net Spd 0.01 Hz",
                65,"400B/6 NetSpdSign 0.1Hz",
                66,"400B/7 Net PID Stpnt",
                67,"400B/8 Net Torque Stpnt",
                68,"6040/0 Control Word",
                69,"6042/0 Target Veloc",
                70,"6046/1 Veloc Min",
                71,"6046/2 Veloc Max",
                72,"6048/1 Delta Speed",
                73,"6048/2 Delta Time",
                74,"6049/1 Delta Speed",
                75,"6049/2 Delta Time",
                76,"6060/0 402 Control Modes",
                77,"6071/0 402 TargetTorq",
                78,"6080/0 Mot Max Speed",
                79,"60E0/0 Pos TorqLimit",
                80,"60E1/0 Neg TorqLimit",
                82,"400B/13 Proc Input Freq";
        Param34000052 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Output#3",      $ name
                "",                     $ units
                "",                     $ help string
                0,65535,67,             $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000052 =
                0,"ignore",
                51,"SINT_OUT",
                52,"INT_OUT",
                53,"DINT_OUT",
                54,"2946/1 Trq Mode Hi Spd",
                55,"2946/2 Trq Mode Lo Spd",
                56,"4008/1 NetWordIN1",
                57,"4008/2 NetWordIN2",
                58,"4008/3 NetWordIN3",
                59,"4008/4 NetWordIN4",
                60,"400B/1 AC Drv Ctrl Word",
                61,"400B/2 C0135 Ctrl Word",
                62,"400B/3 Net Spd Stpnt Hz",
                63,"400B/4 Net Spd Stpnt RPM",
                64,"400B/5 Net Spd 0.01 Hz",
                65,"400B/6 NetSpdSign 0.1Hz",
                66,"400B/7 Net PID Stpnt",
                67,"400B/8 Net Torque Stpnt",
                68,"6040/0 Control Word",
                69,"6042/0 Target Veloc",
                70,"6046/1 Veloc Min",
                71,"6046/2 Veloc Max",
                72,"6048/1 Delta Speed",
                73,"6048/2 Delta Time",
                74,"6049/1 Delta Speed",
                75,"6049/2 Delta Time",
                76,"6060/0 402 Control Modes",
                77,"6071/0 402 TargetTorq",
                78,"6080/0 Mot Max Speed",
                79,"60E0/0 Pos TorqLimit",
                80,"60E1/0 Neg TorqLimit",
                82,"400B/13 Proc Input Freq";
        Param34000053 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Output#4",      $ name
                "",                     $ units
                "",                     $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000053 =
                0,"ignore",
                51,"SINT_OUT",
                52,"INT_OUT",
                53,"DINT_OUT",
                54,"2946/1 Trq Mode Hi Spd",
                55,"2946/2 Trq Mode Lo Spd",
                56,"4008/1 NetWordIN1",
                57,"4008/2 NetWordIN2",
                58,"4008/3 NetWordIN3",
                59,"4008/4 NetWordIN4",
                60,"400B/1 AC Drv Ctrl Word",
                61,"400B/2 C0135 Ctrl Word",
                62,"400B/3 Net Spd Stpnt Hz",
                63,"400B/4 Net Spd Stpnt RPM",
                64,"400B/5 Net Spd 0.01 Hz",
                65,"400B/6 NetSpdSign 0.1Hz",
                66,"400B/7 Net PID Stpnt",
                67,"400B/8 Net Torque Stpnt",
                68,"6040/0 Control Word",
                69,"6042/0 Target Veloc",
                70,"6046/1 Veloc Min",
                71,"6046/2 Veloc Max",
                72,"6048/1 Delta Speed",
                73,"6048/2 Delta Time",
                74,"6049/1 Delta Speed",
                75,"6049/2 Delta Time",
                76,"6060/0 402 Control Modes",
                77,"6071/0 402 TargetTorq",
                78,"6080/0 Mot Max Speed",
                79,"60E0/0 Pos TorqLimit",
                80,"60E1/0 Neg TorqLimit",
                82,"400B/13 Proc Input Freq";
        Param34000054 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Output#5",      $ name
                "",                     $ units
                "",                     $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000054 =
                0,"ignore",
                51,"SINT_OUT",
                52,"INT_OUT",
                53,"DINT_OUT",
                54,"2946/1 Trq Mode Hi Spd",
                55,"2946/2 Trq Mode Lo Spd",
                56,"4008/1 NetWordIN1",
                57,"4008/2 NetWordIN2",
                58,"4008/3 NetWordIN3",
                59,"4008/4 NetWordIN4",
                60,"400B/1 AC Drv Ctrl Word",
                61,"400B/2 C0135 Ctrl Word",
                62,"400B/3 Net Spd Stpnt Hz",
                63,"400B/4 Net Spd Stpnt RPM",
                64,"400B/5 Net Spd 0.01 Hz",
                65,"400B/6 NetSpdSign 0.1Hz",
                66,"400B/7 Net PID Stpnt",
                67,"400B/8 Net Torque Stpnt",
                68,"6040/0 Control Word",
                69,"6042/0 Target Veloc",
                70,"6046/1 Veloc Min",
                71,"6046/2 Veloc Max",
                72,"6048/1 Delta Speed",
                73,"6048/2 Delta Time",
                74,"6049/1 Delta Speed",
                75,"6049/2 Delta Time",
                76,"6060/0 402 Control Modes",
                77,"6071/0 402 TargetTorq",
                78,"6080/0 Mot Max Speed",
                79,"60E0/0 Pos TorqLimit",
                80,"60E1/0 Neg TorqLimit",
                82,"400B/13 Proc Input Freq";
        Param34000055 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Output#6",      $ name
                "",                     $ units
                "",                     $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000055 =
                0,"ignore",
                51,"SINT_OUT",
                52,"INT_OUT",
                53,"DINT_OUT",
                54,"2946/1 Trq Mode Hi Spd",
                55,"2946/2 Trq Mode Lo Spd",
                56,"4008/1 NetWordIN1",
                57,"4008/2 NetWordIN2",
                58,"4008/3 NetWordIN3",
                59,"4008/4 NetWordIN4",
                60,"400B/1 AC Drv Ctrl Word",
                61,"400B/2 C0135 Ctrl Word",
                62,"400B/3 Net Spd Stpnt Hz",
                63,"400B/4 Net Spd Stpnt RPM",
                64,"400B/5 Net Spd 0.01 Hz",
                65,"400B/6 NetSpdSign 0.1Hz",
                66,"400B/7 Net PID Stpnt",
                67,"400B/8 Net Torque Stpnt",
                68,"6040/0 Control Word",
                69,"6042/0 Target Veloc",
                70,"6046/1 Veloc Min",
                71,"6046/2 Veloc Max",
                72,"6048/1 Delta Speed",
                73,"6048/2 Delta Time",
                74,"6049/1 Delta Speed",
                75,"6049/2 Delta Time",
                76,"6060/0 402 Control Modes",
                77,"6071/0 402 TargetTorq",
                78,"6080/0 Mot Max Speed",
                79,"60E0/0 Pos TorqLimit",
                80,"60E1/0 Neg TorqLimit",
                82,"400B/13 Proc Input Freq";
        Param34000056 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Output#7",      $ name
                "",                     $ units
                "",                     $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000056 =
                0,"ignore",
                51,"SINT_OUT",
                52,"INT_OUT",
                53,"DINT_OUT",
                54,"2946/1 Trq Mode Hi Spd",
                55,"2946/2 Trq Mode Lo Spd",
                56,"4008/1 NetWordIN1",
                57,"4008/2 NetWordIN2",
                58,"4008/3 NetWordIN3",
                59,"4008/4 NetWordIN4",
                60,"400B/1 AC Drv Ctrl Word",
                61,"400B/2 C0135 Ctrl Word",
                62,"400B/3 Net Spd Stpnt Hz",
                63,"400B/4 Net Spd Stpnt RPM",
                64,"400B/5 Net Spd 0.01 Hz",
                65,"400B/6 NetSpdSign 0.1Hz",
                66,"400B/7 Net PID Stpnt",
                67,"400B/8 Net Torque Stpnt",
                68,"6040/0 Control Word",
                69,"6042/0 Target Veloc",
                70,"6046/1 Veloc Min",
                71,"6046/2 Veloc Max",
                72,"6048/1 Delta Speed",
                73,"6048/2 Delta Time",
                74,"6049/1 Delta Speed",
                75,"6049/2 Delta Time",
                76,"6060/0 402 Control Modes",
                77,"6071/0 402 TargetTorq",
                78,"6080/0 Mot Max Speed",
                79,"60E0/0 Pos TorqLimit",
                80,"60E1/0 Neg TorqLimit",
                82,"400B/13 Proc Input Freq";
        Param34000057 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Output#8",      $ name
                "",                     $ units
                "",                     $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000057 =
                0,"ignore",
                51,"SINT_OUT",
                52,"INT_OUT",
                53,"DINT_OUT",
                54,"2946/1 Trq Mode Hi Spd",
                55,"2946/2 Trq Mode Lo Spd",
                56,"4008/1 NetWordIN1",
                57,"4008/2 NetWordIN2",
                58,"4008/3 NetWordIN3",
                59,"4008/4 NetWordIN4",
                60,"400B/1 AC Drv Ctrl Word",
                61,"400B/2 C0135 Ctrl Word",
                62,"400B/3 Net Spd Stpnt Hz",
                63,"400B/4 Net Spd Stpnt RPM",
                64,"400B/5 Net Spd 0.01 Hz",
                65,"400B/6 NetSpdSign 0.1Hz",
                66,"400B/7 Net PID Stpnt",
                67,"400B/8 Net Torque Stpnt",
                68,"6040/0 Control Word",
                69,"6042/0 Target Veloc",
                70,"6046/1 Veloc Min",
                71,"6046/2 Veloc Max",
                72,"6048/1 Delta Speed",
                73,"6048/2 Delta Time",
                74,"6049/1 Delta Speed",
                75,"6049/2 Delta Time",
                76,"6060/0 402 Control Modes",
                77,"6071/0 402 TargetTorq",
                78,"6080/0 Mot Max Speed",
                79,"60E0/0 Pos TorqLimit",
                80,"60E1/0 Neg TorqLimit",
                82,"400B/13 Proc Input Freq";
        Param34000058 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Output#9",      $ name
                "",                     $ units
                "",                     $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000058 =
                0,"ignore",
                51,"SINT_OUT",
                52,"INT_OUT",
                53,"DINT_OUT",
                54,"2946/1 Trq Mode Hi Spd",
                55,"2946/2 Trq Mode Lo Spd",
                56,"4008/1 NetWordIN1",
                57,"4008/2 NetWordIN2",
                58,"4008/3 NetWordIN3",
                59,"4008/4 NetWordIN4",
                60,"400B/1 AC Drv Ctrl Word",
                61,"400B/2 C0135 Ctrl Word",
                62,"400B/3 Net Spd Stpnt Hz",
                63,"400B/4 Net Spd Stpnt RPM",
                64,"400B/5 Net Spd 0.01 Hz",
                65,"400B/6 NetSpdSign 0.1Hz",
                66,"400B/7 Net PID Stpnt",
                67,"400B/8 Net Torque Stpnt",
                68,"6040/0 Control Word",
                69,"6042/0 Target Veloc",
                70,"6046/1 Veloc Min",
                71,"6046/2 Veloc Max",
                72,"6048/1 Delta Speed",
                73,"6048/2 Delta Time",
                74,"6049/1 Delta Speed",
                75,"6049/2 Delta Time",
                76,"6060/0 402 Control Modes",
                77,"6071/0 402 TargetTorq",
                78,"6080/0 Mot Max Speed",
                79,"60E0/0 Pos TorqLimit",
                80,"60E1/0 Neg TorqLimit",
                82,"400B/13 Proc Input Freq";
        Param34000059 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Output#10",     $ name
                "",                     $ units
                "",                     $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000059 =
                0,"ignore",
                51,"SINT_OUT",
                52,"INT_OUT",
                53,"DINT_OUT",
                54,"2946/1 Trq Mode Hi Spd",
                55,"2946/2 Trq Mode Lo Spd",
                56,"4008/1 NetWordIN1",
                57,"4008/2 NetWordIN2",
                58,"4008/3 NetWordIN3",
                59,"4008/4 NetWordIN4",
                60,"400B/1 AC Drv Ctrl Word",
                61,"400B/2 C0135 Ctrl Word",
                62,"400B/3 Net Spd Stpnt Hz",
                63,"400B/4 Net Spd Stpnt RPM",
                64,"400B/5 Net Spd 0.01 Hz",
                65,"400B/6 NetSpdSign 0.1Hz",
                66,"400B/7 Net PID Stpnt",
                67,"400B/8 Net Torque Stpnt",
                68,"6040/0 Control Word",
                69,"6042/0 Target Veloc",
                70,"6046/1 Veloc Min",
                71,"6046/2 Veloc Max",
                72,"6048/1 Delta Speed",
                73,"6048/2 Delta Time",
                74,"6049/1 Delta Speed",
                75,"6049/2 Delta Time",
                76,"6060/0 402 Control Modes",
                77,"6071/0 402 TargetTorq",
                78,"6080/0 Mot Max Speed",
                79,"60E0/0 Pos TorqLimit",
                80,"60E1/0 Neg TorqLimit",
                82,"400B/13 Proc Input Freq";
        Param34000060 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Output#11",     $ name
                "",                     $ units
                "",                     $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000060 =
                0,"ignore",
                51,"SINT_OUT",
                52,"INT_OUT",
                53,"DINT_OUT",
                54,"2946/1 Trq Mode Hi Spd",
                55,"2946/2 Trq Mode Lo Spd",
                56,"4008/1 NetWordIN1",
                57,"4008/2 NetWordIN2",
                58,"4008/3 NetWordIN3",
                59,"4008/4 NetWordIN4",
                60,"400B/1 AC Drv Ctrl Word",
                61,"400B/2 C0135 Ctrl Word",
                62,"400B/3 Net Spd Stpnt Hz",
                63,"400B/4 Net Spd Stpnt RPM",
                64,"400B/5 Net Spd 0.01 Hz",
                65,"400B/6 NetSpdSign 0.1Hz",
                66,"400B/7 Net PID Stpnt",
                67,"400B/8 Net Torque Stpnt",
                68,"6040/0 Control Word",
                69,"6042/0 Target Veloc",
                70,"6046/1 Veloc Min",
                71,"6046/2 Veloc Max",
                72,"6048/1 Delta Speed",
                73,"6048/2 Delta Time",
                74,"6049/1 Delta Speed",
                75,"6049/2 Delta Time",
                76,"6060/0 402 Control Modes",
                77,"6071/0 402 TargetTorq",
                78,"6080/0 Mot Max Speed",
                79,"60E0/0 Pos TorqLimit",
                80,"60E1/0 Neg TorqLimit",
                82,"400B/13 Proc Input Freq";
        Param34000061 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Output#12",     $ name
                "",                     $ units
                "",                     $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000061 =
                0,"ignore",
                51,"SINT_OUT",
                52,"INT_OUT",
                53,"DINT_OUT",
                54,"2946/1 Trq Mode Hi Spd",
                55,"2946/2 Trq Mode Lo Spd",
                56,"4008/1 NetWordIN1",
                57,"4008/2 NetWordIN2",
                58,"4008/3 NetWordIN3",
                59,"4008/4 NetWordIN4",
                60,"400B/1 AC Drv Ctrl Word",
                61,"400B/2 C0135 Ctrl Word",
                62,"400B/3 Net Spd Stpnt Hz",
                63,"400B/4 Net Spd Stpnt RPM",
                64,"400B/5 Net Spd 0.01 Hz",
                65,"400B/6 NetSpdSign 0.1Hz",
                66,"400B/7 Net PID Stpnt",
                67,"400B/8 Net Torque Stpnt",
                68,"6040/0 Control Word",
                69,"6042/0 Target Veloc",
                70,"6046/1 Veloc Min",
                71,"6046/2 Veloc Max",
                72,"6048/1 Delta Speed",
                73,"6048/2 Delta Time",
                74,"6049/1 Delta Speed",
                75,"6049/2 Delta Time",
                76,"6060/0 402 Control Modes",
                77,"6071/0 402 TargetTorq",
                78,"6080/0 Mot Max Speed",
                79,"60E0/0 Pos TorqLimit",
                80,"60E1/0 Neg TorqLimit",
                82,"400B/13 Proc Input Freq";
        Param34000062 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Output#13",     $ name
                "",                     $ units
                "",                     $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000062 =
                0,"ignore",
                51,"SINT_OUT",
                52,"INT_OUT",
                53,"DINT_OUT",
                54,"2946/1 Trq Mode Hi Spd",
                55,"2946/2 Trq Mode Lo Spd",
                56,"4008/1 NetWordIN1",
                57,"4008/2 NetWordIN2",
                58,"4008/3 NetWordIN3",
                59,"4008/4 NetWordIN4",
                60,"400B/1 AC Drv Ctrl Word",
                61,"400B/2 C0135 Ctrl Word",
                62,"400B/3 Net Spd Stpnt Hz",
                63,"400B/4 Net Spd Stpnt RPM",
                64,"400B/5 Net Spd 0.01 Hz",
                65,"400B/6 NetSpdSign 0.1Hz",
                66,"400B/7 Net PID Stpnt",
                67,"400B/8 Net Torque Stpnt",
                68,"6040/0 Control Word",
                69,"6042/0 Target Veloc",
                70,"6046/1 Veloc Min",
                71,"6046/2 Veloc Max",
                72,"6048/1 Delta Speed",
                73,"6048/2 Delta Time",
                74,"6049/1 Delta Speed",
                75,"6049/2 Delta Time",
                76,"6060/0 402 Control Modes",
                77,"6071/0 402 TargetTorq",
                78,"6080/0 Mot Max Speed",
                79,"60E0/0 Pos TorqLimit",
                80,"60E1/0 Neg TorqLimit",
                82,"400B/13 Proc Input Freq";
        Param34000063 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Output#14",     $ name
                "",                     $ units
                "",                     $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000063 =
                0,"ignore",
                51,"SINT_OUT",
                52,"INT_OUT",
                53,"DINT_OUT",
                54,"2946/1 Trq Mode Hi Spd",
                55,"2946/2 Trq Mode Lo Spd",
                56,"4008/1 NetWordIN1",
                57,"4008/2 NetWordIN2",
                58,"4008/3 NetWordIN3",
                59,"4008/4 NetWordIN4",
                60,"400B/1 AC Drv Ctrl Word",
                61,"400B/2 C0135 Ctrl Word",
                62,"400B/3 Net Spd Stpnt Hz",
                63,"400B/4 Net Spd Stpnt RPM",
                64,"400B/5 Net Spd 0.01 Hz",
                65,"400B/6 NetSpdSign 0.1Hz",
                66,"400B/7 Net PID Stpnt",
                67,"400B/8 Net Torque Stpnt",
                68,"6040/0 Control Word",
                69,"6042/0 Target Veloc",
                70,"6046/1 Veloc Min",
                71,"6046/2 Veloc Max",
                72,"6048/1 Delta Speed",
                73,"6048/2 Delta Time",
                74,"6049/1 Delta Speed",
                75,"6049/2 Delta Time",
                76,"6060/0 402 Control Modes",
                77,"6071/0 402 TargetTorq",
                78,"6080/0 Mot Max Speed",
                79,"60E0/0 Pos TorqLimit",
                80,"60E1/0 Neg TorqLimit",
                82,"400B/13 Proc Input Freq";
        Param34000064 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Output#15",     $ name
                "",                     $ units
                "",                     $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000064 =
                0,"ignore",
                51,"SINT_OUT",
                52,"INT_OUT",
                53,"DINT_OUT",
                54,"2946/1 Trq Mode Hi Spd",
                55,"2946/2 Trq Mode Lo Spd",
                56,"4008/1 NetWordIN1",
                57,"4008/2 NetWordIN2",
                58,"4008/3 NetWordIN3",
                59,"4008/4 NetWordIN4",
                60,"400B/1 AC Drv Ctrl Word",
                61,"400B/2 C0135 Ctrl Word",
                62,"400B/3 Net Spd Stpnt Hz",
                63,"400B/4 Net Spd Stpnt RPM",
                64,"400B/5 Net Spd 0.01 Hz",
                65,"400B/6 NetSpdSign 0.1Hz",
                66,"400B/7 Net PID Stpnt",
                67,"400B/8 Net Torque Stpnt",
                68,"6040/0 Control Word",
                69,"6042/0 Target Veloc",
                70,"6046/1 Veloc Min",
                71,"6046/2 Veloc Max",
                72,"6048/1 Delta Speed",
                73,"6048/2 Delta Time",
                74,"6049/1 Delta Speed",
                75,"6049/2 Delta Time",
                76,"6060/0 402 Control Modes",
                77,"6071/0 402 TargetTorq",
                78,"6080/0 Mot Max Speed",
                79,"60E0/0 Pos TorqLimit",
                80,"60E1/0 Neg TorqLimit",
                82,"400B/13 Proc Input Freq";
        Param34000065 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Output#16",     $ name
                "",                     $ units
                "",                     $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000065 =
                0,"ignore",
                51,"SINT_OUT",
                52,"INT_OUT",
                53,"DINT_OUT",
                54,"2946/1 Trq Mode Hi Spd",
                55,"2946/2 Trq Mode Lo Spd",
                56,"4008/1 NetWordIN1",
                57,"4008/2 NetWordIN2",
                58,"4008/3 NetWordIN3",
                59,"4008/4 NetWordIN4",
                60,"400B/1 AC Drv Ctrl Word",
                61,"400B/2 C0135 Ctrl Word",
                62,"400B/3 Net Spd Stpnt Hz",
                63,"400B/4 Net Spd Stpnt RPM",
                64,"400B/5 Net Spd 0.01 Hz",
                65,"400B/6 NetSpdSign 0.1Hz",
                66,"400B/7 Net PID Stpnt",
                67,"400B/8 Net Torque Stpnt",
                68,"6040/0 Control Word",
                69,"6042/0 Target Veloc",
                70,"6046/1 Veloc Min",
                71,"6046/2 Veloc Max",
                72,"6048/1 Delta Speed",
                73,"6048/2 Delta Time",
                74,"6049/1 Delta Speed",
                75,"6049/2 Delta Time",
                76,"6060/0 402 Control Modes",
                77,"6071/0 402 TargetTorq",
                78,"6080/0 Mot Max Speed",
                79,"60E0/0 Pos TorqLimit",
                80,"60E1/0 Neg TorqLimit",
                82,"400B/13 Proc Input Freq";

        Param34000100 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Input Trailer",        $ name
                "",                     $ units
                "",                     $ help string
                100,100,100,            $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param34000101 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Output Trailer",       $ name
                "",                     $ units
                "",                     $ help string
                101,101,101,            $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places



        Param34000200 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Input#1",              $ name
                "",                     $ units
                "",                     $ help string
                29,29,29,               $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000200 =
                29,"400C/1 AC Drv Stat Word";
        Param34000201 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Input#2",              $ name
                "",                     $ units
                "",                     $ help string
                32,32,32,               $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000201 =
                32,"400C/4 Actual Speed RPM";
        Param34000202 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Input#3",              $ name
                "",                     $ units
                "",                     $ help string
                35,35,35,               $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000202 =
                35,"400C/7 Actual Torque Scaled";


        Param34000250 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Output#1",             $ name
                "",                     $ units
                "",                     $ help string
                60,60,60,               $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000250 =
                60,"400B/1 AC Drv Ctrl Word";
        Param34000251 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Output#2",             $ name
                "",                     $ units
                "",                     $ help string
                63,63,63,               $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000251 =
                63,"400B/4 Net Spd Stpnt RPM";
        Param34000252 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Output#3",             $ name
                "",                     $ units
                "",                     $ help string
                67,67,67,               $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000252 =
                67,"400B/8 Net Torque Stpnt";


[Assembly]
        Object_Name = "Assembly Object";
        Object_Class_Code = 0x04;

        Assem20 =                       $ Assemb21 selected by parameter Param1000
                "Speed Ctrl Out",
                ,
                4,
                0x0001,
                ,,
                16,Param60,
                16,Param63;
        Assem22 =                       $ Assemb23 selected by parameter Param1002
                "Speed & Torque Ctrl Out",
                ,
                6,
                0x0001,
                ,,
                16,Param60,
                16,Param63,
                16,Param67;
        Assem70 =                       $ Assemb71 selected by parameter Param1001
                "Speed Ctrl Inp",
                ,
                4,
                0x0001,
                ,,
                16,Param29,
                16,Param32;
        Assem72 =                       $ Assemb73 selected by parameter Param1003
                "Speed & Torque Ctrl Inp",
                ,
                6,
                0x0001,
                ,,
                16,Param29,
                16,Param32,
                16,Param35;
        Assem110 =
                "Custom Output Assembly",
                ,
                ,
                0x0001,
                ,,
                ,Param34000050,
                ,Param34000051,
                ,Param34000052,
                ,Param34000053,
                ,Param34000054,
                ,Param34000055,
                ,Param34000056,
                ,Param34000057,
                ,Param34000058,
                ,Param34000059,
                ,Param34000060,
                ,Param34000061,
                ,Param34000062,
                ,Param34000063,
                ,Param34000064,
                ,Param34000065,
                32,Param34000101;
        Assem111 =
                "Custom Input Assembly",
                ,
                ,
                0x0001,
                ,,
                ,Param34000000,
                ,Param34000001,
                ,Param34000002,
                ,Param34000003,
                ,Param34000004,
                ,Param34000005,
                ,Param34000006,
                ,Param34000007,
                ,Param34000008,
                ,Param34000009,
                ,Param34000010,
                ,Param34000011,
                ,Param34000012,
                ,Param34000013,
                ,Param34000014,
                ,Param34000015,
                32,Param34000100;
        Assem130 =
                "Config Assembly",
                ,
                ,
                0x0801,
                ,,
                16,Param34000000,
                16,Param34000001,
                16,Param34000002,
                16,Param34000003,
                16,Param34000004,
                16,Param34000005,
                16,Param34000006,
                16,Param34000007,
                16,Param34000008,
                16,Param34000009,
                16,Param34000010,
                16,Param34000011,
                16,Param34000012,
                16,Param34000013,
                16,Param34000014,
                16,Param34000015,
                16,Param34000100,

                16,Param34000050,
                16,Param34000051,
                16,Param34000052,
                16,Param34000053,
                16,Param34000054,
                16,Param34000055,
                16,Param34000056,
                16,Param34000057,
                16,Param34000058,
                16,Param34000059,
                16,Param34000060,
                16,Param34000061,
                16,Param34000062,
                16,Param34000063,
                16,Param34000064,
                16,Param34000065,
                16,Param34000101;

[Connection Manager]
        Revision = 1;
        Object_Name = "Connection Manager Object";
        Object_Class_Code = 0x06;
        MaxInst = 1;
        Number_Of_Static_Instances = 1;
        Max_Number_Of_Dynamic_Instances = 0;
        Connection1 =
                0x04010002,             $ 0-15    = supported transport classes
                                        $ 16      = trigger: cyclic
                                        $ 17      = trigger: change of state
                                        $ 18      = trigger: application
                                        $ 19-23   = trigger: reserved
                                        $ 24      = application type: listen-only
                                        $ 25      = application type: input-only
                                        $ 26      = application type: exclusive-owner
                                        $ 27      = application type: redundant-owner
                                        $ 28-30   = reserved
                                        $ 31      = Direction: Client = 0 / Server = 1
                0x4464040F,             $ 0       = O->T fixed size supported
                                        $ 1       = O->T variable size supported
                                        $ 2       = T->O fixed size supported
                                        $ 3       = T->O variable size supported
                                        $ 4-5     = O->T number of bytes per slot (obsolete)
                                        $ 6-7     = T->O number of bytes per slot (obsolete)
                                        $ 8-10    = O->T Real time transfer format
                                        $ 11      = reserved
                                        $ 12-14   = T->O Real time transfer format
                                        $ 15      = reserved
                                        $ 16      = O->T connection type: NULL
                                        $ 17      = O->T connection type: MULTICAST
                                        $ 18      = O->T connection type: POINT2POINT
                                        $ 19      = O->T connection type: reserved
                                        $ 20      = T->O connection type: NULL
                                        $ 21      = T->O connection type: MULTICAST
                                        $ 22      = T->O connection type: POINT2POINT
                                        $ 23      = T->O connection type: reserved
                                        $ 24      = O->T priority: LOW
                                        $ 25      = O->T priority: HIGH
                                        $ 26      = O->T priority: SCHEDULED
                                        $ 27      = O->T priority: reserved
                                        $ 28      = T->O priority: LOW
                                        $ 29      = T->O priority: HIGH
                                        $ 30      = T->O priority: SCHEDULED
                                        $ 31      = T->O priority: reserved
                Param2000,4,Assem20,    $ O->T RPI, size, format
                Param2000,4,Assem70,    $ T->O RPI, size, format
                ,,                      $ proxy config size, format
                0,,                     $ target config size, format
                "Speed",                $ Connection Name
                "",                     $ help string
                "20 04 24 82 2C [Param1000] 2C [Param1001]";    $ Path
        Connection2 =
                0x04010002,             $ 0-15    = supported transport classes
                                        $ 16      = trigger: cyclic
                                        $ 17      = trigger: change of state
                                        $ 18      = trigger: application
                                        $ 19-23   = trigger: reserved
                                        $ 24      = application type: listen-only
                                        $ 25      = application type: input-only
                                        $ 26      = application type: exclusive-owner
                                        $ 27      = application type: redundant-owner
                                        $ 28-30   = reserved
                                        $ 31      = Direction: Client = 0 / Server = 1
                0x4464040F,             $ 0       = O->T fixed size supported
                                        $ 1       = O->T variable size supported
                                        $ 2       = T->O fixed size supported
                                        $ 3       = T->O variable size supported
                                        $ 4-5     = O->T number of bytes per slot (obsolete)
                                        $ 6-7     = T->O number of bytes per slot (obsolete)
                                        $ 8-10    = O->T Real time transfer format
                                        $ 11      = reserved
                                        $ 12-14   = T->O Real time transfer format
                                        $ 15      = reserved
                                        $ 16      = O->T connection type: NULL
                                        $ 17      = O->T connection type: MULTICAST
                                        $ 18      = O->T connection type: POINT2POINT
                                        $ 19      = O->T connection type: reserved
                                        $ 20      = T->O connection type: NULL
                                        $ 21      = T->O connection type: MULTICAST
                                        $ 22      = T->O connection type: POINT2POINT
                                        $ 23      = T->O connection type: reserved
                                        $ 24      = O->T priority: LOW
                                        $ 25      = O->T priority: HIGH
                                        $ 26      = O->T priority: SCHEDULED
                                        $ 27      = O->T priority: reserved
                                        $ 28      = T->O priority: LOW
                                        $ 29      = T->O priority: HIGH
                                        $ 30      = T->O priority: SCHEDULED
                                        $ 31      = T->O priority: reserved
                Param2000,6,Assem22,    $ O->T RPI, size, format
                Param2000,6,Assem72,    $ T->O RPI, size, format
                ,,                      $ proxy config size, format
                0,,                     $ target config size, format
                "Speed & Torque",       $ Connection Name
                "",                     $ help string
                "20 04 24 82 2C [Param1002] 2C [Param1003]";    $ Path
        Connection3 =
                0x04010002,             $ 0-15    = supported transport classes
                                        $ 16      = trigger: cyclic
                                        $ 17      = trigger: change of state
                                        $ 18      = trigger: application
                                        $ 19-23   = trigger: reserved
                                        $ 24      = application type: listen-only
                                        $ 25      = application type: input-only
                                        $ 26      = application type: exclusive-owner
                                        $ 27      = application type: redundant-owner
                                        $ 28-30   = reserved
                                        $ 31      = Direction: Client = 0 / Server = 1
                0x4464040F,             $ 0       = O->T fixed size supported
                                        $ 1       = O->T variable size supported
                                        $ 2       = T->O fixed size supported
                                        $ 3       = T->O variable size supported
                                        $ 4-5     = O->T number of bytes per slot (obsolete)
                                        $ 6-7     = T->O number of bytes per slot (obsolete)
                                        $ 8-10    = O->T Real time transfer format
                                        $ 11      = reserved
                                        $ 12-14   = T->O Real time transfer format
                                        $ 15      = reserved
                                        $ 16      = O->T connection type: NULL
                                        $ 17      = O->T connection type: MULTICAST
                                        $ 18      = O->T connection type: POINT2POINT
                                        $ 19      = O->T connection type: reserved
                                        $ 20      = T->O connection type: NULL
                                        $ 21      = T->O connection type: MULTICAST
                                        $ 22      = T->O connection type: POINT2POINT
                                        $ 23      = T->O connection type: reserved
                                        $ 24      = O->T priority: LOW
                                        $ 25      = O->T priority: HIGH
                                        $ 26      = O->T priority: SCHEDULED
                                        $ 27      = O->T priority: reserved
                                        $ 28      = T->O priority: LOW
                                        $ 29      = T->O priority: HIGH
                                        $ 30      = T->O priority: SCHEDULED
                                        $ 31      = T->O priority: reserved
                Param2000,,Assem110,    $ O->T RPI, size, format
                Param2000,,Assem111,    $ T->O RPI, size, format
                ,,                      $ proxy config size, format
                ,Assem130,              $ target config size, format
                "Custom I/O Connection",$ Connection Name
                "",                     $ help string
                "20 04 24 82 2C 6E 2C 6F";    $ Path

[Port]
        Revision = 2;
        Object_Name = "Port Object";
        Object_Class_Code = 0xF4;
        MaxInst = 2;
        Number_Of_Static_Instances = 2;
        Max_Number_Of_Dynamic_Instances = 0;
        Port1 =
                TCP,
                "Port 1",
                "20 F5 24 01",
                1,
                63,
                ;

[Capacity]

        ConnOverhead = .004;            $ Connection Overhead

        MaxIOConnections = 3;           $ Maximum number of Class 1 Connections
        MaxMsgConnections = 5;          $ Maximum number of Class 3 Connections
        TSpec1 = TxRx, 10, 1400;        $ packets per sec @ 10 bytes
        TSpec2 = TxRx, 100, 1300;       $ packets per sec @ 100 bytes
        TSpec3 = TxRx, 200, 1120;       $ packets per sec @ 200 bytes

[DLR Class]
        Revision = 3;
        Object_Name = "Device Level Ring Object";
        Object_Class_Code = 0x47;
        MaxInst = 1;
        Number_Of_Static_Instances = 1;
        Max_Number_Of_Dynamic_Instances = 0;

[Ethernet Link Class]
        Revision = 4;
        Object_Name = "Ethernet Link Object";
        Object_Class_Code = 0xF6;
        MaxInst = 2;
        Number_Of_Static_Instances = 2;
        Max_Number_Of_Dynamic_Instances = 0;
        Class_Attributes =
                2,
                3;
        Instance_Attributes =
                1,
                2,
                3,
                6,
                7,
                8,
                9,
                10;
        Class_Services = 0x0E;
        Instance_Services =
                0x0E,
                0x10;
        InterfaceLabel1 = "P1";
        InterfaceLabel2 = "P2";
        InterfaceType1 = 2;
        InterfaceType2 = 2;

