$ EZ-EDS Version 3.36.1.20241010 Generated Electronic Data Sheet

[File]
        DescText = "EDS file for Lenze i650 motec Inverter Drive ES with CIP Safety";
        CreateDate = 09-19-2023;
        CreateTime = 15:50:09;
        ModDate = 11-19-2024;
        ModTime = 10:36:04;
        Revision = 1.1;
        HomeURL = "https://www.lenze.com";
        EDSFileCRC = 0xB650F00B;

[Device]
        VendCode = 587;
        VendName = "Lenze";
        ProdType = 2;
        ProdTypeStr = "AC Drive Device";
        ProdCode = 601;
        MajRev = 6;
        MinRev = 1;
        ProdName = "i650 motec-ES";
        Catalog = "Inverter Drive i650 motec with Extended Safety";
        Icon = "i650motec_CIP_Safety_eip_eds_icon.ico";
        IconContents =
                "AAABAAEAQEAAAAEACAAoFgAAFgAAACgAAABAAAAAgAAAAAEACAAAAAAAABYA"
                "AAAAAAAAAAAAAAAAAAAAAAD///8A/v7+APz8/ADz+/8A+vr6APn5+QD39/cA"
                "5vb+APb29QD09PMA8/LwANjw/QDx8O8AFf//AO/u7QAR//8Ay+v9AO3s6gAU"
                "+/8A5OvuAOvq6AAV+P8Aveb8AOno5gAV9P8AEvT/AObl5QAW8v8AFfD/ACHx"
                "9wCv4PsAFe7/AOPi4QDh4N8AFOv8AN/f3QCh2/sAEev1AN3d3ADc3NkAD+X9"
                "AJLW+gDa2dcAQuHtABLk8QDY19UA1dXTAIPQ+QAT3+wA09LRACDd6ADR0M8A"
                "dMv5AA/Z6ADNzcwANdbeABfY3gCF0NMAzMvJAA3P+gDKysgAY8X4AMnIxgDG"
                "xsUAGNHXAFTA+ADFxMMACcX5AMLCwQASytsAdrziAEG79wC/vr0AE8fUAL28"
                "ugAHvPcAjbjQALu6uAAWxMwALrT2ALi4twC4trMAtrWzABqw9gAVvscAtLOy"
                "ADu5wwCysbAA+6upABe5wwAfquwAr66tAACq9QBCqt4AD6nwABi3uQCsq6sA"
                "FrG/AKqppwALpOkAqKelAKWkowALnuEAoqGgABOd3QAXqKwAn56dAAOa3gAa"
                "l9IAm5qZABKhrgALltUAGJ+nAJiXlgAaoKEAlZSTABKQywAhkMUAk5KPAJCP"
                "jQAIisYAO4qyACiKuACNjIsAE5GbAIqKiAANhLsAiIeFAC6DqwAYi5MAhYSD"
                "AB2KjQAyf6MAgYB/ABiFigA1fJ4AfX18AHt7eQA7dpEAeHZ1ABt6fgB0c3MA"
                "H3l4AEBvgwAXbZcAb29vAB1zdQBtbW0AQmt+AA9pkwBra2sARmh2AGhoaABT"
                "Z3IASGZxACJqbwBlZGQAYWJhAExhZwA2X3UAXl5eABxiZQBcW1sAIV9gAFFZ"
                "WABYWFgAKlZsABtaXwBVVVQAUlJRACVVVQBXUkkAT09PACdRUQBNTU0ASkpK"
                "AC1KTQBcSjkAR0dHAARFYgAjR0sARUVFACdFRQBCQkIANUBGAEFAQAA/Pz8A"
                "MkBAAGFCJwA+Pj4APDw8ACQ7RwApPT4AOjo6ADc3NwApNzoAZjsVADY2NgBB"
                "NTUANDQ0ADMzMwA8MjEAMjIyACUxOAA5MTEAMTExAEMvLQAwMDAALy8vACAt"
                "MwApLS8ALS0tADQsLAASKzkALCwsACsqKgApKSkANignACcnKAAyJiYAJiYm"
                "AEEkIgAlJSUALyQjACMjIwAiIiEANCAgAC0gIAAgICAAGB8jABAeJQAeHh4A"
                "LRwcABwcHAAaGhoAMhgXAC0XFgAXFxcAFRUVAC0TEgAUFBMAMBAQACgQDwAS"
                "ERAAMA4NAA8PDgAXDgsAHw0LAC4LCQANDAsADAoJAAkHBAAHBQMABgMBAAQC"
                "AAABAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAYAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAhAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAgYjwAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAQIKGjEuLjZIAQAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAB"
                "SG2IYmRkPyc+AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAEECBo2V4WgzdfNz6lQGiBEPAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAABCSA2ZIWl2PDz59zTzcXCyMrkqD5n"
                "hZx3AQAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAQoCAABExcjg"
                "6ure2M/Hxc/T1tja3uTg1trpultI/y0ABggAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAEFDjNnmNbptQgAr9zT09PT09rg5+rt8/P5+/79/tjNyM2oV/VlBnNi"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAOVXed2vXw3tPCwdrpluTW1tDNytPu/f3/"
                "/v3+/Pz7+/3Yz8q6x9fqcyp7YAAAAAAAAAAAAAAAAAAAAQlCEQAB3ufn2tPI"
                "ytPT2NjT0+HIzcfTsq/W8P/8+/v7+/v7/Pv92MjKvr3C7nsUcWAAAAAAAAAA"
                "AAAABBpIiNjq1uo8ZdjT09PT2NfQ5NfHyMjIyMjXomBqtfn59f78/Pz///v7"
                "/djHyr69wfN9CSc+AQAAAAAAAip2oND19enPws/T9erI0NPNxcXNt3uv08jI"
                "yMjH6meu3pP++vr18/3/r8r//P3a4NjBvb71fRcXGgIAAAAABeHt7t66oHEh"
                "rODQx83Kx8fHx8jN03OsidPHyMjIx+l3pZy+9frh6uT/cQgBrPn64Eilx7q+"
                "84IMKiMCAAAAAH3WlnMzGiYRAKLhwsjIyMjIyMjI2qCgvZHYxcjIyMjKx429"
                "2vD9/Pr73gkOAnPq89hgpce9vu2NCiEMAAAAAFtVMwkEAD8uMQCl5MXIyMjI"
                "yMjIyM3Qgo2s18jNz83KyNPq3Mjt8/n68P86AAXQ//7kzb7BvcHtkxEIAAAA"
                "AABtIyZIIQlCLT4AouTCyMjIyMjIyMjIz9be18jQ0MfTzcjW3NfX8/Xp9dz7"
                "86Xp//v83srHwb3B7pMOCAAAAAABVTEgIS4XREQaAKXkx8rIyMjIyMjIyMrH"
                "yMjQx7KvvtPKwoKCxfX79fnk/vz//vv7/N7HyMG9vu6RDggAAAAABU0zV0IA"
                "CiYFFwCs58LIyMjIyMjIyMjQyK/I07e60LLa5IKYqZb+5/X8//v8+/v7+/zg"
                "wsjBvb7tnA4JAAAAAAZQIxQRATE6LjwgwohIx8jIyMrKysrK3n1ngti61r63"
                "4edzt6Wp+v77+/v7+/v8/P3/1sjHvr2+6agKDAAAAAAFUDNEIAEzNjYuKrWc"
                "k9DKysjIyMjK4JyW05Haz76319rWrJGl4PD+/P39/f79+/r58MfB2tC5vues"
                "CgwAAAAABVUuSAAAMUhgkcXX3tDKyMrKysrKyte1jaig2M/T3NzKzdi+0M/u"
                "+vb39/Ly6N/TyLvAz9Dt2LnnrAoMAAAAAAh7i5N7k8f1+fDw19zHyMrKysrK"
                "ysrI2LKi4NDTwsLFx8LJzt30+OPSsKqbjIZ8YUksD6Hv3O3g7qkJDAAAAAAJ"
                "qajT/frq4efq6tbax8rKysrKys3KysrW3tTUzMzZ3+PStJuDcFlURSwZDw8N"
                "DQ0NFQ1U38Xk3M+yCg4AAAAAAcLe19DF4drW19fT2sfKzcrIx8XU4uvr28fA"
                "tKeMcE4wJSIcGRINEhIVGBscHBwbGxsYD7bCwpiNxRcRAAAAAALNx83X4Ofg"
                "3Ofw2NbHx8LH4vjsw6OSgW5JJQ8NDQ0YHB8fHx8fHx8cHBwcHBsbHBsbHw2B"
                "2bnB6cEXDgAAAAIMmOnq6ent8/v8+dfeytfT04xZSTUfDw8NEhgfHx8fHBwf"
                "HBwcHB8cHBwcGxscGxsbGxwoNdS9veDBFw4AAADn2NPh3Onk2tPNyM3Kz8rK"
                "zcMPGxgbHB8fHx8fHx8fHx8fHx8fHx8fHBwcHBwbGxwbGxsiVjetxr3cwRQU"
                "AAAA2MrW57h0XFxcXFxcXFxcXFxcXFxcXFxcXFxcXFxcXFxobFxcXFxDHxwc"
                "HxwcGxsYHBsZMlg5qsa92M0aFwAAANfP19FvXFxcXGh1XHVsdWNcXFxodVxo"
                "dXVobFx1Y1x1hMSAXFxcXEMbHBwcHBgbGxsbGCIrHa3GutbcIxQAAADYz9Jv"
                "XFxcXGjEvJfEl8R1XFxoxLyesbzEiqSPvLyHxHXEl1xcXFxcOxwcHBwbGxsb"
                "GxscGSXWvbrW3CMUAAAA2M/DXFxcXFx1xICPxJfEl2xcY4+rsY+8xIqkpLHE"
                "l6R6xLFcXFxcXEsbHBwbGxsbGxsbGw1p4rq60+AjFwAAANbQy1xcXFxcdcR1"
                "gMSXxLyrXGPEsYCexLGevJq8xJ68nrHEaFxcXFxLGxwbGxsYHBsbGBsNo9S9"
                "us/gIRoAAADp5+VcXFxcXGjEvJfEl8TEnlxcvLyXY3Voj8R1dWiPq3VodZTE"
                "dVxcQxscGxscGxsYGBgSJcPNvbrP3jEUAAAASmR9eVxcXFxcaHVcdWx1dVxc"
                "XGN1XFxcXGN1Y1xcXFxcXFxsdWNcXCgbGBgVFRISEhIVDXDoyL29z9w/EQAA"
                "AAAAAANPXFxcXFxcXFxcXFxcXFxcXFxcXFxcXFxcXFxcXFxcXFxcXEMNDxIi"
                "MDhATl9yg4zA1MW5us3cPBEAAAAAAAAATFxcXFxcXFxcXFxcXEcpU1xcXFxT"
                "L0dcXFxcXFxcXFxcXFxwg46jrcDY6PTx8e/iucjawrfP4DoRAAAAAAhbrul4"
                "XFxcXFxcXFxcXFwWAAMvXFw0AwAQXFxcXFxcXFxcXFyQ7O/s6+Lb19THwsG+"
                "wdbH0NjKyt48FAEAAAGu5/nz1VxcXFxcXFxcXFxcEAAAAAcLAAAAEFxcXFxc"
                "XFxcXFxmyMK+tbKvr7K1wb61osfp09Ph5/DYTQ4BAAABotrw8O2VXFxcXFxc"
                "XFxcXCQAAAAAAAAAAB5cXFxcXFxcXFxclKiprrq3rJ2Cd21bVSZi5+HpwpOl"
                "6lcOAQAAAaLc7vD15mtcXFxcXFxcXFxTKQAAAAAAACRTXFxcXFxcXFxcdZOF"
                "alVEMxcIAgEAAAAAAErC6qJVcfVXDgEAAAGi3O3c7u2zXFxcXFxcLwspXFxH"
                "EAAAC0FcXC8LKVxcXFxcUwcABAQABAAAABoAMxo2ZFtttfnBf/X1Ug4BAAAC"
                "stzuk9ju+XhcXFxcXBAAAAdBXFw0NFxcQQsAABBcXFxcXEYhRBoaCSBQYHau"
                "qbnKx+Tk7cWonZxzYCAXAgAAAsXa5LXT4ee/XFxcXFwQAAAAABZTXFxTJAAA"
                "AAAQXFxcXFqYk5ydwuDh4c/BubegjXZbUEItJy4qKiotFwgAAATh8N7Q1tft"
                "2pBcXFxcEAAAAAAAAy80AwAAAAAAEFxcXFym5+m3opGCbVdIOiAgFy5VZVI+"
                "d6KlmGRKSCcXCAABPyqI58XCvb66ZlxcXBAAAAAAAAAAAAAAAAAAABBcXFxd"
                "VzMjICERETNESC5tW3G5tcG5UoLFwqJKRCcnIxoBAAAAAHHNvre3t59cXFwe"
                "AAAAAAAAAAAAAAAAAAAWXFxTEwwAFE0tdzainIUzgn1tdn93TTY+NjM2Qi4A"
                "ADEIAgAAAAAOfa7FwcLPflxcUx4AAAAAAAAAAAAAAAAWU1xcJAEBABd9QlUn"
                "i6+oRGJ/e2dXUFJbYmdxd2VbAAF2AAEAAAAAGs/g6uHWypleXFxcQQsAAAAA"
                "AAAAAAdBXFxcRwAAAAABFFcxAFu6yG08f4mLgn1/gn99d3Z9ggUUf1cCAAAA"
                "AAFgamU+IwUAKVxcXFxcKQMAAAAAAClTXFxcXBAAAAAAAABqTQAKqal/J3+I"
                "iX97d3t7e3d2dn0xJndnBQAAAAAAAAAAAAAAAABPXFxcXFxPEAAAEEdcXFxc"
                "XDQAAAAAAAAASJEGAmKNcUpKi4V7dnZ3d3d2c3Nzd3ZzagUAAAAAAAAAAAAA"
                "AAAAEFxcXFxcXFxHQVxcXFxcXFMDAAAAAAAADoKJLT4zRDM6I3GFfX9/fXt2"
                "cW1qYlJEMyAAAAAAAAAAAAAAAAAAAAA9XFxcXFxcXFxcXFxcXFwkAAAAAAAA"
                "ABGFgn2LdlF2ZGRRbWVbRDMjFwkFAAAAAAAAAAAAAAAAAAAAAAAAAAAAB1Nc"
                "XFxcXFxcXFxcXFxHAAAAAAAAAAACISAaFA4JBgQCAQAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAApXFxcXFxcXFxcXFxcEAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAEFcXFxcXFxc"
                "XFxcKQAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAABwcHBwcHBwcHAwAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA"
                "AAAAAAAAAAAAAAAAAAAAAAAAAAAAAAAA";

[Device Classification]
        Class1 = EtherNetIP;
        Class2 = Safety;                $ Mandatory for CIP Safety


[Params]
        Param1 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC2,                   $ Data Type
                1,                      $ Data Size in bytes
                "SINT_INP",             $ name
                "",                     $ units
                "(8bit)",               $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param2 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "INT_INP",              $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param3 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC4,                   $ Data Type
                4,                      $ Data Size in bytes
                "DINT_INP",             $ name
                "",                     $ units
                "(32bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param4 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "2B0B/0 Freq Setpoint Hz",    $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param5 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "2D40/4 Device Load Act.",    $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param6 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "2D4F/0 Motor i2t utiliz.",    $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param7 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC4,                   $ Data Type
                4,                      $ Data Size in bytes
                "2D82/0 Motor voltage", $ name
                "",                     $ units
                "(32bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param8 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "2D88/0 Motor current", $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param9 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC4,                   $ Data Type
                4,                      $ Data Size in bytes
                "2DA2/1 Effective Power",    $ name
                "",                     $ units
                "(32bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param10 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC4,                   $ Data Type
                4,                      $ Data Size in bytes
                "2DA2/2 Apparent Power",$ name
                "",                     $ units
                "(32bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param11 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC4,                   $ Data Type
                4,                      $ Data Size in bytes
                "2DA3/1 Energy Out Motor",    $ name
                "",                     $ units
                "(32bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param12 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC4,                   $ Data Type
                4,                      $ Data Size in bytes
                "2DA3/2 Energy Out Gen.",    $ name
                "",                     $ units
                "(32bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param24 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC4,                   $ Data Type
                4,                      $ Data Size in bytes
                "2DD3/1 Speed set",     $ name
                "",                     $ units
                "(32bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param26 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "2DDD/0 Actual Frequency",    $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param27 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "400A/1 NetWordOUT1",   $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param29 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "400C/1 AC Drv Stat Word",    $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param31 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "400C/3 Actual Speed Hz",    $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param32 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "400C/4 Actual Speed RPM",    $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param33 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "400C/5 Drive State",   $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param34 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "400C/6 Act Speed 0.01Hz",    $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param35 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "400C/7 Actual Torque Scaled",    $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param37 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "401F/1 Actual PID Stpnt",    $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param38 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "401F/2 Actual PID Fbk",$ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param39 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC2,                   $ Data Type
                1,                      $ Data Size in bytes
                "401F/3 PID bits",      $ name
                "",                     $ units
                "(8bit)",               $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param40 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "603F/0 Current Fault", $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param41 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "6041/0 Status Word",   $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param42 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "6043/0 Veloc Demand",  $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param43 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "6044/0 Veloc Actual",  $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param44 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC2,                   $ Data Type
                1,                      $ Data Size in bytes
                "6061/0 402 Mode Display",    $ name
                "",                     $ units
                "(8bit)",               $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param45 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "6077/0 402 ActualTorq %",    $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param46 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "6078/0 402 ActualCur %",    $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param47 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC4,                   $ Data Type
                4,                      $ Data Size in bytes
                "6079/0 402 DClink Volt",    $ name
                "",                     $ units
                "(32bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param48 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC4,                   $ Data Type
                4,                      $ Data Size in bytes
                "60FD/0 Dig Inputs Stat",    $ name
                "",                     $ units
                "(32bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param50 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "400C/9 Proc Output Freq",    $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places




        Param51 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC2,                   $ Data Type
                1,                      $ Data Size in bytes
                "SINT_OUT",             $ name
                "",                     $ units
                "(8bit)",               $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param52 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "INT_OUT",              $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param53 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC4,                   $ Data Type
                4,                      $ Data Size in bytes
                "DINT_OUT",             $ name
                "",                     $ units
                "(32bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places

        Param54 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC4,                   $ Data Type
                4,                      $ Data Size in bytes
                "2946/1 Trq Mode Hi Spd",    $ name
                "",                     $ units
                "(32bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places

        Param55 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC4,                   $ Data Type
                4,                      $ Data Size in bytes
                "2946/2 Trq Mode Lo Spd",    $ name
                "",                     $ units
                "(32bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places


        Param56 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "4008/1 NetWordIN1",    $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places

        Param57 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "4008/2 NetWordIN2",    $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places

        Param60 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "400B/1 AC Drv Ctrl Word",    $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places

        Param62 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "400B/3 Net Spd Stpnt Hz",    $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param63 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "400B/4 Net Spd Stpnt RPM",    $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param64 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "400B/5 Net Spd 0.01 Hz",    $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param65 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "400B/6 NetSpdSign 0.1Hz",    $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param66 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "400B/7 Net PID Stpnt", $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param67 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "400B/8 Net Torque Stpnt",    $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param68 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "6040/0 Control Word",  $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param69 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "6042/0 Target Veloc",  $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param70 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC4,                   $ Data Type
                4,                      $ Data Size in bytes
                "6046/1 Veloc Min",     $ name
                "",                     $ units
                "(32bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param71 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC4,                   $ Data Type
                4,                      $ Data Size in bytes
                "6046/2 Veloc Max",     $ name
                "",                     $ units
                "(32bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param72 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC4,                   $ Data Type
                4,                      $ Data Size in bytes
                "6048/1 Delta Speed",   $ name
                "",                     $ units
                "(32bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param73 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "6048/2 Delta Time",    $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param74 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC4,                   $ Data Type
                4,                      $ Data Size in bytes
                "6049/1 Delta Speed",   $ name
                "",                     $ units
                "(32bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param75 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "6049/2 Delta Time",    $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param76 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC2,                   $ Data Type
                1,                      $ Data Size in bytes
                "6060/0 402 Control Modes",    $ name
                "",                     $ units
                "(8bit)",               $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param77 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "6071/0 402 TargetTorq",$ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param78 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC4,                   $ Data Type
                4,                      $ Data Size in bytes
                "6080/0 Mot Max Speed", $ name
                "",                     $ units
                "(32bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param79 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "60E0/0 Pos TorqLimit", $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param80 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "60E1/0 Neg TorqLimit", $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param82 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC3,                   $ Data Type
                2,                      $ Data Size in bytes
                "400B/13 Proc Input Freq",    $ name
                "",                     $ units
                "(16bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places


        Param100 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC4,                   $ Data Type
                4,                      $ Data Size in bytes
                "Trailer Input",        $ name
                "",                     $ units
                "(32bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places

        Param101 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC4,                   $ Data Type
                4,                      $ Data Size in bytes
                "Trailer Output",       $ name
                "",                     $ units
                "(32bit)",              $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places


        Param1000 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0002,                 $ Descriptor
                0xC6,                   $ Data Type
                1,                      $ Data Size in bytes
                "OUT Ctrl1:",           $ name
                "",                     $ units
                "New Help String",      $ help string
                0x14,0x15,0x15,         $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum1000 =
                0x14,"Basic",
                0x15,"Extended";
        Param1001 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0002,                 $ Descriptor
                0xC6,                   $ Data Type
                1,                      $ Data Size in bytes
                "INP Ctrl1:",           $ name
                "",                     $ units
                "New Help String",      $ help string
                0x46,0x47,0x47,         $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum1001 =
                0x46,"Basic",
                0x47,"Extended";
        Param1002 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0002,                 $ Descriptor
                0xC6,                   $ Data Type
                1,                      $ Data Size in bytes
                "OUT Ctrl2:",           $ name
                "",                     $ units
                "New Help String",      $ help string
                0x16,0x17,0x17,         $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum1002 =
                0x16,"Basic",
                0x17,"Extended";
        Param1003 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0002,                 $ Descriptor
                0xC6,                   $ Data Type
                1,                      $ Data Size in bytes
                "INP Ctrl2:",           $ name
                "",                     $ units
                "New Help String",      $ help string
                0x48,0x49,0x49,         $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum1003 =
                0x48,"Basic",
                0x49,"Extended";


        Param2000 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC8,                   $ Data Type
                4,                      $ Data Size in bytes
                "RPI Value",            $ name
                "",                     $ units
                "",                     $ help string
                4000,100000,10000,      $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places


        Param34000000 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Input#1",       $ name
                "",                     $ units
                "",                     $ help string
                0,65535,29,             $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000000 =
                0,"ignore",
                1,"SINT_INP",
                2,"INT_INP",
                3,"DINT_INP",
                4,"2B0B/0 Freq Setpoint Hz",
                5,"2D40/4 Device Load Act.",
                6,"2D4F/0 Motor i2t utiliz.",
                7,"2D82/0 Motor voltage",
                8,"2D88/0 Motor current",
                9,"2DA2/1 Effective Power",
                10,"2DA2/2 Apparent Power",
                11,"2DA3/1 Energy Out Motor",
                12,"2DA3/2 Energy Out Gen.",
                13,"2DA4/1 Anlg In1 %",
                14,"2DA4/2 Anlg In1 Freq",
                15,"2DA4/3 Anlg In1 PidVal",
                16,"2DA4/4 Anlg In1 TorqVal",
                17,"2DA5/1 Anlg In2 %",
                18,"2DA5/2 Anlg In2 Freq",
                19,"2DA5/3 Anlg In2 PidVal",
                20,"2DA5/4 Anlg In2 TorqVal",
                21,"2DAA/1 AO1 Value (VDC)",
                22,"2DAA/2 AO1 Value (IDC)",
                23,"reserved23",
                24,"2DD3/1 Speed set",
                25,"reserved25",
                26,"2DDD/0 Actual Frequency",
                27,"400A/1 NetWordOUT1",
                28,"400A/2 NetWordOUT2",
                29,"400C/1 AC Drv Stat Word",
                30,"400C/2 C0150 Stat Word",
                31,"400C/3 Actual Speed Hz",
                32,"400C/4 Actual Speed RPM",
                33,"400C/5 Drive State",
                34,"400C/6 Act Speed 0.01Hz",
                35,"400C/7 Actual Torque Scaled",
                36,"400D/0 Scaled Speed",
                37,"401F/1 Actual PID Stpnt",
                38,"401F/2 Actual PID Fbk",
                39,"401F/3 PID bits",
                40,"603F/0 Current Fault",
                41,"6041/0 Status Word",
                42,"6043/0 Veloc Demand",
                43,"6044/0 Veloc Actual",
                44,"6061/0 402 Mode Display",
                45,"6077/0 402 ActualTorq %",
                46,"6078/0 402 ActualCur %",
                47,"6079/0 402 DClink Volt",
                48,"60FD/0 Dig Inputs Stat",
                50,"400C/9 Proc Output Freq";
        Param34000001 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Input#2",       $ name
                "",                     $ units
                "",                     $ help string
                0,65535,32,             $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000001 =
                0,"ignore",
                1,"SINT_INP",
                2,"INT_INP",
                3,"DINT_INP",
                4,"2B0B/0 Freq Setpoint Hz",
                5,"2D40/4 Device Load Act.",
                6,"2D4F/0 Motor i2t utiliz.",
                7,"2D82/0 Motor voltage",
                8,"2D88/0 Motor current",
                9,"2DA2/1 Effective Power",
                10,"2DA2/2 Apparent Power",
                11,"2DA3/1 Energy Out Motor",
                12,"2DA3/2 Energy Out Gen.",
                13,"2DA4/1 Anlg In1 %",
                14,"2DA4/2 Anlg In1 Freq",
                15,"2DA4/3 Anlg In1 PidVal",
                16,"2DA4/4 Anlg In1 TorqVal",
                17,"2DA5/1 Anlg In2 %",
                18,"2DA5/2 Anlg In2 Freq",
                19,"2DA5/3 Anlg In2 PidVal",
                20,"2DA5/4 Anlg In2 TorqVal",
                21,"2DAA/1 AO1 Value (VDC)",
                22,"2DAA/2 AO1 Value (IDC)",
                23,"reserved23",
                24,"2DD3/1 Speed set",
                25,"reserved25",
                26,"2DDD/0 Actual Frequency",
                27,"400A/1 NetWordOUT1",
                28,"400A/2 NetWordOUT2",
                29,"400C/1 AC Drv Stat Word",
                30,"400C/2 C0150 Stat Word",
                31,"400C/3 Actual Speed Hz",
                32,"400C/4 Actual Speed RPM",
                33,"400C/5 Drive State",
                34,"400C/6 Act Speed 0.01Hz",
                35,"400C/7 Actual Torque Scaled",
                36,"400D/0 Scaled Speed",
                37,"401F/1 Actual PID Stpnt",
                38,"401F/2 Actual PID Fbk",
                39,"401F/3 PID bits",
                40,"603F/0 Current Fault",
                41,"6041/0 Status Word",
                42,"6043/0 Veloc Demand",
                43,"6044/0 Veloc Actual",
                44,"6061/0 402 Mode Display",
                45,"6077/0 402 ActualTorq %",
                46,"6078/0 402 ActualCur %",
                47,"6079/0 402 DClink Volt",
                48,"60FD/0 Dig Inputs Stat",
                50,"400C/9 Proc Output Freq";
        Param34000002 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Input#3",       $ name
                "",                     $ units
                "",                     $ help string
                0,65535,35,             $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000002 =
                0,"ignore",
                1,"SINT_INP",
                2,"INT_INP",
                3,"DINT_INP",
                4,"2B0B/0 Freq Setpoint Hz",
                5,"2D40/4 Device Load Act.",
                6,"2D4F/0 Motor i2t utiliz.",
                7,"2D82/0 Motor voltage",
                8,"2D88/0 Motor current",
                9,"2DA2/1 Effective Power",
                10,"2DA2/2 Apparent Power",
                11,"2DA3/1 Energy Out Motor",
                12,"2DA3/2 Energy Out Gen.",
                13,"2DA4/1 Anlg In1 %",
                14,"2DA4/2 Anlg In1 Freq",
                15,"2DA4/3 Anlg In1 PidVal",
                16,"2DA4/4 Anlg In1 TorqVal",
                17,"2DA5/1 Anlg In2 %",
                18,"2DA5/2 Anlg In2 Freq",
                19,"2DA5/3 Anlg In2 PidVal",
                20,"2DA5/4 Anlg In2 TorqVal",
                21,"2DAA/1 AO1 Value (VDC)",
                22,"2DAA/2 AO1 Value (IDC)",
                23,"reserved23",
                24,"2DD3/1 Speed set",
                25,"reserved25",
                26,"2DDD/0 Actual Frequency",
                27,"400A/1 NetWordOUT1",
                28,"400A/2 NetWordOUT2",
                29,"400C/1 AC Drv Stat Word",
                30,"400C/2 C0150 Stat Word",
                31,"400C/3 Actual Speed Hz",
                32,"400C/4 Actual Speed RPM",
                33,"400C/5 Drive State",
                34,"400C/6 Act Speed 0.01Hz",
                35,"400C/7 Actual Torque Scaled",
                36,"400D/0 Scaled Speed",
                37,"401F/1 Actual PID Stpnt",
                38,"401F/2 Actual PID Fbk",
                39,"401F/3 PID bits",
                40,"603F/0 Current Fault",
                41,"6041/0 Status Word",
                42,"6043/0 Veloc Demand",
                43,"6044/0 Veloc Actual",
                44,"6061/0 402 Mode Display",
                45,"6077/0 402 ActualTorq %",
                46,"6078/0 402 ActualCur %",
                47,"6079/0 402 DClink Volt",
                48,"60FD/0 Dig Inputs Stat",
                50,"400C/9 Proc Output Freq";
        Param34000003 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Input#4",       $ name
                "",                     $ units
                "",                     $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000003 =
                0,"ignore",
                1,"SINT_INP",
                2,"INT_INP",
                3,"DINT_INP",
                4,"2B0B/0 Freq Setpoint Hz",
                5,"2D40/4 Device Load Act.",
                6,"2D4F/0 Motor i2t utiliz.",
                7,"2D82/0 Motor voltage",
                8,"2D88/0 Motor current",
                9,"2DA2/1 Effective Power",
                10,"2DA2/2 Apparent Power",
                11,"2DA3/1 Energy Out Motor",
                12,"2DA3/2 Energy Out Gen.",
                13,"2DA4/1 Anlg In1 %",
                14,"2DA4/2 Anlg In1 Freq",
                15,"2DA4/3 Anlg In1 PidVal",
                16,"2DA4/4 Anlg In1 TorqVal",
                17,"2DA5/1 Anlg In2 %",
                18,"2DA5/2 Anlg In2 Freq",
                19,"2DA5/3 Anlg In2 PidVal",
                20,"2DA5/4 Anlg In2 TorqVal",
                21,"2DAA/1 AO1 Value (VDC)",
                22,"2DAA/2 AO1 Value (IDC)",
                23,"reserved23",
                24,"2DD3/1 Speed set",
                25,"reserved25",
                26,"2DDD/0 Actual Frequency",
                27,"400A/1 NetWordOUT1",
                28,"400A/2 NetWordOUT2",
                29,"400C/1 AC Drv Stat Word",
                30,"400C/2 C0150 Stat Word",
                31,"400C/3 Actual Speed Hz",
                32,"400C/4 Actual Speed RPM",
                33,"400C/5 Drive State",
                34,"400C/6 Act Speed 0.01Hz",
                35,"400C/7 Actual Torque Scaled",
                36,"400D/0 Scaled Speed",
                37,"401F/1 Actual PID Stpnt",
                38,"401F/2 Actual PID Fbk",
                39,"401F/3 PID bits",
                40,"603F/0 Current Fault",
                41,"6041/0 Status Word",
                42,"6043/0 Veloc Demand",
                43,"6044/0 Veloc Actual",
                44,"6061/0 402 Mode Display",
                45,"6077/0 402 ActualTorq %",
                46,"6078/0 402 ActualCur %",
                47,"6079/0 402 DClink Volt",
                48,"60FD/0 Dig Inputs Stat",
                50,"400C/9 Proc Output Freq";
        Param34000004 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Input#5",       $ name
                "",                     $ units
                "",                     $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000004 =
                0,"ignore",
                1,"SINT_INP",
                2,"INT_INP",
                3,"DINT_INP",
                4,"2B0B/0 Freq Setpoint Hz",
                5,"2D40/4 Device Load Act.",
                6,"2D4F/0 Motor i2t utiliz.",
                7,"2D82/0 Motor voltage",
                8,"2D88/0 Motor current",
                9,"2DA2/1 Effective Power",
                10,"2DA2/2 Apparent Power",
                11,"2DA3/1 Energy Out Motor",
                12,"2DA3/2 Energy Out Gen.",
                13,"2DA4/1 Anlg In1 %",
                14,"2DA4/2 Anlg In1 Freq",
                15,"2DA4/3 Anlg In1 PidVal",
                16,"2DA4/4 Anlg In1 TorqVal",
                17,"2DA5/1 Anlg In2 %",
                18,"2DA5/2 Anlg In2 Freq",
                19,"2DA5/3 Anlg In2 PidVal",
                20,"2DA5/4 Anlg In2 TorqVal",
                21,"2DAA/1 AO1 Value (VDC)",
                22,"2DAA/2 AO1 Value (IDC)",
                23,"reserved23",
                24,"2DD3/1 Speed set",
                25,"reserved25",
                26,"2DDD/0 Actual Frequency",
                27,"400A/1 NetWordOUT1",
                28,"400A/2 NetWordOUT2",
                29,"400C/1 AC Drv Stat Word",
                30,"400C/2 C0150 Stat Word",
                31,"400C/3 Actual Speed Hz",
                32,"400C/4 Actual Speed RPM",
                33,"400C/5 Drive State",
                34,"400C/6 Act Speed 0.01Hz",
                35,"400C/7 Actual Torque Scaled",
                36,"400D/0 Scaled Speed",
                37,"401F/1 Actual PID Stpnt",
                38,"401F/2 Actual PID Fbk",
                39,"401F/3 PID bits",
                40,"603F/0 Current Fault",
                41,"6041/0 Status Word",
                42,"6043/0 Veloc Demand",
                43,"6044/0 Veloc Actual",
                44,"6061/0 402 Mode Display",
                45,"6077/0 402 ActualTorq %",
                46,"6078/0 402 ActualCur %",
                47,"6079/0 402 DClink Volt",
                48,"60FD/0 Dig Inputs Stat",
                50,"400C/9 Proc Output Freq";
        Param34000005 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Input#6",       $ name
                "",                     $ units
                "",                     $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000005 =
                0,"ignore",
                1,"SINT_INP",
                2,"INT_INP",
                3,"DINT_INP",
                4,"2B0B/0 Freq Setpoint Hz",
                5,"2D40/4 Device Load Act.",
                6,"2D4F/0 Motor i2t utiliz.",
                7,"2D82/0 Motor voltage",
                8,"2D88/0 Motor current",
                9,"2DA2/1 Effective Power",
                10,"2DA2/2 Apparent Power",
                11,"2DA3/1 Energy Out Motor",
                12,"2DA3/2 Energy Out Gen.",
                13,"2DA4/1 Anlg In1 %",
                14,"2DA4/2 Anlg In1 Freq",
                15,"2DA4/3 Anlg In1 PidVal",
                16,"2DA4/4 Anlg In1 TorqVal",
                17,"2DA5/1 Anlg In2 %",
                18,"2DA5/2 Anlg In2 Freq",
                19,"2DA5/3 Anlg In2 PidVal",
                20,"2DA5/4 Anlg In2 TorqVal",
                21,"2DAA/1 AO1 Value (VDC)",
                22,"2DAA/2 AO1 Value (IDC)",
                23,"reserved23",
                24,"2DD3/1 Speed set",
                25,"reserved25",
                26,"2DDD/0 Actual Frequency",
                27,"400A/1 NetWordOUT1",
                28,"400A/2 NetWordOUT2",
                29,"400C/1 AC Drv Stat Word",
                30,"400C/2 C0150 Stat Word",
                31,"400C/3 Actual Speed Hz",
                32,"400C/4 Actual Speed RPM",
                33,"400C/5 Drive State",
                34,"400C/6 Act Speed 0.01Hz",
                35,"400C/7 Actual Torque Scaled",
                36,"400D/0 Scaled Speed",
                37,"401F/1 Actual PID Stpnt",
                38,"401F/2 Actual PID Fbk",
                39,"401F/3 PID bits",
                40,"603F/0 Current Fault",
                41,"6041/0 Status Word",
                42,"6043/0 Veloc Demand",
                43,"6044/0 Veloc Actual",
                44,"6061/0 402 Mode Display",
                45,"6077/0 402 ActualTorq %",
                46,"6078/0 402 ActualCur %",
                47,"6079/0 402 DClink Volt",
                48,"60FD/0 Dig Inputs Stat",
                50,"400C/9 Proc Output Freq";
        Param34000006 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Input#7",       $ name
                "",                     $ units
                "",                     $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000006 =
                0,"ignore",
                1,"SINT_INP",
                2,"INT_INP",
                3,"DINT_INP",
                4,"2B0B/0 Freq Setpoint Hz",
                5,"2D40/4 Device Load Act.",
                6,"2D4F/0 Motor i2t utiliz.",
                7,"2D82/0 Motor voltage",
                8,"2D88/0 Motor current",
                9,"2DA2/1 Effective Power",
                10,"2DA2/2 Apparent Power",
                11,"2DA3/1 Energy Out Motor",
                12,"2DA3/2 Energy Out Gen.",
                13,"2DA4/1 Anlg In1 %",
                14,"2DA4/2 Anlg In1 Freq",
                15,"2DA4/3 Anlg In1 PidVal",
                16,"2DA4/4 Anlg In1 TorqVal",
                17,"2DA5/1 Anlg In2 %",
                18,"2DA5/2 Anlg In2 Freq",
                19,"2DA5/3 Anlg In2 PidVal",
                20,"2DA5/4 Anlg In2 TorqVal",
                21,"2DAA/1 AO1 Value (VDC)",
                22,"2DAA/2 AO1 Value (IDC)",
                23,"reserved23",
                24,"2DD3/1 Speed set",
                25,"reserved25",
                26,"2DDD/0 Actual Frequency",
                27,"400A/1 NetWordOUT1",
                28,"400A/2 NetWordOUT2",
                29,"400C/1 AC Drv Stat Word",
                30,"400C/2 C0150 Stat Word",
                31,"400C/3 Actual Speed Hz",
                32,"400C/4 Actual Speed RPM",
                33,"400C/5 Drive State",
                34,"400C/6 Act Speed 0.01Hz",
                35,"400C/7 Actual Torque Scaled",
                36,"400D/0 Scaled Speed",
                37,"401F/1 Actual PID Stpnt",
                38,"401F/2 Actual PID Fbk",
                39,"401F/3 PID bits",
                40,"603F/0 Current Fault",
                41,"6041/0 Status Word",
                42,"6043/0 Veloc Demand",
                43,"6044/0 Veloc Actual",
                44,"6061/0 402 Mode Display",
                45,"6077/0 402 ActualTorq %",
                46,"6078/0 402 ActualCur %",
                47,"6079/0 402 DClink Volt",
                48,"60FD/0 Dig Inputs Stat",
                50,"400C/9 Proc Output Freq";
        Param34000007 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Input#8",       $ name
                "",                     $ units
                "",                     $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000007 =
                0,"ignore",
                1,"SINT_INP",
                2,"INT_INP",
                3,"DINT_INP",
                4,"2B0B/0 Freq Setpoint Hz",
                5,"2D40/4 Device Load Act.",
                6,"2D4F/0 Motor i2t utiliz.",
                7,"2D82/0 Motor voltage",
                8,"2D88/0 Motor current",
                9,"2DA2/1 Effective Power",
                10,"2DA2/2 Apparent Power",
                11,"2DA3/1 Energy Out Motor",
                12,"2DA3/2 Energy Out Gen.",
                13,"2DA4/1 Anlg In1 %",
                14,"2DA4/2 Anlg In1 Freq",
                15,"2DA4/3 Anlg In1 PidVal",
                16,"2DA4/4 Anlg In1 TorqVal",
                17,"2DA5/1 Anlg In2 %",
                18,"2DA5/2 Anlg In2 Freq",
                19,"2DA5/3 Anlg In2 PidVal",
                20,"2DA5/4 Anlg In2 TorqVal",
                21,"2DAA/1 AO1 Value (VDC)",
                22,"2DAA/2 AO1 Value (IDC)",
                23,"reserved23",
                24,"2DD3/1 Speed set",
                25,"reserved25",
                26,"2DDD/0 Actual Frequency",
                27,"400A/1 NetWordOUT1",
                28,"400A/2 NetWordOUT2",
                29,"400C/1 AC Drv Stat Word",
                30,"400C/2 C0150 Stat Word",
                31,"400C/3 Actual Speed Hz",
                32,"400C/4 Actual Speed RPM",
                33,"400C/5 Drive State",
                34,"400C/6 Act Speed 0.01Hz",
                35,"400C/7 Actual Torque Scaled",
                36,"400D/0 Scaled Speed",
                37,"401F/1 Actual PID Stpnt",
                38,"401F/2 Actual PID Fbk",
                39,"401F/3 PID bits",
                40,"603F/0 Current Fault",
                41,"6041/0 Status Word",
                42,"6043/0 Veloc Demand",
                43,"6044/0 Veloc Actual",
                44,"6061/0 402 Mode Display",
                45,"6077/0 402 ActualTorq %",
                46,"6078/0 402 ActualCur %",
                47,"6079/0 402 DClink Volt",
                48,"60FD/0 Dig Inputs Stat",
                50,"400C/9 Proc Output Freq";
        Param34000008 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Input#9",       $ name
                "",                     $ units
                "",                     $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000008 =
                0,"ignore",
                1,"SINT_INP",
                2,"INT_INP",
                3,"DINT_INP",
                4,"2B0B/0 Freq Setpoint Hz",
                5,"2D40/4 Device Load Act.",
                6,"2D4F/0 Motor i2t utiliz.",
                7,"2D82/0 Motor voltage",
                8,"2D88/0 Motor current",
                9,"2DA2/1 Effective Power",
                10,"2DA2/2 Apparent Power",
                11,"2DA3/1 Energy Out Motor",
                12,"2DA3/2 Energy Out Gen.",
                13,"2DA4/1 Anlg In1 %",
                14,"2DA4/2 Anlg In1 Freq",
                15,"2DA4/3 Anlg In1 PidVal",
                16,"2DA4/4 Anlg In1 TorqVal",
                17,"2DA5/1 Anlg In2 %",
                18,"2DA5/2 Anlg In2 Freq",
                19,"2DA5/3 Anlg In2 PidVal",
                20,"2DA5/4 Anlg In2 TorqVal",
                21,"2DAA/1 AO1 Value (VDC)",
                22,"2DAA/2 AO1 Value (IDC)",
                23,"reserved23",
                24,"2DD3/1 Speed set",
                25,"reserved25",
                26,"2DDD/0 Actual Frequency",
                27,"400A/1 NetWordOUT1",
                28,"400A/2 NetWordOUT2",
                29,"400C/1 AC Drv Stat Word",
                30,"400C/2 C0150 Stat Word",
                31,"400C/3 Actual Speed Hz",
                32,"400C/4 Actual Speed RPM",
                33,"400C/5 Drive State",
                34,"400C/6 Act Speed 0.01Hz",
                35,"400C/7 Actual Torque Scaled",
                36,"400D/0 Scaled Speed",
                37,"401F/1 Actual PID Stpnt",
                38,"401F/2 Actual PID Fbk",
                39,"401F/3 PID bits",
                40,"603F/0 Current Fault",
                41,"6041/0 Status Word",
                42,"6043/0 Veloc Demand",
                43,"6044/0 Veloc Actual",
                44,"6061/0 402 Mode Display",
                45,"6077/0 402 ActualTorq %",
                46,"6078/0 402 ActualCur %",
                47,"6079/0 402 DClink Volt",
                48,"60FD/0 Dig Inputs Stat",
                50,"400C/9 Proc Output Freq";
        Param34000009 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Input#10",      $ name
                "",                     $ units
                "",                     $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000009 =
                0,"ignore",
                1,"SINT_INP",
                2,"INT_INP",
                3,"DINT_INP",
                4,"2B0B/0 Freq Setpoint Hz",
                5,"2D40/4 Device Load Act.",
                6,"2D4F/0 Motor i2t utiliz.",
                7,"2D82/0 Motor voltage",
                8,"2D88/0 Motor current",
                9,"2DA2/1 Effective Power",
                10,"2DA2/2 Apparent Power",
                11,"2DA3/1 Energy Out Motor",
                12,"2DA3/2 Energy Out Gen.",
                13,"2DA4/1 Anlg In1 %",
                14,"2DA4/2 Anlg In1 Freq",
                15,"2DA4/3 Anlg In1 PidVal",
                16,"2DA4/4 Anlg In1 TorqVal",
                17,"2DA5/1 Anlg In2 %",
                18,"2DA5/2 Anlg In2 Freq",
                19,"2DA5/3 Anlg In2 PidVal",
                20,"2DA5/4 Anlg In2 TorqVal",
                21,"2DAA/1 AO1 Value (VDC)",
                22,"2DAA/2 AO1 Value (IDC)",
                23,"reserved23",
                24,"2DD3/1 Speed set",
                25,"reserved25",
                26,"2DDD/0 Actual Frequency",
                27,"400A/1 NetWordOUT1",
                28,"400A/2 NetWordOUT2",
                29,"400C/1 AC Drv Stat Word",
                30,"400C/2 C0150 Stat Word",
                31,"400C/3 Actual Speed Hz",
                32,"400C/4 Actual Speed RPM",
                33,"400C/5 Drive State",
                34,"400C/6 Act Speed 0.01Hz",
                35,"400C/7 Actual Torque Scaled",
                36,"400D/0 Scaled Speed",
                37,"401F/1 Actual PID Stpnt",
                38,"401F/2 Actual PID Fbk",
                39,"401F/3 PID bits",
                40,"603F/0 Current Fault",
                41,"6041/0 Status Word",
                42,"6043/0 Veloc Demand",
                43,"6044/0 Veloc Actual",
                44,"6061/0 402 Mode Display",
                45,"6077/0 402 ActualTorq %",
                46,"6078/0 402 ActualCur %",
                47,"6079/0 402 DClink Volt",
                48,"60FD/0 Dig Inputs Stat",
                50,"400C/9 Proc Output Freq";
        Param34000010 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Input#11",      $ name
                "",                     $ units
                "",                     $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000010 =
                0,"ignore",
                1,"SINT_INP",
                2,"INT_INP",
                3,"DINT_INP",
                4,"2B0B/0 Freq Setpoint Hz",
                5,"2D40/4 Device Load Act.",
                6,"2D4F/0 Motor i2t utiliz.",
                7,"2D82/0 Motor voltage",
                8,"2D88/0 Motor current",
                9,"2DA2/1 Effective Power",
                10,"2DA2/2 Apparent Power",
                11,"2DA3/1 Energy Out Motor",
                12,"2DA3/2 Energy Out Gen.",
                13,"2DA4/1 Anlg In1 %",
                14,"2DA4/2 Anlg In1 Freq",
                15,"2DA4/3 Anlg In1 PidVal",
                16,"2DA4/4 Anlg In1 TorqVal",
                17,"2DA5/1 Anlg In2 %",
                18,"2DA5/2 Anlg In2 Freq",
                19,"2DA5/3 Anlg In2 PidVal",
                20,"2DA5/4 Anlg In2 TorqVal",
                21,"2DAA/1 AO1 Value (VDC)",
                22,"2DAA/2 AO1 Value (IDC)",
                23,"reserved23",
                24,"2DD3/1 Speed set",
                25,"reserved25",
                26,"2DDD/0 Actual Frequency",
                27,"400A/1 NetWordOUT1",
                28,"400A/2 NetWordOUT2",
                29,"400C/1 AC Drv Stat Word",
                30,"400C/2 C0150 Stat Word",
                31,"400C/3 Actual Speed Hz",
                32,"400C/4 Actual Speed RPM",
                33,"400C/5 Drive State",
                34,"400C/6 Act Speed 0.01Hz",
                35,"400C/7 Actual Torque Scaled",
                36,"400D/0 Scaled Speed",
                37,"401F/1 Actual PID Stpnt",
                38,"401F/2 Actual PID Fbk",
                39,"401F/3 PID bits",
                40,"603F/0 Current Fault",
                41,"6041/0 Status Word",
                42,"6043/0 Veloc Demand",
                43,"6044/0 Veloc Actual",
                44,"6061/0 402 Mode Display",
                45,"6077/0 402 ActualTorq %",
                46,"6078/0 402 ActualCur %",
                47,"6079/0 402 DClink Volt",
                48,"60FD/0 Dig Inputs Stat",
                50,"400C/9 Proc Output Freq";
        Param34000011 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Input#12",      $ name
                "",                     $ units
                "",                     $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000011 =
                0,"ignore",
                1,"SINT_INP",
                2,"INT_INP",
                3,"DINT_INP",
                4,"2B0B/0 Freq Setpoint Hz",
                5,"2D40/4 Device Load Act.",
                6,"2D4F/0 Motor i2t utiliz.",
                7,"2D82/0 Motor voltage",
                8,"2D88/0 Motor current",
                9,"2DA2/1 Effective Power",
                10,"2DA2/2 Apparent Power",
                11,"2DA3/1 Energy Out Motor",
                12,"2DA3/2 Energy Out Gen.",
                13,"2DA4/1 Anlg In1 %",
                14,"2DA4/2 Anlg In1 Freq",
                15,"2DA4/3 Anlg In1 PidVal",
                16,"2DA4/4 Anlg In1 TorqVal",
                17,"2DA5/1 Anlg In2 %",
                18,"2DA5/2 Anlg In2 Freq",
                19,"2DA5/3 Anlg In2 PidVal",
                20,"2DA5/4 Anlg In2 TorqVal",
                21,"2DAA/1 AO1 Value (VDC)",
                22,"2DAA/2 AO1 Value (IDC)",
                23,"reserved23",
                24,"2DD3/1 Speed set",
                25,"reserved25",
                26,"2DDD/0 Actual Frequency",
                27,"400A/1 NetWordOUT1",
                28,"400A/2 NetWordOUT2",
                29,"400C/1 AC Drv Stat Word",
                30,"400C/2 C0150 Stat Word",
                31,"400C/3 Actual Speed Hz",
                32,"400C/4 Actual Speed RPM",
                33,"400C/5 Drive State",
                34,"400C/6 Act Speed 0.01Hz",
                35,"400C/7 Actual Torque Scaled",
                36,"400D/0 Scaled Speed",
                37,"401F/1 Actual PID Stpnt",
                38,"401F/2 Actual PID Fbk",
                39,"401F/3 PID bits",
                40,"603F/0 Current Fault",
                41,"6041/0 Status Word",
                42,"6043/0 Veloc Demand",
                43,"6044/0 Veloc Actual",
                44,"6061/0 402 Mode Display",
                45,"6077/0 402 ActualTorq %",
                46,"6078/0 402 ActualCur %",
                47,"6079/0 402 DClink Volt",
                48,"60FD/0 Dig Inputs Stat",
                50,"400C/9 Proc Output Freq";
        Param34000012 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Input#13",      $ name
                "",                     $ units
                "",                     $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000012 =
                0,"ignore",
                1,"SINT_INP",
                2,"INT_INP",
                3,"DINT_INP",
                4,"2B0B/0 Freq Setpoint Hz",
                5,"2D40/4 Device Load Act.",
                6,"2D4F/0 Motor i2t utiliz.",
                7,"2D82/0 Motor voltage",
                8,"2D88/0 Motor current",
                9,"2DA2/1 Effective Power",
                10,"2DA2/2 Apparent Power",
                11,"2DA3/1 Energy Out Motor",
                12,"2DA3/2 Energy Out Gen.",
                13,"2DA4/1 Anlg In1 %",
                14,"2DA4/2 Anlg In1 Freq",
                15,"2DA4/3 Anlg In1 PidVal",
                16,"2DA4/4 Anlg In1 TorqVal",
                17,"2DA5/1 Anlg In2 %",
                18,"2DA5/2 Anlg In2 Freq",
                19,"2DA5/3 Anlg In2 PidVal",
                20,"2DA5/4 Anlg In2 TorqVal",
                21,"2DAA/1 AO1 Value (VDC)",
                22,"2DAA/2 AO1 Value (IDC)",
                23,"reserved23",
                24,"2DD3/1 Speed set",
                25,"reserved25",
                26,"2DDD/0 Actual Frequency",
                27,"400A/1 NetWordOUT1",
                28,"400A/2 NetWordOUT2",
                29,"400C/1 AC Drv Stat Word",
                30,"400C/2 C0150 Stat Word",
                31,"400C/3 Actual Speed Hz",
                32,"400C/4 Actual Speed RPM",
                33,"400C/5 Drive State",
                34,"400C/6 Act Speed 0.01Hz",
                35,"400C/7 Actual Torque Scaled",
                36,"400D/0 Scaled Speed",
                37,"401F/1 Actual PID Stpnt",
                38,"401F/2 Actual PID Fbk",
                39,"401F/3 PID bits",
                40,"603F/0 Current Fault",
                41,"6041/0 Status Word",
                42,"6043/0 Veloc Demand",
                43,"6044/0 Veloc Actual",
                44,"6061/0 402 Mode Display",
                45,"6077/0 402 ActualTorq %",
                46,"6078/0 402 ActualCur %",
                47,"6079/0 402 DClink Volt",
                48,"60FD/0 Dig Inputs Stat",
                50,"400C/9 Proc Output Freq";
        Param34000013 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Input#14",      $ name
                "",                     $ units
                "",                     $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000013 =
                0,"ignore",
                1,"SINT_INP",
                2,"INT_INP",
                3,"DINT_INP",
                4,"2B0B/0 Freq Setpoint Hz",
                5,"2D40/4 Device Load Act.",
                6,"2D4F/0 Motor i2t utiliz.",
                7,"2D82/0 Motor voltage",
                8,"2D88/0 Motor current",
                9,"2DA2/1 Effective Power",
                10,"2DA2/2 Apparent Power",
                11,"2DA3/1 Energy Out Motor",
                12,"2DA3/2 Energy Out Gen.",
                13,"2DA4/1 Anlg In1 %",
                14,"2DA4/2 Anlg In1 Freq",
                15,"2DA4/3 Anlg In1 PidVal",
                16,"2DA4/4 Anlg In1 TorqVal",
                17,"2DA5/1 Anlg In2 %",
                18,"2DA5/2 Anlg In2 Freq",
                19,"2DA5/3 Anlg In2 PidVal",
                20,"2DA5/4 Anlg In2 TorqVal",
                21,"2DAA/1 AO1 Value (VDC)",
                22,"2DAA/2 AO1 Value (IDC)",
                23,"reserved23",
                24,"2DD3/1 Speed set",
                25,"reserved25",
                26,"2DDD/0 Actual Frequency",
                27,"400A/1 NetWordOUT1",
                28,"400A/2 NetWordOUT2",
                29,"400C/1 AC Drv Stat Word",
                30,"400C/2 C0150 Stat Word",
                31,"400C/3 Actual Speed Hz",
                32,"400C/4 Actual Speed RPM",
                33,"400C/5 Drive State",
                34,"400C/6 Act Speed 0.01Hz",
                35,"400C/7 Actual Torque Scaled",
                36,"400D/0 Scaled Speed",
                37,"401F/1 Actual PID Stpnt",
                38,"401F/2 Actual PID Fbk",
                39,"401F/3 PID bits",
                40,"603F/0 Current Fault",
                41,"6041/0 Status Word",
                42,"6043/0 Veloc Demand",
                43,"6044/0 Veloc Actual",
                44,"6061/0 402 Mode Display",
                45,"6077/0 402 ActualTorq %",
                46,"6078/0 402 ActualCur %",
                47,"6079/0 402 DClink Volt",
                48,"60FD/0 Dig Inputs Stat",
                50,"400C/9 Proc Output Freq";
        Param34000014 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Input#15",      $ name
                "",                     $ units
                "",                     $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000014 =
                0,"ignore",
                1,"SINT_INP",
                2,"INT_INP",
                3,"DINT_INP",
                4,"2B0B/0 Freq Setpoint Hz",
                5,"2D40/4 Device Load Act.",
                6,"2D4F/0 Motor i2t utiliz.",
                7,"2D82/0 Motor voltage",
                8,"2D88/0 Motor current",
                9,"2DA2/1 Effective Power",
                10,"2DA2/2 Apparent Power",
                11,"2DA3/1 Energy Out Motor",
                12,"2DA3/2 Energy Out Gen.",
                13,"2DA4/1 Anlg In1 %",
                14,"2DA4/2 Anlg In1 Freq",
                15,"2DA4/3 Anlg In1 PidVal",
                16,"2DA4/4 Anlg In1 TorqVal",
                17,"2DA5/1 Anlg In2 %",
                18,"2DA5/2 Anlg In2 Freq",
                19,"2DA5/3 Anlg In2 PidVal",
                20,"2DA5/4 Anlg In2 TorqVal",
                21,"2DAA/1 AO1 Value (VDC)",
                22,"2DAA/2 AO1 Value (IDC)",
                23,"reserved23",
                24,"2DD3/1 Speed set",
                25,"reserved25",
                26,"2DDD/0 Actual Frequency",
                27,"400A/1 NetWordOUT1",
                28,"400A/2 NetWordOUT2",
                29,"400C/1 AC Drv Stat Word",
                30,"400C/2 C0150 Stat Word",
                31,"400C/3 Actual Speed Hz",
                32,"400C/4 Actual Speed RPM",
                33,"400C/5 Drive State",
                34,"400C/6 Act Speed 0.01Hz",
                35,"400C/7 Actual Torque Scaled",
                36,"400D/0 Scaled Speed",
                37,"401F/1 Actual PID Stpnt",
                38,"401F/2 Actual PID Fbk",
                39,"401F/3 PID bits",
                40,"603F/0 Current Fault",
                41,"6041/0 Status Word",
                42,"6043/0 Veloc Demand",
                43,"6044/0 Veloc Actual",
                44,"6061/0 402 Mode Display",
                45,"6077/0 402 ActualTorq %",
                46,"6078/0 402 ActualCur %",
                47,"6079/0 402 DClink Volt",
                48,"60FD/0 Dig Inputs Stat",
                50,"400C/9 Proc Output Freq";
        Param34000015 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Input#16",      $ name
                "",                     $ units
                "",                     $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000015 =
                0,"ignore",
                1,"SINT_INP",
                2,"INT_INP",
                3,"DINT_INP",
                4,"2B0B/0 Freq Setpoint Hz",
                5,"2D40/4 Device Load Act.",
                6,"2D4F/0 Motor i2t utiliz.",
                7,"2D82/0 Motor voltage",
                8,"2D88/0 Motor current",
                9,"2DA2/1 Effective Power",
                10,"2DA2/2 Apparent Power",
                11,"2DA3/1 Energy Out Motor",
                12,"2DA3/2 Energy Out Gen.",
                13,"2DA4/1 Anlg In1 %",
                14,"2DA4/2 Anlg In1 Freq",
                15,"2DA4/3 Anlg In1 PidVal",
                16,"2DA4/4 Anlg In1 TorqVal",
                17,"2DA5/1 Anlg In2 %",
                18,"2DA5/2 Anlg In2 Freq",
                19,"2DA5/3 Anlg In2 PidVal",
                20,"2DA5/4 Anlg In2 TorqVal",
                21,"2DAA/1 AO1 Value (VDC)",
                22,"2DAA/2 AO1 Value (IDC)",
                23,"reserved23",
                24,"2DD3/1 Speed set",
                25,"reserved25",
                26,"2DDD/0 Actual Frequency",
                27,"400A/1 NetWordOUT1",
                28,"400A/2 NetWordOUT2",
                29,"400C/1 AC Drv Stat Word",
                30,"400C/2 C0150 Stat Word",
                31,"400C/3 Actual Speed Hz",
                32,"400C/4 Actual Speed RPM",
                33,"400C/5 Drive State",
                34,"400C/6 Act Speed 0.01Hz",
                35,"400C/7 Actual Torque Scaled",
                36,"400D/0 Scaled Speed",
                37,"401F/1 Actual PID Stpnt",
                38,"401F/2 Actual PID Fbk",
                39,"401F/3 PID bits",
                40,"603F/0 Current Fault",
                41,"6041/0 Status Word",
                42,"6043/0 Veloc Demand",
                43,"6044/0 Veloc Actual",
                44,"6061/0 402 Mode Display",
                45,"6077/0 402 ActualTorq %",
                46,"6078/0 402 ActualCur %",
                47,"6079/0 402 DClink Volt",
                48,"60FD/0 Dig Inputs Stat",
                50,"400C/9 Proc Output Freq";

        Param34000050 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Output#1",      $ name
                "",                     $ units
                "",                     $ help string
                0,65535,60,             $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000050 =
                0,"ignore",
                51,"SINT_OUT",
                52,"INT_OUT",
                53,"DINT_OUT",
                54,"2946/1 Trq Mode Hi Spd",
                55,"2946/2 Trq Mode Lo Spd",
                56,"4008/1 NetWordIN1",
                57,"4008/2 NetWordIN2",
                58,"4008/3 NetWordIN3",
                59,"4008/4 NetWordIN4",
                60,"400B/1 AC Drv Ctrl Word",
                61,"400B/2 C0135 Ctrl Word",
                62,"400B/3 Net Spd Stpnt Hz",
                63,"400B/4 Net Spd Stpnt RPM",
                64,"400B/5 Net Spd 0.01 Hz",
                65,"400B/6 NetSpdSign 0.1Hz",
                66,"400B/7 Net PID Stpnt",
                67,"400B/8 Net Torque Stpnt",
                68,"6040/0 Control Word",
                69,"6042/0 Target Veloc",
                70,"6046/1 Veloc Min",
                71,"6046/2 Veloc Max",
                72,"6048/1 Delta Speed",
                73,"6048/2 Delta Time",
                74,"6049/1 Delta Speed",
                75,"6049/2 Delta Time",
                76,"6060/0 402 Control Modes",
                77,"6071/0 402 TargetTorq",
                78,"6080/0 Mot Max Speed",
                79,"60E0/0 Pos TorqLimit",
                80,"60E1/0 Neg TorqLimit",
                82,"400B/13 Proc Input Freq";
        Param34000051 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Output#2",      $ name
                "",                     $ units
                "",                     $ help string
                0,65535,63,             $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000051 =
                0,"ignore",
                51,"SINT_OUT",
                52,"INT_OUT",
                53,"DINT_OUT",
                54,"2946/1 Trq Mode Hi Spd",
                55,"2946/2 Trq Mode Lo Spd",
                56,"4008/1 NetWordIN1",
                57,"4008/2 NetWordIN2",
                58,"4008/3 NetWordIN3",
                59,"4008/4 NetWordIN4",
                60,"400B/1 AC Drv Ctrl Word",
                61,"400B/2 C0135 Ctrl Word",
                62,"400B/3 Net Spd Stpnt Hz",
                63,"400B/4 Net Spd Stpnt RPM",
                64,"400B/5 Net Spd 0.01 Hz",
                65,"400B/6 NetSpdSign 0.1Hz",
                66,"400B/7 Net PID Stpnt",
                67,"400B/8 Net Torque Stpnt",
                68,"6040/0 Control Word",
                69,"6042/0 Target Veloc",
                70,"6046/1 Veloc Min",
                71,"6046/2 Veloc Max",
                72,"6048/1 Delta Speed",
                73,"6048/2 Delta Time",
                74,"6049/1 Delta Speed",
                75,"6049/2 Delta Time",
                76,"6060/0 402 Control Modes",
                77,"6071/0 402 TargetTorq",
                78,"6080/0 Mot Max Speed",
                79,"60E0/0 Pos TorqLimit",
                80,"60E1/0 Neg TorqLimit",
                82,"400B/13 Proc Input Freq";
        Param34000052 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Output#3",      $ name
                "",                     $ units
                "",                     $ help string
                0,65535,67,             $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000052 =
                0,"ignore",
                51,"SINT_OUT",
                52,"INT_OUT",
                53,"DINT_OUT",
                54,"2946/1 Trq Mode Hi Spd",
                55,"2946/2 Trq Mode Lo Spd",
                56,"4008/1 NetWordIN1",
                57,"4008/2 NetWordIN2",
                58,"4008/3 NetWordIN3",
                59,"4008/4 NetWordIN4",
                60,"400B/1 AC Drv Ctrl Word",
                61,"400B/2 C0135 Ctrl Word",
                62,"400B/3 Net Spd Stpnt Hz",
                63,"400B/4 Net Spd Stpnt RPM",
                64,"400B/5 Net Spd 0.01 Hz",
                65,"400B/6 NetSpdSign 0.1Hz",
                66,"400B/7 Net PID Stpnt",
                67,"400B/8 Net Torque Stpnt",
                68,"6040/0 Control Word",
                69,"6042/0 Target Veloc",
                70,"6046/1 Veloc Min",
                71,"6046/2 Veloc Max",
                72,"6048/1 Delta Speed",
                73,"6048/2 Delta Time",
                74,"6049/1 Delta Speed",
                75,"6049/2 Delta Time",
                76,"6060/0 402 Control Modes",
                77,"6071/0 402 TargetTorq",
                78,"6080/0 Mot Max Speed",
                79,"60E0/0 Pos TorqLimit",
                80,"60E1/0 Neg TorqLimit",
                82,"400B/13 Proc Input Freq";
        Param34000053 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Output#4",      $ name
                "",                     $ units
                "",                     $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000053 =
                0,"ignore",
                51,"SINT_OUT",
                52,"INT_OUT",
                53,"DINT_OUT",
                54,"2946/1 Trq Mode Hi Spd",
                55,"2946/2 Trq Mode Lo Spd",
                56,"4008/1 NetWordIN1",
                57,"4008/2 NetWordIN2",
                58,"4008/3 NetWordIN3",
                59,"4008/4 NetWordIN4",
                60,"400B/1 AC Drv Ctrl Word",
                61,"400B/2 C0135 Ctrl Word",
                62,"400B/3 Net Spd Stpnt Hz",
                63,"400B/4 Net Spd Stpnt RPM",
                64,"400B/5 Net Spd 0.01 Hz",
                65,"400B/6 NetSpdSign 0.1Hz",
                66,"400B/7 Net PID Stpnt",
                67,"400B/8 Net Torque Stpnt",
                68,"6040/0 Control Word",
                69,"6042/0 Target Veloc",
                70,"6046/1 Veloc Min",
                71,"6046/2 Veloc Max",
                72,"6048/1 Delta Speed",
                73,"6048/2 Delta Time",
                74,"6049/1 Delta Speed",
                75,"6049/2 Delta Time",
                76,"6060/0 402 Control Modes",
                77,"6071/0 402 TargetTorq",
                78,"6080/0 Mot Max Speed",
                79,"60E0/0 Pos TorqLimit",
                80,"60E1/0 Neg TorqLimit",
                82,"400B/13 Proc Input Freq";
        Param34000054 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Output#5",      $ name
                "",                     $ units
                "",                     $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000054 =
                0,"ignore",
                51,"SINT_OUT",
                52,"INT_OUT",
                53,"DINT_OUT",
                54,"2946/1 Trq Mode Hi Spd",
                55,"2946/2 Trq Mode Lo Spd",
                56,"4008/1 NetWordIN1",
                57,"4008/2 NetWordIN2",
                58,"4008/3 NetWordIN3",
                59,"4008/4 NetWordIN4",
                60,"400B/1 AC Drv Ctrl Word",
                61,"400B/2 C0135 Ctrl Word",
                62,"400B/3 Net Spd Stpnt Hz",
                63,"400B/4 Net Spd Stpnt RPM",
                64,"400B/5 Net Spd 0.01 Hz",
                65,"400B/6 NetSpdSign 0.1Hz",
                66,"400B/7 Net PID Stpnt",
                67,"400B/8 Net Torque Stpnt",
                68,"6040/0 Control Word",
                69,"6042/0 Target Veloc",
                70,"6046/1 Veloc Min",
                71,"6046/2 Veloc Max",
                72,"6048/1 Delta Speed",
                73,"6048/2 Delta Time",
                74,"6049/1 Delta Speed",
                75,"6049/2 Delta Time",
                76,"6060/0 402 Control Modes",
                77,"6071/0 402 TargetTorq",
                78,"6080/0 Mot Max Speed",
                79,"60E0/0 Pos TorqLimit",
                80,"60E1/0 Neg TorqLimit",
                82,"400B/13 Proc Input Freq";
        Param34000055 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Output#6",      $ name
                "",                     $ units
                "",                     $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000055 =
                0,"ignore",
                51,"SINT_OUT",
                52,"INT_OUT",
                53,"DINT_OUT",
                54,"2946/1 Trq Mode Hi Spd",
                55,"2946/2 Trq Mode Lo Spd",
                56,"4008/1 NetWordIN1",
                57,"4008/2 NetWordIN2",
                58,"4008/3 NetWordIN3",
                59,"4008/4 NetWordIN4",
                60,"400B/1 AC Drv Ctrl Word",
                61,"400B/2 C0135 Ctrl Word",
                62,"400B/3 Net Spd Stpnt Hz",
                63,"400B/4 Net Spd Stpnt RPM",
                64,"400B/5 Net Spd 0.01 Hz",
                65,"400B/6 NetSpdSign 0.1Hz",
                66,"400B/7 Net PID Stpnt",
                67,"400B/8 Net Torque Stpnt",
                68,"6040/0 Control Word",
                69,"6042/0 Target Veloc",
                70,"6046/1 Veloc Min",
                71,"6046/2 Veloc Max",
                72,"6048/1 Delta Speed",
                73,"6048/2 Delta Time",
                74,"6049/1 Delta Speed",
                75,"6049/2 Delta Time",
                76,"6060/0 402 Control Modes",
                77,"6071/0 402 TargetTorq",
                78,"6080/0 Mot Max Speed",
                79,"60E0/0 Pos TorqLimit",
                80,"60E1/0 Neg TorqLimit",
                82,"400B/13 Proc Input Freq";
        Param34000056 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Output#7",      $ name
                "",                     $ units
                "",                     $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000056 =
                0,"ignore",
                51,"SINT_OUT",
                52,"INT_OUT",
                53,"DINT_OUT",
                54,"2946/1 Trq Mode Hi Spd",
                55,"2946/2 Trq Mode Lo Spd",
                56,"4008/1 NetWordIN1",
                57,"4008/2 NetWordIN2",
                58,"4008/3 NetWordIN3",
                59,"4008/4 NetWordIN4",
                60,"400B/1 AC Drv Ctrl Word",
                61,"400B/2 C0135 Ctrl Word",
                62,"400B/3 Net Spd Stpnt Hz",
                63,"400B/4 Net Spd Stpnt RPM",
                64,"400B/5 Net Spd 0.01 Hz",
                65,"400B/6 NetSpdSign 0.1Hz",
                66,"400B/7 Net PID Stpnt",
                67,"400B/8 Net Torque Stpnt",
                68,"6040/0 Control Word",
                69,"6042/0 Target Veloc",
                70,"6046/1 Veloc Min",
                71,"6046/2 Veloc Max",
                72,"6048/1 Delta Speed",
                73,"6048/2 Delta Time",
                74,"6049/1 Delta Speed",
                75,"6049/2 Delta Time",
                76,"6060/0 402 Control Modes",
                77,"6071/0 402 TargetTorq",
                78,"6080/0 Mot Max Speed",
                79,"60E0/0 Pos TorqLimit",
                80,"60E1/0 Neg TorqLimit",
                82,"400B/13 Proc Input Freq";
        Param34000057 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Output#8",      $ name
                "",                     $ units
                "",                     $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000057 =
                0,"ignore",
                51,"SINT_OUT",
                52,"INT_OUT",
                53,"DINT_OUT",
                54,"2946/1 Trq Mode Hi Spd",
                55,"2946/2 Trq Mode Lo Spd",
                56,"4008/1 NetWordIN1",
                57,"4008/2 NetWordIN2",
                58,"4008/3 NetWordIN3",
                59,"4008/4 NetWordIN4",
                60,"400B/1 AC Drv Ctrl Word",
                61,"400B/2 C0135 Ctrl Word",
                62,"400B/3 Net Spd Stpnt Hz",
                63,"400B/4 Net Spd Stpnt RPM",
                64,"400B/5 Net Spd 0.01 Hz",
                65,"400B/6 NetSpdSign 0.1Hz",
                66,"400B/7 Net PID Stpnt",
                67,"400B/8 Net Torque Stpnt",
                68,"6040/0 Control Word",
                69,"6042/0 Target Veloc",
                70,"6046/1 Veloc Min",
                71,"6046/2 Veloc Max",
                72,"6048/1 Delta Speed",
                73,"6048/2 Delta Time",
                74,"6049/1 Delta Speed",
                75,"6049/2 Delta Time",
                76,"6060/0 402 Control Modes",
                77,"6071/0 402 TargetTorq",
                78,"6080/0 Mot Max Speed",
                79,"60E0/0 Pos TorqLimit",
                80,"60E1/0 Neg TorqLimit",
                82,"400B/13 Proc Input Freq";
        Param34000058 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Output#9",      $ name
                "",                     $ units
                "",                     $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000058 =
                0,"ignore",
                51,"SINT_OUT",
                52,"INT_OUT",
                53,"DINT_OUT",
                54,"2946/1 Trq Mode Hi Spd",
                55,"2946/2 Trq Mode Lo Spd",
                56,"4008/1 NetWordIN1",
                57,"4008/2 NetWordIN2",
                58,"4008/3 NetWordIN3",
                59,"4008/4 NetWordIN4",
                60,"400B/1 AC Drv Ctrl Word",
                61,"400B/2 C0135 Ctrl Word",
                62,"400B/3 Net Spd Stpnt Hz",
                63,"400B/4 Net Spd Stpnt RPM",
                64,"400B/5 Net Spd 0.01 Hz",
                65,"400B/6 NetSpdSign 0.1Hz",
                66,"400B/7 Net PID Stpnt",
                67,"400B/8 Net Torque Stpnt",
                68,"6040/0 Control Word",
                69,"6042/0 Target Veloc",
                70,"6046/1 Veloc Min",
                71,"6046/2 Veloc Max",
                72,"6048/1 Delta Speed",
                73,"6048/2 Delta Time",
                74,"6049/1 Delta Speed",
                75,"6049/2 Delta Time",
                76,"6060/0 402 Control Modes",
                77,"6071/0 402 TargetTorq",
                78,"6080/0 Mot Max Speed",
                79,"60E0/0 Pos TorqLimit",
                80,"60E1/0 Neg TorqLimit",
                82,"400B/13 Proc Input Freq";
        Param34000059 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Output#10",     $ name
                "",                     $ units
                "",                     $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000059 =
                0,"ignore",
                51,"SINT_OUT",
                52,"INT_OUT",
                53,"DINT_OUT",
                54,"2946/1 Trq Mode Hi Spd",
                55,"2946/2 Trq Mode Lo Spd",
                56,"4008/1 NetWordIN1",
                57,"4008/2 NetWordIN2",
                58,"4008/3 NetWordIN3",
                59,"4008/4 NetWordIN4",
                60,"400B/1 AC Drv Ctrl Word",
                61,"400B/2 C0135 Ctrl Word",
                62,"400B/3 Net Spd Stpnt Hz",
                63,"400B/4 Net Spd Stpnt RPM",
                64,"400B/5 Net Spd 0.01 Hz",
                65,"400B/6 NetSpdSign 0.1Hz",
                66,"400B/7 Net PID Stpnt",
                67,"400B/8 Net Torque Stpnt",
                68,"6040/0 Control Word",
                69,"6042/0 Target Veloc",
                70,"6046/1 Veloc Min",
                71,"6046/2 Veloc Max",
                72,"6048/1 Delta Speed",
                73,"6048/2 Delta Time",
                74,"6049/1 Delta Speed",
                75,"6049/2 Delta Time",
                76,"6060/0 402 Control Modes",
                77,"6071/0 402 TargetTorq",
                78,"6080/0 Mot Max Speed",
                79,"60E0/0 Pos TorqLimit",
                80,"60E1/0 Neg TorqLimit",
                82,"400B/13 Proc Input Freq";
        Param34000060 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Output#11",     $ name
                "",                     $ units
                "",                     $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000060 =
                0,"ignore",
                51,"SINT_OUT",
                52,"INT_OUT",
                53,"DINT_OUT",
                54,"2946/1 Trq Mode Hi Spd",
                55,"2946/2 Trq Mode Lo Spd",
                56,"4008/1 NetWordIN1",
                57,"4008/2 NetWordIN2",
                58,"4008/3 NetWordIN3",
                59,"4008/4 NetWordIN4",
                60,"400B/1 AC Drv Ctrl Word",
                61,"400B/2 C0135 Ctrl Word",
                62,"400B/3 Net Spd Stpnt Hz",
                63,"400B/4 Net Spd Stpnt RPM",
                64,"400B/5 Net Spd 0.01 Hz",
                65,"400B/6 NetSpdSign 0.1Hz",
                66,"400B/7 Net PID Stpnt",
                67,"400B/8 Net Torque Stpnt",
                68,"6040/0 Control Word",
                69,"6042/0 Target Veloc",
                70,"6046/1 Veloc Min",
                71,"6046/2 Veloc Max",
                72,"6048/1 Delta Speed",
                73,"6048/2 Delta Time",
                74,"6049/1 Delta Speed",
                75,"6049/2 Delta Time",
                76,"6060/0 402 Control Modes",
                77,"6071/0 402 TargetTorq",
                78,"6080/0 Mot Max Speed",
                79,"60E0/0 Pos TorqLimit",
                80,"60E1/0 Neg TorqLimit",
                82,"400B/13 Proc Input Freq";
        Param34000061 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Output#12",     $ name
                "",                     $ units
                "",                     $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000061 =
                0,"ignore",
                51,"SINT_OUT",
                52,"INT_OUT",
                53,"DINT_OUT",
                54,"2946/1 Trq Mode Hi Spd",
                55,"2946/2 Trq Mode Lo Spd",
                56,"4008/1 NetWordIN1",
                57,"4008/2 NetWordIN2",
                58,"4008/3 NetWordIN3",
                59,"4008/4 NetWordIN4",
                60,"400B/1 AC Drv Ctrl Word",
                61,"400B/2 C0135 Ctrl Word",
                62,"400B/3 Net Spd Stpnt Hz",
                63,"400B/4 Net Spd Stpnt RPM",
                64,"400B/5 Net Spd 0.01 Hz",
                65,"400B/6 NetSpdSign 0.1Hz",
                66,"400B/7 Net PID Stpnt",
                67,"400B/8 Net Torque Stpnt",
                68,"6040/0 Control Word",
                69,"6042/0 Target Veloc",
                70,"6046/1 Veloc Min",
                71,"6046/2 Veloc Max",
                72,"6048/1 Delta Speed",
                73,"6048/2 Delta Time",
                74,"6049/1 Delta Speed",
                75,"6049/2 Delta Time",
                76,"6060/0 402 Control Modes",
                77,"6071/0 402 TargetTorq",
                78,"6080/0 Mot Max Speed",
                79,"60E0/0 Pos TorqLimit",
                80,"60E1/0 Neg TorqLimit",
                82,"400B/13 Proc Input Freq";
        Param34000062 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Output#13",     $ name
                "",                     $ units
                "",                     $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000062 =
                0,"ignore",
                51,"SINT_OUT",
                52,"INT_OUT",
                53,"DINT_OUT",
                54,"2946/1 Trq Mode Hi Spd",
                55,"2946/2 Trq Mode Lo Spd",
                56,"4008/1 NetWordIN1",
                57,"4008/2 NetWordIN2",
                58,"4008/3 NetWordIN3",
                59,"4008/4 NetWordIN4",
                60,"400B/1 AC Drv Ctrl Word",
                61,"400B/2 C0135 Ctrl Word",
                62,"400B/3 Net Spd Stpnt Hz",
                63,"400B/4 Net Spd Stpnt RPM",
                64,"400B/5 Net Spd 0.01 Hz",
                65,"400B/6 NetSpdSign 0.1Hz",
                66,"400B/7 Net PID Stpnt",
                67,"400B/8 Net Torque Stpnt",
                68,"6040/0 Control Word",
                69,"6042/0 Target Veloc",
                70,"6046/1 Veloc Min",
                71,"6046/2 Veloc Max",
                72,"6048/1 Delta Speed",
                73,"6048/2 Delta Time",
                74,"6049/1 Delta Speed",
                75,"6049/2 Delta Time",
                76,"6060/0 402 Control Modes",
                77,"6071/0 402 TargetTorq",
                78,"6080/0 Mot Max Speed",
                79,"60E0/0 Pos TorqLimit",
                80,"60E1/0 Neg TorqLimit",
                82,"400B/13 Proc Input Freq";
        Param34000063 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Output#14",     $ name
                "",                     $ units
                "",                     $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000063 =
                0,"ignore",
                51,"SINT_OUT",
                52,"INT_OUT",
                53,"DINT_OUT",
                54,"2946/1 Trq Mode Hi Spd",
                55,"2946/2 Trq Mode Lo Spd",
                56,"4008/1 NetWordIN1",
                57,"4008/2 NetWordIN2",
                58,"4008/3 NetWordIN3",
                59,"4008/4 NetWordIN4",
                60,"400B/1 AC Drv Ctrl Word",
                61,"400B/2 C0135 Ctrl Word",
                62,"400B/3 Net Spd Stpnt Hz",
                63,"400B/4 Net Spd Stpnt RPM",
                64,"400B/5 Net Spd 0.01 Hz",
                65,"400B/6 NetSpdSign 0.1Hz",
                66,"400B/7 Net PID Stpnt",
                67,"400B/8 Net Torque Stpnt",
                68,"6040/0 Control Word",
                69,"6042/0 Target Veloc",
                70,"6046/1 Veloc Min",
                71,"6046/2 Veloc Max",
                72,"6048/1 Delta Speed",
                73,"6048/2 Delta Time",
                74,"6049/1 Delta Speed",
                75,"6049/2 Delta Time",
                76,"6060/0 402 Control Modes",
                77,"6071/0 402 TargetTorq",
                78,"6080/0 Mot Max Speed",
                79,"60E0/0 Pos TorqLimit",
                80,"60E1/0 Neg TorqLimit",
                82,"400B/13 Proc Input Freq";
        Param34000064 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Output#15",     $ name
                "",                     $ units
                "",                     $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000064 =
                0,"ignore",
                51,"SINT_OUT",
                52,"INT_OUT",
                53,"DINT_OUT",
                54,"2946/1 Trq Mode Hi Spd",
                55,"2946/2 Trq Mode Lo Spd",
                56,"4008/1 NetWordIN1",
                57,"4008/2 NetWordIN2",
                58,"4008/3 NetWordIN3",
                59,"4008/4 NetWordIN4",
                60,"400B/1 AC Drv Ctrl Word",
                61,"400B/2 C0135 Ctrl Word",
                62,"400B/3 Net Spd Stpnt Hz",
                63,"400B/4 Net Spd Stpnt RPM",
                64,"400B/5 Net Spd 0.01 Hz",
                65,"400B/6 NetSpdSign 0.1Hz",
                66,"400B/7 Net PID Stpnt",
                67,"400B/8 Net Torque Stpnt",
                68,"6040/0 Control Word",
                69,"6042/0 Target Veloc",
                70,"6046/1 Veloc Min",
                71,"6046/2 Veloc Max",
                72,"6048/1 Delta Speed",
                73,"6048/2 Delta Time",
                74,"6049/1 Delta Speed",
                75,"6049/2 Delta Time",
                76,"6060/0 402 Control Modes",
                77,"6071/0 402 TargetTorq",
                78,"6080/0 Mot Max Speed",
                79,"60E0/0 Pos TorqLimit",
                80,"60E1/0 Neg TorqLimit",
                82,"400B/13 Proc Input Freq";
        Param34000065 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Custom Output#16",     $ name
                "",                     $ units
                "",                     $ help string
                0,65535,0,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000065 =
                0,"ignore",
                51,"SINT_OUT",
                52,"INT_OUT",
                53,"DINT_OUT",
                54,"2946/1 Trq Mode Hi Spd",
                55,"2946/2 Trq Mode Lo Spd",
                56,"4008/1 NetWordIN1",
                57,"4008/2 NetWordIN2",
                58,"4008/3 NetWordIN3",
                59,"4008/4 NetWordIN4",
                60,"400B/1 AC Drv Ctrl Word",
                61,"400B/2 C0135 Ctrl Word",
                62,"400B/3 Net Spd Stpnt Hz",
                63,"400B/4 Net Spd Stpnt RPM",
                64,"400B/5 Net Spd 0.01 Hz",
                65,"400B/6 NetSpdSign 0.1Hz",
                66,"400B/7 Net PID Stpnt",
                67,"400B/8 Net Torque Stpnt",
                68,"6040/0 Control Word",
                69,"6042/0 Target Veloc",
                70,"6046/1 Veloc Min",
                71,"6046/2 Veloc Max",
                72,"6048/1 Delta Speed",
                73,"6048/2 Delta Time",
                74,"6049/1 Delta Speed",
                75,"6049/2 Delta Time",
                76,"6060/0 402 Control Modes",
                77,"6071/0 402 TargetTorq",
                78,"6080/0 Mot Max Speed",
                79,"60E0/0 Pos TorqLimit",
                80,"60E1/0 Neg TorqLimit",
                82,"400B/13 Proc Input Freq";

        Param34000100 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Input Trailer",        $ name
                "",                     $ units
                "",                     $ help string
                100,100,100,            $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param34000101 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Output Trailer",       $ name
                "",                     $ units
                "",                     $ help string
                101,101,101,            $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places



        Param34000200 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Input#1",              $ name
                "",                     $ units
                "",                     $ help string
                29,29,29,               $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000200 =
                29,"400C/1 AC Drv Stat Word";
        Param34000201 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Input#2",              $ name
                "",                     $ units
                "",                     $ help string
                32,32,32,               $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000201 =
                32,"400C/4 Actual Speed RPM";
        Param34000202 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Input#3",              $ name
                "",                     $ units
                "",                     $ help string
                35,35,35,               $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000202 =
                35,"400C/7 Actual Torque Scaled";


        Param34000250 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Output#1",             $ name
                "",                     $ units
                "",                     $ help string
                60,60,60,               $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000250 =
                60,"400B/1 AC Drv Ctrl Word";
        Param34000251 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Output#2",             $ name
                "",                     $ units
                "",                     $ help string
                63,63,63,               $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000251 =
                63,"400B/4 Net Spd Stpnt RPM";
        Param34000252 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0400,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Output#3",             $ name
                "",                     $ units
                "",                     $ help string
                67,67,67,               $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Enum34000252 =
                67,"400B/8 Net Torque Stpnt";

    $ +++++++++++++++++++++ Safety parameters +++++++++++++++++++++++++++++++++++++

        Param34000300 =                 $ prev. Param8   Demo only!!!
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC8,                   $ Data Type
                4,                      $ Data Size in bytes
                "RPI Range for Safety Output assembly",    $ name
                "",                     $ units
                "",                     $ help string
                10000,1000000,20000,    $ min, max, default data values
                ,,,,                    $ decimal places
                ,,,,
                ;
        Param34000302 =                 $ prev. Param9   Demo only!!!
                0,                      $ reserved, shall equal 0
                ,"",                    $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC1,                   $ Data Type
                1,                      $ Data Size in bytes
                "Safe Torque Off",      $ name
                "",                     $ units
                "= Disable(0) / Permit(1) Torque",    $ help string
                0,1,0,                  $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param34000303 =                 $ prev. Param10   Demo only!!!
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC1,                   $ Data Type
                1,                      $ Data Size in bytes
                "Torque Disabled",      $ name
                "",                     $ units
                "= Torque permitted(0) / disabled(1)",    $ help string
                0,1,0,                  $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param34000304 =                 $ prev. Param11   Demo only!!!
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC1,                   $ Data Type
                1,                      $ Data Size in bytes
                "Safety Reset",         $ name
                "",                     $ units
                "= Transition 0->1 to recover from a safety fault",    $ help string
                0,1,0,                  $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param34000305 =                 $ prev. Param12   Demo only!!!
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC1,                   $ Data Type
                1,                      $ Data Size in bytes
                "Safety Fault",         $ name
                "",                     $ units
                "= No safety fault(0) / safety fault present(1)",    $ help string
                0,1,0,                  $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param34000306 =                 $ prev. Param13   Demo only!!!
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC1,                   $ Data Type
                1,                      $ Data Size in bytes
                "Restart required",     $ name
                "",                     $ units
                "= (1) Reset required to restart the device",    $ help string
                0,1,0,                  $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param34000307 =                 $ prev. Param14   Demo only!!!
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC8,                   $ Data Type
                4,                      $ Data Size in bytes
                "RPI Range for Safety Input assembly",    $ name
                "",                     $ units
                "",                     $ help string
                10000,1000000,40000,    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param34000308 =                 $ prev. Param34000308 Safety Output only!!!
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xD3,                   $ Data Type
                4,                      $ Data Size in bytes
                "SafetyOut1",           $ name
                "",                     $ units
                "New Help String",      $ help string
                0,4294967295,0,         $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param34000309 =                 $ prev. Param34000309 Safety Input only!!!
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0030,                 $ Descriptor
                0xD3,                   $ Data Type
                4,                      $ Data Size in bytes
                "SafetyInp1",           $ name
                "",                     $ units
                "New Help String",      $ help string
                0,4294967295,0,         $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places


[Assembly]
        Object_Name = "Assembly Object";
        Object_Class_Code = 0x04;

        Assem20 =                       $ Assemb21 selected by parameter Param1000
                "Speed Ctrl Out",
                ,
                4,
                0x0001,
                ,,
                16,Param60,
                16,Param63;
        Assem22 =                       $ Assemb23 selected by parameter Param1002
                "Speed & Torque Ctrl Out",
                ,
                6,
                0x0001,
                ,,
                16,Param60,
                16,Param63,
                16,Param67;
        Assem70 =                       $ Assemb71 selected by parameter Param1001
                "Speed Ctrl Inp",
                ,
                4,
                0x0001,
                ,,
                16,Param29,
                16,Param32;
        Assem72 =                       $ Assemb73 selected by parameter Param1003
                "Speed & Torque Ctrl Inp",
                ,
                6,
                0x0001,
                ,,
                16,Param29,
                16,Param32,
                16,Param35;
        Assem110 =
                "Custom Output Assembly",
                ,
                ,
                0x0001,
                ,,
                ,Param34000050,
                ,Param34000051,
                ,Param34000052,
                ,Param34000053,
                ,Param34000054,
                ,Param34000055,
                ,Param34000056,
                ,Param34000057,
                ,Param34000058,
                ,Param34000059,
                ,Param34000060,
                ,Param34000061,
                ,Param34000062,
                ,Param34000063,
                ,Param34000064,
                ,Param34000065,
                32,Param34000101;
        Assem111 =
                "Custom Input Assembly",
                ,
                ,
                0x0001,
                ,,
                ,Param34000000,
                ,Param34000001,
                ,Param34000002,
                ,Param34000003,
                ,Param34000004,
                ,Param34000005,
                ,Param34000006,
                ,Param34000007,
                ,Param34000008,
                ,Param34000009,
                ,Param34000010,
                ,Param34000011,
                ,Param34000012,
                ,Param34000013,
                ,Param34000014,
                ,Param34000015,
                32,Param34000100;
        Assem130 =
                "Config Assembly",
                ,
                ,
                0x0801,
                ,,
                16,Param34000000,
                16,Param34000001,
                16,Param34000002,
                16,Param34000003,
                16,Param34000004,
                16,Param34000005,
                16,Param34000006,
                16,Param34000007,
                16,Param34000008,
                16,Param34000009,
                16,Param34000010,
                16,Param34000011,
                16,Param34000012,
                16,Param34000013,
                16,Param34000014,
                16,Param34000015,
                16,Param34000100,

                16,Param34000050,
                16,Param34000051,
                16,Param34000052,
                16,Param34000053,
                16,Param34000054,
                16,Param34000055,
                16,Param34000056,
                16,Param34000057,
                16,Param34000058,
                16,Param34000059,
                16,Param34000060,
                16,Param34000061,
                16,Param34000062,
                16,Param34000063,
                16,Param34000064,
                16,Param34000065,
                16,Param34000101;
        Assem151 =
                "Safety Config",
                ,
                0,
                0x0000,
                ,,
                0,;
        Assem161 =
                "Safety Output Data with STO",
                "20 04 24 A1 30 03",
                8,
                0x0000,
                ,,
                32,Param34000308,
                32,;
        Assem171 =
                "Safety Input Data with STO",
                "20 04 24 AB 30 03",
                12,
                0x0000,
                ,,
                32,Param34000309,
                64,;
        Assem199 =                      $ Mandatory for CIP Safety
                "Null Connection point",
                ,
                0,
                0x0000,
                ,,
                0,;
        Assem254 =
                "Input Only Output",
                ,
                0,
                0x0000,
                ,,
                0,;
        Assem255 =
                "Listen Only Output",
                ,
                0,
                0x0000,
                ,,
                0,;


[Connection Manager]
        Revision = 1;
        Object_Name = "Connection Manager Object";
        Object_Class_Code = 0x06;
        MaxInst = 1;
        Number_Of_Static_Instances = 1;
        Max_Number_Of_Dynamic_Instances = 0;
        MaxSafetyConnections = 2;       $ Mandatory for CIP Safety
        MaxSafetyInputCnxns = 1;        $ Mandatory for CIP Safety
        MaxSafetyOutputCnxns = 1;       $ Mandatory for CIP Safety
        DefaultSafetyConnections = 4,5; $ Mandatory for CIP Safety
        SafetyFormat = 2;               $ Mandatory for CIP Safety, 1= base format only; 2= extended format only; 3= support for base and extended format

        Connection1 =
                0x04010002,             $ 0-15    = supported transport classes
                                        $ 16      = trigger: cyclic
                                        $ 17      = trigger: change of state
                                        $ 18      = trigger: application
                                        $ 19-23   = trigger: reserved
                                        $ 24      = application type: listen-only
                                        $ 25      = application type: input-only
                                        $ 26      = application type: exclusive-owner
                                        $ 27      = application type: redundant-owner
                                        $ 28-30   = reserved
                                        $ 31      = Direction: Client = 0 / Server = 1
                0x4464040F,             $ 0       = O->T fixed size supported
                                        $ 1       = O->T variable size supported
                                        $ 2       = T->O fixed size supported
                                        $ 3       = T->O variable size supported
                                        $ 4-5     = O->T number of bytes per slot (obsolete)
                                        $ 6-7     = T->O number of bytes per slot (obsolete)
                                        $ 8-10    = O->T Real time transfer format
                                        $ 11      = reserved
                                        $ 12-14   = T->O Real time transfer format
                                        $ 15      = reserved
                                        $ 16      = O->T connection type: NULL
                                        $ 17      = O->T connection type: MULTICAST
                                        $ 18      = O->T connection type: POINT2POINT
                                        $ 19      = O->T connection type: reserved
                                        $ 20      = T->O connection type: NULL
                                        $ 21      = T->O connection type: MULTICAST
                                        $ 22      = T->O connection type: POINT2POINT
                                        $ 23      = T->O connection type: reserved
                                        $ 24      = O->T priority: LOW
                                        $ 25      = O->T priority: HIGH
                                        $ 26      = O->T priority: SCHEDULED
                                        $ 27      = O->T priority: reserved
                                        $ 28      = T->O priority: LOW
                                        $ 29      = T->O priority: HIGH
                                        $ 30      = T->O priority: SCHEDULED
                                        $ 31      = T->O priority: reserved
                Param2000,4,Assem20,    $ O->T RPI, size, format
                Param2000,4,Assem70,    $ T->O RPI, size, format
                ,,                      $ proxy config size, format
                0,,                     $ target config size, format
                "Speed",                $ Connection Name
                "",                     $ help string
                "20 04 24 82 2C [Param1000] 2C [Param1001]";    $ Path
        Connection2 =
                0x04010002,             $ 0-15    = supported transport classes
                                        $ 16      = trigger: cyclic
                                        $ 17      = trigger: change of state
                                        $ 18      = trigger: application
                                        $ 19-23   = trigger: reserved
                                        $ 24      = application type: listen-only
                                        $ 25      = application type: input-only
                                        $ 26      = application type: exclusive-owner
                                        $ 27      = application type: redundant-owner
                                        $ 28-30   = reserved
                                        $ 31      = Direction: Client = 0 / Server = 1
                0x4464040F,             $ 0       = O->T fixed size supported
                                        $ 1       = O->T variable size supported
                                        $ 2       = T->O fixed size supported
                                        $ 3       = T->O variable size supported
                                        $ 4-5     = O->T number of bytes per slot (obsolete)
                                        $ 6-7     = T->O number of bytes per slot (obsolete)
                                        $ 8-10    = O->T Real time transfer format
                                        $ 11      = reserved
                                        $ 12-14   = T->O Real time transfer format
                                        $ 15      = reserved
                                        $ 16      = O->T connection type: NULL
                                        $ 17      = O->T connection type: MULTICAST
                                        $ 18      = O->T connection type: POINT2POINT
                                        $ 19      = O->T connection type: reserved
                                        $ 20      = T->O connection type: NULL
                                        $ 21      = T->O connection type: MULTICAST
                                        $ 22      = T->O connection type: POINT2POINT
                                        $ 23      = T->O connection type: reserved
                                        $ 24      = O->T priority: LOW
                                        $ 25      = O->T priority: HIGH
                                        $ 26      = O->T priority: SCHEDULED
                                        $ 27      = O->T priority: reserved
                                        $ 28      = T->O priority: LOW
                                        $ 29      = T->O priority: HIGH
                                        $ 30      = T->O priority: SCHEDULED
                                        $ 31      = T->O priority: reserved
                Param2000,6,Assem22,    $ O->T RPI, size, format
                Param2000,6,Assem72,    $ T->O RPI, size, format
                ,,                      $ proxy config size, format
                0,,                     $ target config size, format
                "Speed & Torque",       $ Connection Name
                "",                     $ help string
                "20 04 24 82 2C [Param1002] 2C [Param1003]";    $ Path
        Connection3 =
                0x04010002,             $ 0-15    = supported transport classes
                                        $ 16      = trigger: cyclic
                                        $ 17      = trigger: change of state
                                        $ 18      = trigger: application
                                        $ 19-23   = trigger: reserved
                                        $ 24      = application type: listen-only
                                        $ 25      = application type: input-only
                                        $ 26      = application type: exclusive-owner
                                        $ 27      = application type: redundant-owner
                                        $ 28-30   = reserved
                                        $ 31      = Direction: Client = 0 / Server = 1
                0x4464040F,             $ 0       = O->T fixed size supported
                                        $ 1       = O->T variable size supported
                                        $ 2       = T->O fixed size supported
                                        $ 3       = T->O variable size supported
                                        $ 4-5     = O->T number of bytes per slot (obsolete)
                                        $ 6-7     = T->O number of bytes per slot (obsolete)
                                        $ 8-10    = O->T Real time transfer format
                                        $ 11      = reserved
                                        $ 12-14   = T->O Real time transfer format
                                        $ 15      = reserved
                                        $ 16      = O->T connection type: NULL
                                        $ 17      = O->T connection type: MULTICAST
                                        $ 18      = O->T connection type: POINT2POINT
                                        $ 19      = O->T connection type: reserved
                                        $ 20      = T->O connection type: NULL
                                        $ 21      = T->O connection type: MULTICAST
                                        $ 22      = T->O connection type: POINT2POINT
                                        $ 23      = T->O connection type: reserved
                                        $ 24      = O->T priority: LOW
                                        $ 25      = O->T priority: HIGH
                                        $ 26      = O->T priority: SCHEDULED
                                        $ 27      = O->T priority: reserved
                                        $ 28      = T->O priority: LOW
                                        $ 29      = T->O priority: HIGH
                                        $ 30      = T->O priority: SCHEDULED
                                        $ 31      = T->O priority: reserved
                Param2000,,Assem110,    $ O->T RPI, size, format
                Param2000,,Assem111,    $ T->O RPI, size, format
                ,,                      $ proxy config size, format
                ,Assem130,              $ target config size, format
                "Custom I/O Connection",$ Connection Name
                "",                     $ help string
                "20 04 24 82 2C 6E 2C 6F";    $ Path
    $ +++++++++++++++++++++ Safety connections +++++++++++++++++++++++++++++++++++++

        Connection4 =
                0x84040001,             $ Trigger and transport
                                        $ Consumer (Server, b31 = 1)
                                        $ b31|b30|b29|b28|b27|b26|b25|b24|b23|b22|b21|b20|b19|b18|b17|b16|b15|b14|b13|b12|b11|b10|b9|b8|b7|b6|b5|b4|b3|b2|b1|b0
                                        $ 1000 0100 0000 0100 0000 0000 0000 0001?
                                        $ 0    	= transport class  0 Supported (for I/O safety b0 =1)
                                        $ 1		= transport class 1 Not supported
                                        $ 2		= transport class 2 Not supported
                                        $ 3		= transport class 3 Not supported
                                        $ 4		= transport class 4 Not supported
                                        $ 5		= transport class 5 Not supported
                                        $ 6		= transport class 6 Not supported
                                        $ 7-15	= transport class: reserved
                                        $ 16      = trigger: cyclic
                                        $ 17      = trigger: change of state
                                        $ 18      = trigger: application
                                        $ 19-23   = trigger: reserved
                                        $ 24      = transport type: listen-only
                                        $ 25      = transport type: input-only
                                        $ 26      = transport type: exclusive-owner
                                        $ 27      = transport type: redundant-owner
                                        $ 28-30   = reserved
                                        $ 31      = direction (Client = 0 / Server = 1)
                0x22445505,             $ Connection parameters
                                        $ b31|b30|b29|b28|b27|b26|b25|b24|b23|b22|b21|b20|b19|b18|b17|b16|b15|b14|b13|b12|b11|b10|b9|b8|b7|b6|b5|b4|b3|b2|b1|b0
                                        $ ?0010 0010 0100 0100 0101 0101 0000 0101?
                                        $ 0       = O->T fixed size supported
                                        $ 1       = O->T variable size supported
                                        $ 2       = T->O fixed size supported
                                        $ 3       = T->O variable size supported
                                        $ 4-5     = O->T number of bytes per slot (obsolete)
                                        $ 6-7     = T->O number of bytes per slot (obsolete)
                                        $ 8-10    = O->T Real time transfer format
                                        $ 11      = reserved
                                        $ 12-14   = T->O Real time transfer format
                                        $ 15      = reserved
                                        $ 16      = O->T connection type: NULL
                                        $ 17      = O->T connection type: MULTICAST
                                        $ 18      = O->T connection type: POINT2POINT
                                        $ 19      = O->T connection type: reserved
                                        $ 20      = T->O connection type: NULL
                                        $ 21      = T->O connection type: MULTICAST
                                        $ 22      = T->O connection type: POINT2POINT
                                        $ 23      = T->O connection type: reserved
                                        $ 24      = O->T priority: LOW
                                        $ 25      = O->T priority: HIGH
                                        $ 26      = O->T priority: SCHEDULED
                                        $ 27      = O->T priority: reserved
                                        $ 28      = T->O priority: LOW
                                        $ 29      = T->O priority: HIGH
                                        $ 30      = T->O priority: SCHEDULED
                                        $ 31      = T->O priority: reserved
                Param34000300,,Assem161,$ O->T RPI, size, format
                ,,,                     $ T->O RPI, size, format
                ,,                      $ proxy config size, format
                ,Assem151,              $ target config size, format
                "Safety Output (Consuming)",    $ Connection Name
                "",                     $ help string
                "20 04 24 97 2C A1 2C C7",    $ Config=151; Output=161: Input Null=199
                ,                       $ Asynchronous
                ;                       $ Maximum Consumer Number
        Connection5 =
                0x02040001,             $ Trigger and transport
                                        $ Producer (Client, b31 = 0)
                                        $ b31|b30|b29|b28|b27|b26|b25|b24|b23|b22|b21|b20|b19|b18|b17|b16|b15|b14|b13|b12|b11|b10|b9|b8|b7|b6|b5|b4|b3|b2|b1|b0
                                        $ 0000 ?0010 0000 0100 0000 0000 0000 0001?
                                        $ 0-15    = supported transport classes
                                        $ 16      = trigger: cyclic
                                        $ 17      = trigger: change of state
                                        $ 18      = trigger: application
                                        $ 19-23   = trigger: reserved
                                        $ 24      = transport type: listen-only
                                        $ 25      = transport type: input-only
                                        $ 26      = transport type: exclusive-owner
                                        $ 27      = transport type: redundant-owner
                                        $ 28-30   = reserved
                                        $ 31      = Client = 0 / Server = 1
                0x22645505,             $ Connection parameters
                                        $ b31|b30|b29|b28|b27|b26|b25|b24|b23|b22|b21|b20|b19|b18|b17|b16|b15|b14|b13|b12|b11|b10|b9|b8|b7|b6|b5|b4|b3|b2|b1|b0
                                        $ 0       = O->T fixed size supported
                                        $ 1       = O->T variable size supported
                                        $ 2       = T->O fixed size supported
                                        $ 3       = T->O variable size supported
                                        $ 4-5     = O->T number of bytes per slot (obsolete)
                                        $ 6-7     = T->O number of bytes per slot (obsolete)
                                        $ 8-10    = O->T Real time transfer format
                                        $ 11      = reserved
                                        $ 12-14   = T->O Real time transfer format
                                        $ 15      = reserved
                                        $ 16      = O->T connection type: NULL
                                        $ 17      = O->T connection type: MULTICAST
                                        $ 18      = O->T connection type: POINT2POINT
                                        $ 19      = O->T connection type: reserved
                                        $ 20      = T->O connection type: NULL
                                        $ 21      = T->O connection type: MULTICAST
                                        $ 22      = T->O connection type: POINT2POINT
                                        $ 23      = T->O connection type: reserved
                                        $ 24      = O->T priority: LOW
                                        $ 25      = O->T priority: HIGH
                                        $ 26      = O->T priority: SCHEDULED
                                        $ 27      = O->T priority: reserved
                                        $ 28      = T->O priority: LOW
                                        $ 29      = T->O priority: HIGH
                                        $ 30      = T->O priority: SCHEDULED
                                        $ 31      = T->O priority: reserved
                ,,,                     $ O->T RPI, size, format
                Param34000307,,Assem171,$ T->O RPI, size, format
                ,,                      $ proxy config size, format
                ,Assem151,              $ target config size, format
                "Safety Input (Producing)",    $ Connection Name
                "",                     $ help string
                "20 04 24 97 2C C7 2C AB",    $ Config=151; Output Null=199: Input=171
                1,                      $ Asynchronous
                5;                      $ Maximum Consumer Number

[Port]
        Revision = 2;
        Object_Name = "Port Object";
        Object_Class_Code = 0xF4;
        MaxInst = 2;
        Number_Of_Static_Instances = 2;
        Max_Number_Of_Dynamic_Instances = 0;
        Port1 =
                TCP,
                "Port 1",
                "20 F5 24 01",
                1,
                0x3f,
                ;

[Capacity]

        ConnOverhead = .004;            $ Connection Overhead

        MaxIOConnections = 3;           $ Maximum number of Class 1 Connections
        MaxMsgConnections = 5;          $ Maximum number of Class 3 Connections
        TSpec1 = TxRx, 10, 1400;        $ packets per sec @ 10 bytes
        TSpec2 = TxRx, 100, 1300;       $ packets per sec @ 100 bytes
        TSpec3 = TxRx, 200, 1120;       $ packets per sec @ 200 bytes

[DLR Class]
        Revision = 3;
        Object_Name = "Device Level Ring Object";
        Object_Class_Code = 0x47;
        MaxInst = 1;
        Number_Of_Static_Instances = 1;
        Max_Number_Of_Dynamic_Instances = 0;

[Ethernet Link Class]        $ Class Code: 0x00F6
        Revision = 4;
        Object_Name = "Ethernet Link Object";
        Object_Class_Code = 0xF6;
        MaxInst = 2;
        Number_Of_Static_Instances = 2;
        Max_Number_Of_Dynamic_Instances = 0;
        Class_Attributes =
                2,
                3;
        Instance_Attributes =
                1,
                2,
                3,
                6,
                7,
                8,
                9,
                10;
        Class_Services = 0x0E;
        Instance_Services =
                0x0E,
                0x10;
        InterfaceLabel1 = "P1";
        InterfaceLabel2 = "P2";
        InterfaceType1 = 2;
        InterfaceType2 = 2;


[QoS Class]        $ Class Code: 0x0048
        Revision = 1;
        Object_Name = "QoS Object";
        Object_Class_Code = 0x48;
        MaxInst = 1;
        Number_Of_Static_Instances = 1;
        Max_Number_Of_Dynamic_Instances = 0;
        Class_Attributes =
                1,
                2,
                3,
                6,
                7;
        Instance_Attributes =
                2,
                3,
                4,
                5,
                6,
                7,
                8;
        Class_Services = 0x0E;
        Instance_Services =
                0x0E,
                0x10;

$ End of file
